{"text_format":"1","workbook":"xlsx","n_sheets":11,"sheets":["HIS PPE Public List Price 1_18","Hearing Protection","Eye & Face Protection","Head Protection","Respiratory Protection","Hand Protection","Footwear ","SU Clothing","Chemical Coveralls","Fall Protection","errors"],"not_rendered":{"charts":0,"images":1115,"macros":1,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"HIS PPE Public List Price 1_18","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"cut":false,"hidden":false,"merged":[[5,0,5,11],[1,0,1,11],[3,0,3,11],[4,0,4,11],[11,0,11,11],[10,0,10,11],[8,0,8,11],[7,0,7,11],[6,0,6,11],[9,0,9,11]]}
[]
["Honeywell Industrial Safety PPE Public Price List valid from 1st of September 2018 till further notice "]
[null,null,null,"Insert the reference number and find the product:"]
["Hearing Protection"]
["Eye & Face Protection"]
["Head Protection"]
["Respiratory Protection"]
["Hand Protection"]
["Single Use Clothing"]
["Chemical Coveralls"]
["Footwear "]
["Fall Protection"]

{"sheet":"Hearing Protection","index":1,"n_rows":253,"n_cols":11,"rows_kept":253,"cut":false,"hidden":false,"merged":[[3,1,3,4],[4,1,4,4]]}
[null,"Hearing Protection |  EARPLUGS Single Use"]
[null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per","NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,"Firm Fit single use protective earplugs. "]
[null,"Orange colour, cylinder shape, PVC foam, SNR 37, NRR 30."]
[null,"40% softer, 29% less pressure. Tested and approved in accordance with EN 352-2:2002.Tests performed by Michael & Associates, Inc., State College, Pennsylvania, USA."]
[null,1033010,null,"FirmFit uncorded plugs, polybag","EN 352-2",null,"200 pairs","BOX","BOX",22.651515151515149,7474.9999999999991]
[null,1033012,null,"FirmFit corded plugs, polybag","EN 352-2",null,"100 pairs","BOX","BOX",27.242424242424242,8990]
[null,1033013,null,"FirmFit uncorded plugs, paperbag","EN 352-2",null," 100 pairs","BOX","BOX",19.128787878787879,6312.5]
[null,1033014,null,"FirmFit corded plugs, paperbag","EN 352-2",null,"100 pairs","BOX","BOX",30.606060606060602,10099.999999999998]
[null,1033015,null,"FirmFit uncorded plugs, dispenser refill LS500","EN 352-2",null," 500 pairs","BOX","BOX",49.734848484848484,16412.5]
[null,1033016,null,"FirmFit uncorded plugs, dispenser refill LS400","EN 352-2",null," 200 pairs","BAG","BAG",19.893939393939394,6565]
[null,1005073,null,"303L earplug, individually packed pairs supplied in a dispenser box, size Large","EN352-2",null,"200 pár","CAS","CAS",23.181818181818183,7650.0000000000009]
[null,1005074,null,"303S earplug, individually packed pairs supplied in a dispenser box, size Small","EN352-2",null,"2000 units","CAS","CAS",23.181818181818183,7650.0000000000009]
[null,1007192,null,"303L earplug, packed 10 pairs in one bag supplied in a dispenser box, size Large","EN352-2",null,"2000 units","CAS","CAS",30.454545454545457,10050]
[null,1007193,null,"303L earplug, packed 10 pairs in one bag supplied in a dispenser box, size Small","EN352-2",null,"2000 units","CAS","CAS",30.454545454545457,10050]
[null,1000106,null,"304L corded foam earplug, individually packed pairs supplied in a dispenser box, size Large","EN352-2",null,"500 units","CAS","CAS",14.296969696969697,4718]
[null,1000107,null,"304S corded foam earplug, individually packed pairs supplied in a dispenser box, size Small","EN352-2",null,"500 units","CAS","CAS",14.296969696969697,4718]
[null,3301161,null,"MAX-1 MAX earplug with bell-shape design is easy to insert and counters the tendency to back out of the ear - Extra-high protection from noise\nH: 36  M: 35 L: 34  SNR: 37","EN352-2",null,"200 pár","BOX","BOX",24.848484848484844,8199.9999999999982]
[null,3301130,null,"MAX-30 MAX corded earplug\nH: 36  M: 35 L: 34  SNR: 37 ","EN352-2",null,"100 units","BOX","BOX",30.674242424242426,10122.5]
[null,3301120,null,"LPF-1 MAXLITE earplug, low pressure foam provides long-term comfort for smaller wearers - Ideal size for female workers\nH: 32  M: 32  L: 31  SNR: 34","EN352-2",null,"200 units","BOX","BOX",23.295454545454543,7687.4999999999991]
[null,3301121,null,"LPF-30 MAXLITE corded earplug\nH: 32  M: 32  L: 31  SNR: 34","EN352-2",null,"100 units","BOX","BOX",26.795454545454543,8842.5]
[null,3301105,null,"LL-1 LASERLITE earplug has vibrant colours that make protection visible - Self-adjusting foam expands to fit virtually every wearer\nH: 34  M: 32  L: 31 SNR: 35 ","EN352-2",null,"200 units","BOX","BOX",22.454545454545453,7410]
[null,3301106,null,"LL-30 LASERLITE corded earplug\nH: 34  M: 32  L: 31 SNR: 35 ","EN352-2",null,"100 units","BOX","BOX",26.530303030303031,8755]
[null,3301109,null,"MULTI MAX.  One product, two sizes. Smooth, soil resistant skin prevents dirt build-up. SNR 35.",null,null,200,"BOX","BOX",27.295454545454547,9007.5]
[null,1011236,null,"MATRIX Orange with patented no-roll design makes insertion easy and delivers instant protection upon proper insertion - no need to wait for foam to expand and exceptionally comfortable\nH: 31  M: 25  L: 22  SNR: 29","EN352-2",null,"2000 units","CAS","CAS",20.659090909090907,6817.4999999999991]
[null,1012521,null,"MATRIX Orange corded earplug\nH: 31  M: 25  L: 22  SNR: 29","EN352-2",null,"1000 units","CAS","CAS",22.522727272727273,7432.5]
[]
[null,"Hearing Protection I EARPLUGS Multiple use"]
[null,"Reusable earplugs feature a shell of soft attenuating material around a pocket of air providing superior comfort, extended use and high attenuation - The smooth soil resistant skin can be washed allowing repeated use"]
[null,1034522,null,"TrustFit Pod, uncorded push-in foam plug, poly-bagged SNR 36","EN352-2",null,"100 units","BOX","BOX",53.787878787878782,17749.999999999996]
[null,1034521,null,"TrustFit Pod, corded push-in foam plug, poly-bagged. SNR 36","EN352-2",null,"100 units","BOX","BOX",72.72727272727272,23999.999999999996]
[null,1029810,null,"NEUTRON corded with flip top box  Shape of earphones. Everyday comfort.HearPack.  SNR 20. ","EN352-2",null,"50 units","BOX","BOX",46.015151515151516,15185]
[null,1011239,null,"SmartFit. CMT Technology: material that utilizes body heat to adapt to the shape of the ear. Superior compfort. SNR 30.","EN352-2",null,"50 units","BOX","BOX",48.772727272727266,16094.999999999998]
[null,1011282,null,"FUSION. Corded, standard size. . Unique detachable system, Hearpack storage case.SNR 28","EN352-2",null,"50 units","BOX","BOX",63.79545454545454,21052.499999999996]
[null,1011281,null,"FUSION Green corded, small. Unique detachable system, Hearpack storage case.","EN352-2",null,"50 units","BOX","BOX",63.79545454545454,21052.499999999996]
[null,1005329,null,"CLARITY 656L corded earplug, size Large\nSNR: 22                                                                                                    ","EN352-2",null,"10 units","BOX","BOX",24.325757575757574,8027.4999999999991]
[null,1005328,null,"CLARITY 656S corded earplug, size Small\n SNR: 22                                                                                              ","EN352-2",null,"10 units","BOX","BOX",24.325757575757574,8027.4999999999991]
[null,"AIRSOFT",null,null,null,null,""]
[null,"Reusable earplugs feature a shell of soft attenuating material around a pocket of air providing superior comfort, extended"]
[null,"use and high attenuation - The smooth soil resistant skin can be washed allowing repeated use"]
[null,"H: 29  M: 27  L: 25  SNR: 30",null,null,null,null,""]
[null,1030611,null,"AIRSOFT corded (white nylon cord) with flip top box","EN352-2",null,"50 units","BOX","BOX",55.484848484848477,18309.999999999996]
[null,1030612,null,"AIRSOFT corded (red PVC cord) with flip top box","EN352-2",null,"50 units","BOX","BOX",55.484848484848477,18309.999999999996]
[null,1030610,null,"AIRSOFT uncorded, in practical plastic storage case ","EN352-2",null,"50 units ","BOX","BOX",42.659090909090907,14077.5]
[null,"Hearing Protection |  EARPLUGS Multiple Use",null,null,null,null,""]
[null,"QUIET",null,null,null,null,""]
[null,"Reusable earplug with a soft smooth outer skin for all day comfort - The flexible foam stem enables fast easy insertion -"]
[null,"Can be washed allowing repeated use"]
[null,1028456,null,"QUIET uncorded with flip-top box (replaces 3301170)","EN352-2",null,"50 units","BOX","BOX",23.34090909090909,7702.5]
[null,1028457,null,"QUIET corded with flip-top box (replaces 3301172)","EN352-2",null,"50 units","BOX","BOX",37.742424242424242,12455]
[]
[null,"Hearing Protection |  EARPLUGS Detectable ",null,null,null,null,""]
[null,3301167,null,"LASERTRAK . The highest attenuation rate in its class. Detectable corded earplug supplied in a dispenser box of individually wrapped pairs. SNR 35","EN352-2",null,"100 units","BOX","BOX",54.439393939393938,17965]
[null,1012522,null,"SMARTFIT Detectable corded (Polybag). Long term comfort.  SNR 30. ","EN352-2",null,"50 units","BOX","BOX",71.333333333333329,23540]
[null,1011234,null,"FUSION Detectable Large. SNR 28","EN352-2",null,"50 units","BOX","BOX",75.992424242424235,25077.499999999996]
[null,1011235,null,"FUSION Detectable Small.  SNR 28","EN352-2",null,"50 units","BOX","BOX",75.992424242424235,25077.499999999996]
[null,"Hearing Protection |  EARPLUG DISPENSERS ",null,null,null,null,""]
[null,"HL400-F with canisters and 400 pairs of earplugs"]
[null,"50129760-001",null," HL400-F Frame dispenser with 400 pairs Bilsom 303L EU / UA ","EN 352-2",null,"1 unit","EA","EA",58.333333333333329,19250]
[null,"50129761-001",null," HL400-F Frame dispenser with 400 pairs Bilsom 303S EU / UA ","EN 352-2",null,"1 unit","EA","EA",58.333333333333329,19250]
[null,"50129762-001",null," HL400-F Frame dispenser with 400 pairs Laser Lite EU / UA ","EN 352-2",null,"1 unit","EA","EA",58.333333333333329,19250]
[null,"50129763-001",null," HL400-F Frame dispenser with 400 pairs Max EU / UA ","EN 352-2",null,"1 unit","EA","EA",58.333333333333329,19250]
[null,"50129764-001",null," HL400-F Frame dispenser with 400 pairs Max Lite EU / UA ","EN 352-2",null,"1 unit","EA","EA",58.333333333333329,19250]
[null,"50129765-001",null," HL400-F Frame dispenser with 400 pairs MultiMax EU / UA ","EN 352-2",null,"1 unit","EA","EA",58.333333333333329,19250]
[null,"50129766-001",null," HL400-F Frame dispenser with 400 pairs FirmFit EU / UA ","EN 352-2",null,"1 unit","EA","EA",58.333333333333329,19250]
[null,"HL400 Lite with canisters and 400 pairs of earplugs"]
[null,"50129767-001",null," HL400 Lite dispenser with 400 pairs Bilsom 303L EU / AU ","EN 352-2",null,"1 unit","EA","EA",56.666666666666664,18700]
[null,"50129768-001",null," HL400 Lite dispenser with 400 pairs Bilsom 303S EU / AU ","EN 352-2",null,"1 unit","EA","EA",56.666666666666664,18700]
[null,"50129769-001",null," HL400 Lite dispenser with 400 pairs Laser Lite EU / AU ","EN 352-2",null,"1 unit","EA","EA",56.666666666666664,18700]
[null,"50129770-001",null," HL400 Lite dispenser with 400 pairs Max EU / AU ","EN 352-2",null,"1 unit","EA","EA",56.666666666666664,18700]
[null,"50129771-001",null," HL400 Lite dispenser with 400 pairs Max Lite EU / AU ","EN 352-2",null,"1 unit","EA","EA",56.666666666666664,18700]
[null,"50129772-001",null," HL400 Lite dispenser with 400 pairs MultiMax Lite EU / AU ","EN 352-2",null,"1 unit","EA","EA",56.666666666666664,18700]
[null,"50129773-001",null," HL400 Lite dispenser with 400 pairs FirmFit EU /AU ","EN 352-2",null,"1 unit","EA","EA",56.666666666666664,18700]
[null,"Canisters prefilled with earplugs"]
[null,"50129774-001",null," HL400 dispenser refill canister of  400 pairs Bilsom 303L EU / UA ","EN 352-2",null,"2 units","CAS","CAS",50,16500]
[null,"50129775-001",null," HL400 dispenser refill canister of  400 pairs Bilsom 303S EU / UA ","EN 352-2",null,"2 units","CAS","CAS",50,16500]
[null,"50129776-001",null," HL400 dispenser refill canister of  400 pairs Laser Lite EU / UA ","EN 352-2",null,"2 units","CAS","CAS",50,16500]
[null,"50129777-001",null," HL400 dispenser refill canister of  400 pairs Max EU / UA ","EN 352-2",null,"2 units","CAS","CAS",50,16500]
[null,"50129778-001",null," HL400 dispenser refill canister of 400 pairs Max Lite EU / UA ","EN 352-2",null,"2 units","CAS","CAS",50,16500]
[null,"50129779-001",null," HL400 dispenser refill canister of 400 pairs MultiMax EU / UA ","EN 352-2",null,"2 units","CAS","CAS",50,16500]
[null,"50129780-001",null," HL400 dispenser refill canister of 400 pairs FirmFit EU / UA ","EN 352-2",null,"2 units","CAS","CAS",50,16500]
[null," DISPENSERS AND REFILL PACKS"]
[null,1013040,null,"Leight Source  400 (LS 400) Empty. Can be fixed on a wall or placed on a table. Can hold 400 pairs of single -use earplugs such as: Max, Max Lite, Laser Lite, MultiMax, Matrix and Bilsom 303",null,null,"1 unit","BOX","EA",21.863636363636363,7215]
[null,1006202,null,"Leight Source 400 (LS400) dispenser supplied filled with 400 pairs of 303L earplugs, size Large. ","EN352-2",null,"400 units","BOX","BOX",50.38636363636364,16627.5]
[null,1006203,null,"Leight Source 400 (LS400) dispenser supplied filled with 400 pairs of 303S earplugs, size Small","EN352-2",null,"400 units","BOX","BOX",50.38636363636364,16627.5]
[null,1006186,null,"303L earplug refill pack for Leight Source 400 (LS400) dispenser, size Large","EN352-2",null,"200 pár","CAS","CAS",21.637878787878787,7140.5]
[null,1006187,null,"303S earplug refill pack for Leight Source 400 (LS400) dispenser, size Small","EN352-2",null,"200 pár","CAS","CAS",21.637878787878787,7140.5]
[null,1005852,null,"303L earplug supplied in the Leight Source 400 (LS400) hand dispenser, size Large                                                                                               ","EN352-2",null,"1200 units","CAS","CAS",15.227272727272728,5025]
[null,1005850,null,"303S earplug supplied in the Leight Source 400 (LS400) disposable hand dispenser, size Small          ","EN352-2",null,"1200 units","CAS","CAS",15.227272727272728,5025]
[null,1013047,null,"LASERLITE LS400 refill pack\nH: 34  M: 32  L: 31 SNR: 35                                                                                           ","EN352-2",null,"200 pár","CAS","CAS",21.992424242424242,7257.5]
[null,1013048,null,"MAXLITE LS400 refill pack\nH: 32  M: 32  L: 31  SNR: 34","EN352-2",null,"200 pár","CAS","CAS",23.3,7689]
[null,1013046,null,"MAX LS400 refill pack\nH: 36  M: 35 L: 34  SNR: 37","EN352-2",null,"200 pár","CAS","CAS",24.075757575757574,7944.9999999999991]
[null,1013042,null,"MATRIX Orange LS400 refill pack\nH: 31  M: 25  L: 22  SNR: 29","EN352-2",null,"2000 units","CAS","CAS",20.503030303030304,6766]
[null,1013045,null,"Howard Leight MULTIMAX REFILL LS400. SNR 35\n","EN352-2",null,"2000 units","CAS","CAS",27.293939393939393,9007]
[null,"LS500 EARPLUG DISPENSER AND REFILL PACKS",null,null,null,null,""]
[null,"Heavy-duty anodised aluminium wall mounted earplug station, dispenses plugs with the turn of a handle"]
[null,3301273,null,"LS500 earplug dispenser\nRefill packs are available as follows:",null,null,"1 unit","EA","EA",129.48484848484847,42729.999999999993]
[null,3301271,null,"LL-1D LASERLITE LS500 refill pack\nH: 34  M: 32  L: 31 SNR: 35                                                                                           ","EN352-2",null,"500 units","BOX","BOX",54.97727272727272,18142.499999999996]
[null,3301272,null,"LPF-1D MAXLITE LS500 refill pack\nH: 32  M: 32  L: 31  SNR: 34","EN352-2",null,"500 units","BOX","BOX",58.25,19222.5]
[null,3301165,null,"MAX-1D MAX LS500 refill pack\nH: 36  M: 35 L: 34  SNR: 37","EN352-2",null,"500 units","BOX","BOX",60.189393939393938,19862.5]
[null,1012723,null,"MATRIX Orange LS500 refill pack\nH: 31  M: 25  L: 22  SNR: 29","EN352-2",null,"2000 units","CAS","CAS",51.257575757575751,16914.999999999996]
[null,1017573,null,"303L LS500 refill pack\nH: 32  M: 29  L: 29  SNR: 33","EN352-2",null,"500 units","BOX","BOX",54.484848484848484,17980]
[null,1017574,null,"303S LS500 refill pack\nH: 32  M: 29  L: 29  SNR: 33","EN352-2",null,"500 units","BOX","BOX",54.484848484848484,17980]
[null,3301275,null,"QUIET re-usable LS500 refill pack\nH: 29  M: 25  L: 23  SNR: 28 ","EN352-2",null,"200 units","BOX","BOX",80.303030303030297,26499.999999999996]
[null,3301261,null,"Howard Leight MULTIMAX REFILL LS500",null,null,"500 units","BOX","BOX",68.242424242424235,22519.999999999996]
[null,"Hearing Protection |  Banded earplugs",null,null,null,null,""]
[null,"Reusable banded earplug with patented band design that prevents earpads from touching dirty or contaminated surfaces"]
[null,3301282,null,"QB1 HYG - Smooth, ergonomic earplugs fit in the ear for maximum protection\nH: 28  M: 22  L: 21  SNR: 26","EN352-2",null,"10 units","BOX","BOX",41.318181818181813,13634.999999999998]
[null,3301281,null,"QB1 HYG replacement earplugs","EN352-2",null,"50 units","BOX","BOX",93.583333333333329,30882.5]
[null,3301280,null,"QB2 HYG - Soft pods rest partially in the ear for a balance of protection and comfort\nH: 26  M: 20  L: 19  SNR: 24","EN352-2",null,"10 units","BOX","BOX",41.318181818181813,13634.999999999998]
[null,3301181,null,"QB2 HYG replacement pods","EN352-2",null,"50 units","BOX","BOX",93.583333333333329,30882.5]
[null,3301279,null,"QB3 HYG - Super soft pads rest on the opening of the ear for outstanding comfort\nH: 25  M: 19  L: 17  SNR: 23","EN352-2",null,"10 units","BOX","BOX",41.318181818181813,13634.999999999998]
[null,3301183,null,"QB3 HYG replacement pads","EN352-2",null,"50 units","BOX","BOX",93.583333333333329,30882.5]
[null,1005952,null,"5720 PERCAP orange banded earplug\nH: 27  M: 20  L: 18  SNR: 24","EN352-2",null,"10 units","CAS","CAS",31.606060606060602,10429.999999999998]
[null,1005980,null,"5730 replacement pods","EN352-2",null,"10 units","BOX","BOX",12.99242424242424,4287.4999999999991]
[null,"Hearing Protection |  NOISE BLOCKING EARMUFFS"]
[null,"Maximum comfort and contemporary design - features patented Air Flow Control™"]
[null,null,null,"AIR FLOW CONTROL™"]
[null,null,null,"Patented high performance design delivers superior low-frequency attenuation and"]
[null,null,null,"performs more consistently across the whole frequency range without increasing"]
[null,null,null,"the size or weight of the earmuff. Overall attenuation is improved because of the better"]
[null,null,null,"low-frequency attenuation."]
[]
[null,null,null,"How does it work?"]
[null,null,null,"• Air is the primary medium through which sounds travels "]
[null,null,null,"• Unique design allows air to move freely from inside the ear cushion to the outside"]
[null,null,null,"• Reduces ear cup vibration caused by low frequency noise"]
[]
[]
[null,"1034321-0",null,"Sync Wireless Impact Earmuff – Headband version. The earmuff connects wirelessly to mobile phones, and features a robust boom microphone that lets you answer calls + amplifies incoming sounds to 82dB. SNR30dB.Hygiene kit: 1035171","EN352-3",null,1,"BOX","EA",257.57575757575756,85000]
[null,"1034323-0",null,"Sync Wireless Impact EaRMUFF – Hard hat version. The earmuff connects wirelessly to mobile phones, and features a robust boom microphone that lets you answer calls + amplifies incoming sounds to 82dB. SNR30dB.Hygiene kit: 1035171","EN352-3",null,1,"BOX","EA",257.57575757575756,85000]
[null,1035170,null,"Sync Wireless Boom microphone kit (Boom microphone assemble kit-Wind cover-Assembly instruction)",null,null,1,"BOX","EA",39.393939393939391,12999.999999999998]
[null,1035171,null,"Sync Wireless Hygiene Kit",null,null,10,"KIT","BOX",68.939393939393938,22750]
[null,1035392,null,"Sync Wireless Wind Sock",null,null,50,"BOX","BOX",39.393939393939391,12999.999999999998]
[null,1034510,null,"New! Sync® Wireless Earmuff. The earmuff connects wirelessly to mobile phones,\nand features a robust boom microphone that lets you answer calls with the confidence you’ll be\nunderstood. SNR32dB.Hygiene kit: 1015280","EN352-2",null,"1 unit","BOX","EA",143.93939393939394,47500]
[null,1030334,null,"SYNC ELECTO H - Helmet version. Combines the FM Radio earmuff with advanced sound mplification technology advanced response technology.Amplifies incoming sounds to 82dB, then acts as a passive earmuff for sounds above 85dB.SNR (dB) 29 Db. Hygiene kit: 1015280. AA batteries included.\n\n","EN 352",null,"1 unit","BOX","EA",106.93939393939394,35290]
[null,1030111,null,"Sync Stereo Volume Management Technolog (VMT) maintaince the sound level from portable audio equipment at safe levels. SNR 31 (audio device not included). Hygiene kit 1030220",null,null,"2 units","BOX","EA",25.719696969696972,8487.5]
[null,1030330,null,"SYNCTM Digital AM/FM Radio Earmuff combines passive hearing protection with clean, crisp digital AM/FM radio and connectivity to listen to music through a personal listening device\nH: 29  M: 27  L: 22  SNR: 29\nHygiene kit: 1015280","EN352-1\nEN352-6\nEN352-8",null,"1 unit","BOX","EA",68.340909090909079,22552.499999999996]
[null,1030332,null,"SYNCTM Hi-Vis Digital AM/FM Radio Earmuff combines passive hearing protection with clean, crisp digital AM/FM radio and connectivity to listen to music through a personal listening device\nH: 29  M: 27  L: 22  SNR: 29\nHygiene kit: 1015280","EN352-1\nEN352-6\nEN352-8",null,"1 unit","BOX","EA",68.340909090909079,22552.499999999996]
[null,1030333,null,"SYNC ELECTO. Combines the FM Radio earmuff with advanced sound mplification technology. Advanced response technology amplifies incoming sounds to 82dB, then acts as a passive earmuff for sounds above 85dB.SNR (dB) 29 Db. Hygiene kit: 1015280. AA batteries included.",null,null,"1 unit","BOX","EA",106.93939393939394,35290]
[null,null,null,null,null,null,null,null,null,null,0]
[null,"CLARITY",null,null,null,null,null,null,null,null,0]
[null,"Advanced Sound Management Technology enhances on-the-job communication",null,null,null,null,null,null,null,null,0]
[null,1011142,null,"CLARITY C1\nH: 24 M: 22 L: 20 SNR: 25\nHygiene kit: 1006080","EN352-1",null,"1 DB","CAS","CAS",10.375757575757575,3424]
[null,1011143,null,"CLARITY C1F - Folding earmuff\nH: 25  M: 24  L: 19  SNR: 26\nHygiene kit: 1006080","EN352-1",null,"10 units","CAS","CAS",14.266666666666666,4708]
[null,1011262,null,"CLARITY C1H - Helmet earmuff\nH: 26  M: 23  L: 19  SNR: 26\nIncludes 3711 / 3712 helmet adaptors\nHygiene kit: 1006080","EN352-3",null,"10 units","CAS","CAS",10.375757575757575,3424]
[null,1011145,null,"CLARITY C2 - Multi-position earmuff\nH: 30  M: 29  L: 25  SNR: 30\nHygiene kit: 1006017","EN352-1",null,"10 units","CAS","CAS",12.971212121212121,4280.5]
[null,1011146,null,"CLARITY C3\nH: 31  M: 32  L: 29  SNR: 33\nHygiene kit: 1006081","EN352-1",null,"10 units","CAS","CAS",16.309090909090909,5382]
[null,1011264,null,"CLARITY C3H - Helmet Earmuff\nH: 28  M: 28  L: 24  SNR: 30\nIncludes 3711 / 3712 helmet adaptors\nHygiene kit: 1006081","EN352-3",null,"10 units","CAS","CAS",16.309090909090909,5382]
[null,null,null,null,null,null,""]
[null,"Hearing Protection |  EARMUFFS",null,null,null,null,""]
[null,"LEIGHTNING",null,null,null,null,""]
[]
[null,1013461,null,"LEIGHTNING L0F - Wire folding headband earmuff with comfort cushions and slimline earcups\nH: 27  M: 21  L: 17  SNR:  25\nHygiene kit: 1011998","EN352-1",null,"20 units","CAS","CAS",13.893939393939393,4585]
[null,1013460,null,"LEIGHTNING L0N - Wire neckband earmuff with comfort cushions and slimline earcups compatible with faceshields, welding screens and other PPE\nH: 24  M: 19  L: 14 SNR:  22\nHygiene kit: 1011998","EN352-1",null,"20 units","CAS","CAS",10.196969696969697,3365]
[null,1010922,null,"LEIGHTNING L1 - Wire headband earmuff with comfort cushions\nH: 31  M: 28  L:23  SNR: 30\nHygiene kit: 1011998","EN352-1",null,"1 db","CAS","CAS",10.375757575757575,3424]
[null,1012539,null,"LEIGHTNING L1H - Wire helmet earmuff with comfort cushions\nH: 31   M: 25   L: 19  SNR: 28\nIncludes 3711 / 3712 helmet adaptors\nHygiene kit: 1011998","EN352-3",null,"20 units","CAS","CAS",10.375757575757575,3424]
[null,1015021,null,"LEIGHTNING L1HHV - Hi-Vis Wire helmet earmuff with comfort cushions - High visibility earcups for enhanced worker safety\nH: 31   M: 25   L: 19  SNR: 28\nIncludes 3711 / 3712 helmet adaptors\nHygiene kit: 1011998 ","EN352-3",null,"20 units","CAS","CAS",10.927272727272726,3605.9999999999995]
[null,1011994,null,"LEIGHTNING L1N - Wire neckband earmuff with comfort cushions\nH: 31   M: 27   L: 21  SNR: 29\nHygiene kit: 1011998","EN352-1",null,"1 db","CAS","CAS",10.375757575757575,3424]
[null,1010923,null,"LEIGHTNING L2 - Wire headband earmuff with comfort cushions\nH: 31  M: 29  L: 23  SNR: 31\nHygiene kit: 1011999","EN352-1",null,"20 units","CAS","CAS",12.969696969696971,4280]
[null,1011997,null,"LEIGHTNING L2F - Wire folding headband earmuff with comfort cushions\nH: 32   M: 30   L: 24  SNR: 32\nHygiene kit: 1011999 ","EN352-1",null,"20 units","CAS","CAS",14.266666666666666,4708]
[null,1013942,null,"LEIGHTNING L2FHV - Hi-Vis Wire folding headband earmuff with comfort cushions - High visibility earcups and reflective headband for enhanced worker safety\nH: 32  M: 30  L: 24 SNR: 32\nHygiene kit: 1011999 ","EN352-1",null,"20 units","CAS","CAS",15.19090909090909,5013]
[null,1011995,null,"LEIGHTNING L2N - Wire neckband earmuff with comfort cushions\nH: 31   M: 29   L: 22  SNR: 31\nHygiene kit: 1011999","EN352-1",null,"20 units","CAS","CAS",12.969696969696971,4280]
[null,1010924,null,"LEIGHTNING L3 - Wire headband earmuff with comfort cushions\nH: 33  M: 32  L: 27  SNR: 34\nHygiene kit: 1012000","EN352-1",null,"20 units","CAS","CAS",15.563636363636363,5136]
[null,1013941,null,"LEIGHTNING L3HV - Hi-Vis Wire headband earmuff with comfort cushions - High visibility earcups and reflective headband for enhanced worker safety\nH: 33  M: 32  L: 27  SNR: 34\nHygiene kit: 1012000","EN352-1",null,"20 units","CAS","CAS",16.674242424242426,5502.5000000000009]
[null,1012541,null,"LEIGHTNING L3H - Wire helmet earmuff with comfort cushions\nH: 30  M:29  L: 24  SNR:  31\nIncludes 3711 / 3712 helmet adaptors\nHygiene kit: 1012000 ","EN352-3",null,"20 units","CAS","CAS",15.563636363636363,5136]
[null,1011996,null,"LEIGHTNING L3N - Wire neckband earmuff with comfort cushions\nH: 31  M: 31  L: 26 SNR: 32\nHygiene kit: 1012000","EN352-1",null,"20 units","CAS","CAS",15.563636363636363,5136]
[null,"MACH 1",null,null,null,null,""]
[null,"Fully adjustable, light weight earmuff offers effective, economical protection",null,null,null,null,""]
[null,1010421,null,"Mach 1 - Value headband earmuff\nH: 29  M: 20  L: 13  SNR: 23\nHygiene kit not available","EN352-1",null,"20 units","CAS","CAS",5.8606060606060604,1934]
[null,"HOWARD LEIGHT QM24+",null,null,null,null,""]
[null,"Multi-position headband for more wearing options",null,null,null,null,""]
[null,3302152,null,"QM24+ Value Multi-position headband earmuff\nH: 29  M: 23  L: 15 SNR: 26\nHygiene kit: 3301283","EN352-1",null,"20 units","BOX","BOX",7.4090909090909083,2444.9999999999995]
[null,null,null,null,null,null,""]
[null,"THUNDER",null,null,null,null,""]
[null,"Top of the line protection and comfort - features patented Air Flow Control™",null,null,null,null,""]
[null,1011600,null,"THUNDER T1F - Noise blocking folding earmuff\nH: 33  M: 28  L: 22  SNR: 31\nHygiene kit: 1010974","EN352-1",null,"10 units","CAS","CAS",14.266666666666666,4708]
[null,1012533,null,"THUNDER T1H - Noise blocking helmet earmuff\nH: 32  M: 26  L: 20  SNR: 29\nIncludes 3711 / 3712 helmet adaptors\nHygiene kit: 1010974","EN352-3",null,"10 units","CAS","CAS",10.384848484848485,3427]
[null,1010929,null,"THUNDER T2 - Noise blocking earmuff\nDual dielectric comfort headband\nH: 34  M: 31  L: 25  SNR: 33\nHygiene kit: 1010975","EN352-1",null,"10 units","CAS","CAS",13.156060606060604,4341.4999999999991]
[null,1010928,null,"Thunder T1s Headband Earmuff. IR FLOW CONTROL™ TECHNOLOGY Bilsom’s patented Air Flow Control™ technology delivers optimal attenuation across all frequencies, without increasing earcup size or weight. A patented baseplate chamber and high-tech non-woven layer manage the flow of air inside the earmuff to control how sound reaches the ear. The result is better, more consistent overall attenuation for virtually all industrial noise environments. Air Flow Control is a standard feature on all Thunder series earmuffs. DIELECTRIC/PLASTIC CONSTRUCTION ",null,null,"10 units","CAS","CAS",10.375757575757575,3424]
[null,1015820,null,"THUNDER T2HV - Noise blocking high visibility earmuff with dual dielectric comfort headband\nH: 34  M: 31  L: 25  SNR: 33\nHygiene kit: 1010975","EN352-1",null,"10 units","CAS","CAS",13.893939393939393,4585]
[null,1012534,null,"THUNDER T2H - Noise blocking helmet earmuff\nH: 32  M: 28  L: 23  SNR: 30\nIncludes 3711 / 3712 helmet adaptors\nHygiene kit: 1010975                                                                                      ","EN352-3",null,"10 units","CAS","CAS",13.156060606060604,4341.4999999999991]
[null,1010970,null,"THUNDER T3 - Noise blocking earmuff\nDual dielectric comfort headband\nH: 37  M: 34  L: 26  SNR: 36\nHygiene kit: 1010976","EN352-1",null,"1 db","CAS","CAS",16.674242424242426,5502.5000000000009]
[null,"VIKING",null,null,null,null,""]
[null,"Multi-position headband for more wearing options works with helmets, face-shields and other protective equipment"]
[null,"Features patented Air Flow Control™",null,null,null,null,""]
[null,1010925,null,"VIKING V1 - Multi-position earmuff\nH: 32  M: 28  L: 21  SNR: 30\nHygiene kit: 1011998","EN352-1",null,"20 units","CAS","CAS",9.8242424242424242,3242]
[null,1011170,null,"VIKING V3 - Multi-position headband earmuff\nH: 33  M: 30  L: 24  SNR: 32\nHygiene kit: 1012000","EN352-1",null,"20 units","CAS","CAS",15.19090909090909,5013]
[null,"Hearing Protection |  ELECTRONIC EARMUFFS",null,null,null,null,""]
[null,1034400,null,"IMPACT SPORT CAMOU - Low profile hearing protector for enhanced communication in environments affected by different noise levels and impulse sounds, integral 3.5mm input jack. Hygiene kit: 1015280","EN352-1                             EN352-4                            EN352-6",null,"1 unit",null,"EA",64.393939393939391,21250]
[null,1034490,null,"IMPACT SPORT BLACK - Low profile hearing protector for enhanced communication in environments affected by different noise levels and impulse sounds, integral 3.5mm input jack Hygiene kit: 1015280","EN352-1                             EN352-4                     EN352-6",null,"1 unit",null,"EA",87.651515151515156,28925]
[null,1013530,null,"IMPACT SPORT - Low profile hearing protector for enhanced communication in environments affected by different noise levels and impulse sounds, integral 3.5mm input jack\nH: 24  M: 22  L: 18  SNR: 25\nHygiene kit: 1015280","EN352-1\nEN352-4\nEN352-6",null,"1 unit","EA","EA",64.393939393939391,21250]
[null,1018953,null,"NEW IMPACT PRO - High attenuation sound amplification earmuff, amplifies low volume sound and conversation up to 4 times louder, automatically cuts out loud impact noise, integral 3.5mm input jack\nH: 32  M: 31  L: 26  SNR: 33\nHygiene Kit: 1030220","EN352-1\nEN352-4\nEN352-6",null,"1 unit","EA","EA",63.446969696969695,20937.5]
[null,1034491,null," IMPACT PRO INDUSTRIAL - High attenuation sound amplification earmuff, amplifies low volume sound and conversation up to 4 times louder, automatically cuts out loud impact noise, integral 3.5mm input jack Hygiene Kit: 1030220","EN352-1    EN352-4   EN352-6",null,"1 unit",null,"EA",63.446969696969695,20937.5]
[null,1010376,null,"IMPACT - Hearing protector for environments affected by impulse sounds\nH: 30  M: 25  L: 20  SNR: 28\nHygiene kit: 1008000","EN352-1\nEN352-4\n",null,"1 unit","EA","EA",120.92424242424242,39905]
[null,1010632,null,"IMPACT Helmet earmuff - as above but for safety helmet - Helmet adapters are required\nH: 27  M: 25  L: 19  SNR: 27\nHygiene kit: 1008000","EN352-3\nEN352-4\n",null,"1 unit","EA","EA",120.92424242424242,39905]
[null,"FORESTRY ",null,null,null,null,""]
[null,"Combined hearing protection and face protection",null,null,null,null,""]
[null,1017291,null,"Forestry Kit; Leightning L1H earmuff complete with safety helmet and mesh visor\nH: 31   M: 25   L: 19  SNR: 28\nHygiene kit: 1011998","EN352-3\nEN1731",null,"1 unit","EA","EA",34.295454545454547,11317.5]
[null,1017292,null,"Garden Kit; Leightning L1 headband earmuff complete with mesh visor\nH: 31  M: 28  L:23  SNR: 30\nHygiene kit: 1011998","EN352-1\nEN1731",null,"1 unit","EA","EA",24.946969696969695,8232.5]
[null,1017800,null,"Mesh faceshield complete with carrier","EN1731",null,"1 unit","EA","EA",7.9772727272727266,2632.5]
[null,1017293,null,"Mesh faceshield without carrier","EN1731",null,"1 unit","EA","EA",6.7045454545454541,2212.5]
[null,1017294,null,"Clear faceshield without carrier","EN166-F",null,"1 unit","EA","EA",12.636363636363635,4169.9999999999991]
[]
[null,"Hearing Protection |  EARMUFF ACCESSORIES",null,null,null,null,""]
[null,1016730,null,"Secure belt-clip attachment for all headband earmuffs",null,null,"10 units","BOX","BOX",13.113636363636362,4327.4999999999991]
[null,3302101,null,"OPTISORB - Absorbent cotton sleeve fits over ear cup for increased wearer comfort. Washable. 100% cotton, provides optimum comfort and hygine. ",null,null,"50 units","BOX","BOX",58.143939393939391,19187.5]
[null,"Hygiene Kit | Contains replacement cushions and foam insert"]
[null,1006080,null,"Hygiene kit for Clarity C1,C1H,C1F",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1006081,null,"Hygiene kit for Clarity C2,C3,C3H",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1010974,null,"Hygiene kit for  Thunder T1/ T1H/ T1F",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1010975,null,"Hygiene kit for  Thunder T2/ T2H/ T2HV",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1010976,null,"Hygiene kit for  Thunder T3/T3H",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1011998,null,"Hygiene kit for Leightning L1, L1H/L1N/L0N/L1HHV/Viking V1",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1011999,null,"Hygiene kit for Leightning L2/L2H/L2N/L2F/L2FHV",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1012000,null,"Hygiene kit for  Leightning L3/L3H/L3N/L3F/L3FHV",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,1008000,null,"Hygiene kit for Radio, Radio HV/ Electo/ Electo H/ Impact/ Impact H",null,null,"1 doboz / 10 szett","CAS","BOX",59.909090909090907,19770]
[null,1015280,null,"Hygiene kit for Impact Sport/ Sync Radio/ Sync Radio HiViz/ Sync Electo/Sync Wireless",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,3301283,null,"Hygiene kit for  QM24+",null,null,"20 pairs","BOX","BOX",121.62121212121211,40135]
[null,1030220,null,"Hygiene kit for  Sync/Impact PRO/Impact PRO Industrial",null,null,"1 doboz / 10 szett","CAS","BOX",60.803030303030305,20065]
[null,"Hearing Protection |  EARMUFF ACCESSORIES",null,null,null,null,""]
[null,1000365,null,"BILSOM COOL II  EAR CUSHIONS ENVELOPE PACK - Absorbent pad for increased comfort and hygiene, made of dermatologically tested material. Cool Pad fits most brands of earmuffs on the market. ",null,null,"100 pairs","BOX","BOX",65.803030303030297,21714.999999999996]
[null,1000364,null,"BILSOM COOL II EAR CUSHIONS DISPENSER PACK - Absorbent pad for increased comfort and hygiene, made of dermatologically tested material. Cool Pad fits most brands of earmuffs on the market. . ",null,null,"100 pairs","BOX ","BOX ",65.803030303030297,21714.999999999996]
[null,"HELMET EARMUFF ADAPTERS",null,null,null,null,""]
[null,1000240,null,"3702 Universal clip-on adapter",null,null,"20 units","CAS","CAS",6.0803030303030301,2006.5]
[null,1000241,null,"3710 Universal bolt-on adapter",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1000242,null,"3711 Adaptor to suit Centurion 1100, 1125 helmets",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1000243,null,"3712 Adaptor to suit JSP Panorama Invincible, Mark IV, Mark V",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1000248,null,"3717 Adaptor to suit JSP MKII and JSP MKIII helmets",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1000249,null,"3718 Adaptor to suit NORTH Peak series and MSA V GARD helmets",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1000245,null,"Adaptor 3714 Protector,AO,JSP,Domeguard ",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1000246,null,"Adaptor 3715 Auboueix ",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1000247,null,"Adaptor 3716 Schubert ",null,null,"20 units","CAS","CAS",1.5530303030303028,512.49999999999989]
[null,1005292,null,"Howard Leight ADAPTOR PROTECTOR 600 3721",null,null,"20 units","CAS","CAS",1.5606060606060606,515]
[null,"*Adapters for other safety helmets are available upon request",null,null,null,null,""]
[]
[null,null,null,"POLAR HOOD - Cold weather hood that can be worn with earmuffs without loss of attenuation",null,null,""]
[null,1016871,null,"● Size S / M",null,null,"5 units","CAS","CAS",27.739393939393938,9154]
[null,1016870,null,"● Size L / XL",null,null,"5 units","CAS","CAS",27.739393939393938,9154]
[null,1000251,null,"EARMUFFS BELT CASE. Durable nylon with belt loops and easy to open Velcro. Flap. Folds flat. Fits to : Leightning L2F, Leightning High Visibility L2FHV, Thunder,  T1F, Clarity C1F and Impact Sport earmuffs. ",null,null,10,"CAS","CAS",10.346969696969696,3414.4999999999995]
[]
[null,"Hearing Protection |  INTELLIGENT HEARING",null,null,null,null,""]
[null,"VERIPRO",null,null,null,null,""]
[null,"VeriPRO™ from Howard Leight measures real-world attenuation of earplugs to deliver an accurate, individual picture of"]
[null,"hearing protection. A user-friendly software interface finds the Personal Attenuation Rating (PAR) your employees are "]
[null,"receiving from their earplugs. Find out whether your employees are receiving optimal protection, require training, or need "]
[null,"to try a new hearing protector."]
[null,"● Works with any earplug, provides results in minutes"]
[null,"● Enhances hearing conservation program effectiveness"]
[null,"● BSIF Product Innovation Award Winner 2010"]
[null,1018064,null,"VeriPRO",null,null,"1 unit","","EA",1960.7954545454545,637258.52272727271]
[null,1000363,null,"Audiometric Cabin",null,null,"1 unit","","EA",6281.924242424242,2041625.3787878787]

{"sheet":"Eye & Face Protection","index":2,"n_rows":657,"n_cols":11,"rows_kept":657,"cut":false,"hidden":false,"merged":[]}
[null,"Eye & Face Protection |  SAFETY SPECTACLES",null,null,null,null,""]
[null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per","NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,null,null,null,null,null,""]
[null,"Eye & Face Protection |  SAFETY SPECTACLES",null,null,null,null,""]
[null,"ADAPTECTM"]
[null,"Adaptec adjustable eyewear system can be worn by the widest range of workers to deliver excellent protection,"]
[null,"superior comfort, customised adjustability, premium optics and a stylish look"]
[null,"• Micro-adjusting temple design (patent pending) allows customised temple tension for personal comfort and security"]
[null,"• Ratcheting temple hinges adjust lens angle for greater protection and reduced fogging"]
[null,"• Three position nose bridge is simple to adjust and keeps eyes centered in the lens for optimum protection"]
[null,null,null,null,null,null,""]
[null,null,null,"Adaptec with black / red frame and Clear lens","2C-1,2 \n1 FT KN",null,"10 pairs"]
[null,"1030739HS",null,"● Size Narrow",null,null,"10 units","BOX","EA",10.606060606060606,3500]
[null,"1030749HS",null,"● Size Regular",null,null,"10 units","BOX","EA",10.606060606060606,3500]
[null,"1030759HS",null,"● Size Wide",null,null,"10 units","BOX","EA",10.606060606060606,3500]
[null,null,null,"Adaptec with black / red frame and Amber lens","2C-1,2 \n1 FT KN",null,"10 pairs"]
[null,"1030738HS",null,"● Size Narrow",null,null,"10 units","BOX","EA",10.795454545454545,3562.5]
[null,"1030748HS",null,"● Size Regular",null,null,"10 units","BOX","EA",10.795454545454545,3562.5]
[null,"1030758HS",null,"● Size Wide",null,null,"10 units","BOX","EA",10.795454545454545,3562.5]
[null,null,null,"Adaptec with black / red frame and Smoke lens","2C-3\n5-3.1\n1 FT KN",null,"10 pairs"]
[null,"1030744HS",null,"● Size Narrow",null,null,"10 units","BOX","EA",11.234848484848484,3707.5]
[null,"1030754HS",null,"● Size Regular",null,null,"10 units","BOX","EA",11.242424242424242,3710]
[null,"1030764HS",null,"● Size Wide",null,null,"10 units","BOX","EA",11.242424242424242,3710]
[]
[null,null,null,"Adaptec with black / red frame and IR 5.0 lens","5\n1 FT",null,"10 pairs"]
[null,"1030737HS",null,"● Size Narrow",null,null,"10 units","BOX","EA",14.666666666666666,4840]
[null,"1030747HS",null,"● Size Regular",null,null,"10 units","BOX","EA",14.666666666666666,4840]
[null,"1030757HS",null,"● Size Wide",null,null,"10 units","BOX","EA",14.666666666666666,4840]
[null,null,null,null,null,null,""]
[null,"SVP200"]
[null,"Economical and stylish eye protection with comfortable fit"]
[null,1928860,null,"Honeywell SVP200 Clear frame, Clear lens, HC ","2C-1.2 1 F",null,"10 units","BOX","EA",1.5151515151515151,500]
[null,1928861,null,"Honeywell SVP200 Clear frame, Clear lens, AF ","2C-1.2 1 F",null,"10 units","BOX","EA",1.7424242424242422,574.99999999999989]
[null,1928862,null,"Honeywell SVP 200 Gray frame, Grey lens, HC ","5-2.5 1 F",null,"10 units","BOX","EA",1.5151515151515151,500]
[null,1928863,null,"Honeywell SVP 200 Gray frame, Grey lens, AF ","5-2.5 1 F",null,"10 units","BOX","EA",1.7424242424242422,574.99999999999989]
[null,1928864,null,"Honeywell SVP 200 Amber frame, Amber lens, AF","2C-1.2 1 F",null,"10 units","BOX","EA",1.7424242424242422,574.99999999999989]
[null,1928865,null,"Honeywell SVP 200 Amber frame, Amber lens, HC","2C-1.2 1 F",null,"10 units","BOX","EA",1.5151515151515151,500]
[null,"A700",null,null,null,null,""]
[null,"Economical and stylish eye protection with sport temples for a fashionable yet comfortable fit",null,null,null,null,""]
[null,"• Secure wrap-around design with Soft temple tip pads for a secure fit",null,null,null,null,""]
[null,1015361,null,"A700 with Clear anti-scratch lens ","2C-1.2 \n1 F",null,"10 units","BOX","EA",1.8181818181818181,600]
[null,1015360,null,"A700 with Clear Fog-Ban anti-scratch lens ","2C-1.2\n1 F",null,"10 units","BOX","EA",2.5757575757575757,850]
[null,1015362,null,"A700 with TSR Grey anti-scratch lens minimises outdoor sunlight and glare","5-2.5\n1 F",null,"10 units","BOX","EA",2.2727272727272725,749.99999999999989]
[null,1015351,null,"A700 with TSR Grey Fog-Ban anti-scratch lens minimises outdoor sunlight and glare","5-2.5\n1 F",null,"10 units","BOX","EA",2.7727272727272725,914.99999999999989]
[null,1015441,null,"A700 with HDL Yellow anti-scratch lens for enhanced contrast in low light conditions","2C-1.2\n1 F",null,"10 units","BOX","EA",2.2272727272727271,734.99999999999989]
[null,1015440,null,"A700 with blue mirror anti-scratch lens for outdoor use - reflects sunlight and glare","5-3.1\n1 F",null,"10 units","BOX","EA",2.7727272727272725,914.99999999999989]
[null,"A800",null,null,null,null,""]
[null,"Sporty styling and a slim profile provide an ideal fit for workers with smaller faces",null,null,null,null,""]
[null,"● Temples feature soft, padded inserts with extra flex for greater comfort ",null,null,null,null,""]
[null,"● Polycarbonate 9-base wrap-around lens provides a 180° field of distortion-free vision",null,null,null,null,""]
[null,1015370,null,"A800 with Clear anti-scratch lens ","2C-1.2\n1 F",null,"10 units","BOX","EA",2.5757575757575757,850]
[null,1015369,null,"A800 with Clear Fog-Ban anti-scratch lens ","2C-1.2\n1 F",null,"10 units","BOX","EA",3.0303030303030303,1000]
[null,1015368,null,"A800 with TSR Grey anti-scratch lens minimises outdoor sunlight and glare","5-2.5\n1 F",null,"10 units","BOX","EA",2.6742424242424239,882.49999999999989]
[null,1015367,null,"A800 with TSR Grey Fog-Ban anti-scratch lens minimises outdoor sunlight and glare","5-2.5\n1 F",null,"10 units","BOX","EA",3.1363636363636358,1034.9999999999998]
[null,1015350,null,"A800 with light I/O silver lens, ideal for workers moving from indoor to outdoor locations for reduced glare","5-1.7\n1 F",null,"10 units","BOX","EA",3.1363636363636358,1034.9999999999998]
[null,"XV100 "]
[null,1028860,null,"XV100 with Clear, abrasion resistant lens","2C-1.2 1 FT",null,"10 units","BOX","EA",2.5454545454545454,840]
[null,1029691,null,"XV with yellow HDL anti-fog lens","2C-1.2 1 FT",null,"1 db","BOX","EA",2.7424242424242422,904.99999999999989]
[null,1029692,null,"XV100 with abrasion resistant TSR Grey lens","5-2.5 1 FT",null,"1 db","BOX","EA",2.6363636363636362,870]
[null,1028862,null,"XV100 with clear anti-fog lens","2C-1.2 1 FT",null,"10 units","BOX","EA",2.7424242424242422,904.99999999999989]
[null,1028861,null,"XV100 with abrasion resistant I-O lens","5C-1.7 1 FT",null,"1 db","BOX","EA",2.7424242424242422,904.99999999999989]
[]
[null,"SANTA CRUZ"]
[null,1002675,null,"SANTA CRUZ. Clear ",null,null,"10 units","BOX","EA",5.045454545454545,1664.9999999999998]
[null,1002677,null,"SANTA CRUZ",null,null,"10 units","BOX","EA",4.7575757575757578,1570]
[null,1002676,null,"SANTA CRUZ. Blue frame , clear lenses",null,null,"10 units","BOX","EA",5.3106060606060606,1752.5]
[]
[null,"Eye & Face Protection |  SAFETY SPECTACLES",null,null,null,null,""]
[null,"ALEXIA™",null,null,null,null,""]
[null,"Specifically designed to fit women, Alexia™ is narrower across the front, shorter at the temple and slimmer in the nose"]
[null,"bridge providing optimum fit and coverage for a woman’s face"]
[null,"● Styling details, such as the crystal accents on each side of the lens produce a fashionable look that appeals to female"]
[null," workers, helping to drive overall compliance levels"]
[null,null,null,null,null,null,""]
[null,1028111,null,"ALEXIA with Clear, abrasion resistant lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",5.0757575757575752,1674.9999999999998]
[null,1028113,null,"ALEXIA with Clear abrasion resistant and anti-fog lens","2C-1.2\n1 FT",null,"1 db","BOX","EA",5.545454545454545,1829.9999999999998]
[null,1028114,null,"ALEXIA with abrasion resistant Macchiato lens","5-1.7/2.5\n1 FT",null,"1 db","BOX","EA",6.0151515151515156,1985.0000000000002]
[null,1028115,null,"ALEXIA  with abrasion resistant I/O Silver lens","2C-1.7\n1 FT",null,"10 units","BOX","EA",6.0151515151515156,1985.0000000000002]
[null,null,null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,"HI-STYLE",null,null,null,null,""]
[null,"An integral temple wire provides side arm adjustment for a precise and individual fit",null,null,null,null,""]
[null,1002267,null,"HI-STYLE 6012C with cobalt blue frame and Clear lens","1 FK",null,"10 units","BOX","EA",10.045454545454545,3315]
[]
[null,"HORIZON",null,null,null,null,""]
[null,"Highly technical spectacle with adjustable temple wires, can be fitted with optional flip-up lenses"]
[null,"3024147-STD",null,"HORIZON with blue frame and reinforced mineral glass Lens (flip up lens not included)","1 S",null,"10 units","BOX","EA",22.27272727272727,7349.9999999999991]
[null,"3024130-STD",null,"HORIZON with blue frame (size 54 mm), Clear polycarbonate, Anti-scratch  (flip up lens not included)",null,null,"10 units","BOX","EA",15.689393939393939,5177.5]
[null,"FLIP-UP LENSES FOR USE WITH HORIZON",null,null,null,null,""]
[null,"3024040-STD",null,"Flip up IR shade 1.7 lens","1.7\n2 F",null,"10 units","BOX","EA",14.393939393939393,4750]
[null,"3024041-STD",null,"Flip up IR shade 3 lens","3.0\n2 F",null,"10 units","BOX","EA",14.393939393939393,4750]
[null,"3024042-STD",null,"Flip up IR shade 5 lens","5.0\n2 F",null,"10 units","BOX","EA",14.393939393939393,4750]
[null,"3024075-STD",null,"Flip-up blue cobalt mineral glass lens","4-6\n1 S",null,"10 units ","BOX","EA",23.742424242424242,7835]
[null,"MILLENNIA 2G"]
[null,"The next generation of Millennia, the Millennia 2G safety spectacle offers greater coverage, better peripheral vision and "]
[null,"more comfort features, in a better looking design"]
[null,"● Classic, simple design, with a sporty touch"]
[null,"● Soft, flexible frame material provides better comfort against the head and ears"]
[null,"● Greater lens coverage to protect the eyes, brow area and under the cheeks"]
[null,"● Improved peripheral vision and less frame interference enhances overall field of vision"]
[null,1032175,null,"MILLENNIA 2G with black frame and Clear abrasion resistant lens","2C-1.2 \n1 FT",null,"10 units","BOX","EA",5.1212121212121211,1690]
[null,1032176,null,"MILLENNIA 2G with black frame and TSR Grey abrasion resistant lens","2C-2.5\n5-2.5\n1 FT",null,"10 units","BOX","EA",6.583333333333333,2172.5]
[null,1032177,null,"MILLENNIA 2G with black frame and HDL Yellow abrasion resistant lens","2C-1.2 \n1 FT",null,"10 units","BOX","EA",6.583333333333333,2172.5]
[null,1032178,null,"MILLENNIA 2G with black frame and I/O Silver abrasion resistant lens","2C-1.7\n5-1.7\n1 FT",null,"10 units","BOX","EA",6.583333333333333,2172.5]
[null,1032179,null,"MILLENNIA 2G with black frame and Clear Fog-Ban lens","2C-1.2 \n1 FT",null,"10 units","BOX","EA",5.8106060606060606,1917.5]
[null,1032180,null,"MILLENNIA 2G with black frame and TSR Grey Fog-Ban lens","2C-2.5\n5-2.5\n1 FT",null,"10 units","BOX","EA",6.7424242424242422,2225]
[null,1032181,null,"MILLENNIA 2G with black frame and HDL Yellow Fog-Ban lens","2C-1.2 \n1 FT",null,"10 units","BOX","EA",6.7424242424242422,2225]
[null,1032182,null,"MILLENNIA 2G with black frame and  Shade 3 Green abrasion resistant lens","3\n1 FT",null,"10 units","BOX","EA",7.6060606060606046,2509.9999999999995]
[null,1032183,null,"MILLENNIA 2G with black frame and  Shade 5 Green abrasion resistant lens","5\n1 FT",null,"10 units","BOX","EA",7.6060606060606046,2509.9999999999995]
[null,"*Each Millennia 2G spectacle is supplied with a Flexicord retainer",null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,"MILLENNIA",null,null,null,null,""]
[null,"9-Base curve lens design for excellent optical qualities",null,null,null,null,""]
[null,"● Straight temple arms with Sensitive Tension Design for a balanced and comfortable fit",null,null,null,null,""]
[null,"● Parallel Vision Control for greater visual comfort and an adjustable, breakaway Flexicord retainer for added security"]
[null,1000001,null,"MILLENNIA with black frame and Clear abrasion resistant lens","2C-1.2\n1 F",null,"10 units","BOX","EA",5.8106060606060606,1917.5]
[null,1002781,null,"MILLENNIA with black frame and Clear abrasion resistant Fog-Ban lens","2C-1.2\n1 F",null,"10 units","BOX","EA",6.2803030303030294,2072.4999999999995]
[null,1000006,null,"MILLENNIA with blue frame and Clear abrasion resistant lens","2C-1.2\n1 F",null,"10 units","BOX","EA",5.8106060606060606,1917.5]
[null,1002783,null,"MILLENNIA with blue frame and Clear Fog-Ban abrasion resistant lens","2C-1.2\n1 F",null,"10 units","BOX","EA",6.2651515151515147,2067.5]
[null,1000002,null,"MILLENNIA with black frame and TSR Grey abrasion resistant lens","5-2.5\n1 F",null,"10 units","BOX","EA",6.5151515151515147,2150]
[null,1002782,null,"MILLENNIA with black frame and TSR Grey abrasion resistant Fog-Ban lens","5-2.5\n1 F ",null,"10 units","BOX","EA",6.9242424242424248,2285]
[null,1000003,null,"MILLENNIA with black frame and HDL Yellow abrasion resistant lens","2C-1.2\n1 F",null,"10 units","BOX","EA",6.5151515151515147,2150]
[null,1005212,null,"MILLENNIA with black frame and HDL Yellow abrasion resistant Fog-Ban lens","2C-1.2\n1 F",null,"10 units","BOX","EA",6.9242424242424248,2285]
[null,1000004,null,"MILLENNIA with black frame and I/O Silver abrasion resistant lens","5-1.7\n1 F",null,"10 units","BOX","EA",8.0303030303030294,2649.9999999999995]
[null,1000005,null,"MILLENNIA with black frame and Silver Mirror abrasion resistant lens","5-3.1\n1 F",null,"10 units","BOX","EA",8.0303030303030294,2649.9999999999995]
[null,1006405,null,"MILLENNIA with black frame and  Shade 3 Green abrasion resistant lens","3.0 \n1 F ",null,"1 db","BOX","EA",9.4999999999999982,3134.9999999999995]
[null,1006406,null,"MILLENNIA with black frame and  Shade 5 Green abrasion resistant lens","5.0\n1 F",null,"10 units","BOX","EA",9.4999999999999982,3134.9999999999995]
[null,1000009,null,"Millenia Silver. Clear  lenses. Anti-Scratch",null,null,"10 units","BOX","EA",5.8106060606060606,1917.5]
[]
[null,1006032,null,"MILLENIA SPORT. Clear frame, grey lenses",null,null,"10 units","BOX","EA",5.7575757575757569,1899.9999999999998]
[null,"REPLACEMENT LENSES",null,null,null,null,""]
[null,1000011,null,"Clear",null,null,"10 units","BOX","EA",4.4924242424242422,1482.5]
[null,1000013,null,"HDL Yellow",null,null,"10 units","BOX","EA",5.1818181818181817,1710]
[null,1000015,null,"Silver Mirror",null,null,"10 units","BOX","EA",6.9696969696969688,2299.9999999999995]
[null,1002787,null,"Clear Fog-Ban Lens",null,null,"10 units","BOX","EA",5.2575757575757578,1735]
[null,"*Each Millennia spectacle is supplied with a Flexicord retainer",null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,"Eye & Face Protection |  SAFETY SPECTACLES",null,null,null,null,""]
[null,"MILLENNIA SPORT",null,null,null,null,""]
[null,"Sport styling with abrasion resistant lens",null,null,null,null,""]
[null,1005981,null,"MILLENNIA SPORT with black frame and Clear lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",4.8560606060606055,1602.4999999999998]
[null,1005985,null,"MILLENNIA SPORT with black frame and Clear Fog-Ban lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",5.3030303030303028,1750]
[null,1005982,null,"MILLENNIA SPORT with black frame and TSR Grey lens","5-2.5\n1 FT",null,"10 units","BOX","EA",5.4015151515151514,1782.5]
[null,1005986,null,"MILLENNIA SPORT with black frame and TSR Grey Fog-Ban lens","5-2.5\n1 FT",null,"10 units","BOX","EA",5.7575757575757569,1899.9999999999998]
[null,1005987,null,"MILLENNIA SPORT with teal frame and Clear lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",4.8560606060606055,1602.4999999999998]
[null,1006031,null,"MILLENNIA SPORT with teal frame and Clear Fog-Ban lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",5.3030303030303028,1750]
[null,"*Each Millennia Sport spectacle is supplied with a Flexicord retainer",null,null,null,null,""]
[null,"OP-TEMA",null,null,null,null,""]
[null,"Abrasion resistant polycarbonate lens with 6-base curve design and adjustable side-arms",null,null,null,null,""]
[null,1000016,null,"OP-TEMA spectacle with black frame and Clear lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",3.9469696969696968,1302.5]
[null,1000018,null,"OP-TEMA spectacle with blue frame Clear lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",3.9469696969696968,1302.5]
[null,1004947,null,"OP-TEMA spectacle with black frame Clear Fog-Ban lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",4.3560606060606055,1437.4999999999998]
[null,1004949,null,"OP-TEMA spectacle with blue frame and Clear Fog-Ban lens","2C-1.2\n1 FT",null,"10 units","BOX","EA",4.3560606060606055,1437.4999999999998]
[null,1000017,null,"OP-TEMA spectacle with black frame and TSR Grey lens","5-2.5\n1 FT",null,"10 units","BOX","EA",4.1439393939393936,1367.4999999999998]
[null,1004948,null,"OP-TEMA spectacle with black frame and TSR Grey Fog-Ban lens","5-2.5\n1 FT",null,"10 units","BOX","EA",4.5757575757575752,1509.9999999999998]
[null,1004960,null,"OP-TEMA spectacle with blue frame and TSR Grey Fog-Ban lens","5-2.5\n1 FT",null,"10 units","BOX","EA",4.5757575757575752,1509.9999999999998]
[null,1000020,null,"OP-TEMA Blue frame, grey lenses",null,null,"10 units","BOX","EA",3.9469696969696968,1302.5]
[null,"*Each Op-tema spectacle is supplied with a Flexicord retainer",null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,"PROTÉGÉ",null,null,null,null,""]
[null,"Radical styling and floating lens design for increased flexibility of fit"]
[null,"● Metallic black plastic frame and polycarbonate 7-base wrap-around lens"]
[null,"● Expandable wrap-around brow conforms to wearer's face profile"]
[null,"● Soft temple tip pads and clear nose pads for a secure comfortable fit"]
[null,"New PROTEGE with Hydroshield lens (K,N marking on both side of the lens)"]
[null,"1015364HS",null,"PROTÉGÉ with Clear Hydroshield lens ","2C-1,2 1FT KN",null,"10 units","BOX","EA",6.416666666666667,2117.5]
[null,"1015353HS",null,"PROTÉGÉ with TSR Grey Hydroshield lens minimises outdoor sunlight and glare","5C-2.5 1FT KN",null,"10 units","BOX","EA",6.8712121212121211,2267.5]
[null,"1016342HS",null,"PROTÉGÉ with HDL Yellow Hydroshield lens for enhanced contrast in low light conditions","2C-1.2 1FT KN",null,"19 units","BOX","EA",6.8712121212121211,2267.5]
[null,1015366,null,"PROTÉGÉ with Clear anti-scratch lens ","2C-1.2\n1 FT",null,"10 units","BOX","EA",5.4015151515151514,1782.5]
[null,1015363,null,"PROTÉGÉ with TSR Grey anti-scratch lens minimises outdoor sunlight and glare","5-2.5\n1 FT",null,"10 units","BOX","EA",5.9621212121212119,1967.5]
[null,1016341,null,"PROTÉGÉ with HDL Yellow anti-scratch lens for enhanced contrast in low light conditions","2C-1.2\n1 FT",null,"10 units","BOX","EA",6.0606060606060606,2000]
[null,1015689,null,"PROTÉGÉ with light I/O silver lens, ideal for workers moving from indoor to outdoor locations for reduced glare","5-1.7\n1 FT",null,"10 units","BOX","EA",7.2651515151515147,2397.5]
[]
[null,"PROTÉGÉ Extreme "]
[null,1031270,null,"Protégé Extreme Clr,Supra-Dura\n",null,null,"10 units","BOX","EA",6.75,2227.5]
[null,1031271,null,"Protégé Extreme CLR, Dura-Streme",null,null,"10 units","BOX","EA",7.6969696969696964,2540]
[null,1031272,null,"Protégé Extreme Blue Mist, FB+",null,null,"10 units","BOX","EA",8.2424242424242422,2720]
[null,1031273,null,"Protégé Extreme HDL.Yellow, FB+",null,null,"10 units","BOX","EA",8.2424242424242422,2720]
[null,1031274,null,"Protégé Extreme, I/O Silver",null,null,"10 units","BOX","EA",8.3787878787878789,2765]
[null,1031275,null,"Protégé Extreme SCT, Supra Dura",null,null,"10 units","BOX","EA",8.2424242424242422,2720]
[null,null,null,null,null,null,""]
[null,"SP10002G",null,null,null,null,""]
[null,"Provides protection against impact, wind, dust and airborne debris. Ideal for dirty, high-particulate work environments"]
[null,null,null,"• Flexible design can be used with temple arm or headband (both included)"]
[null,null,null,"• Premier comfort and seal with high-quality face cushioning and flexible nose piece"]
[null,null,null,"• Exceptional peripheral vision and coverage with wrap-around 8-base dual-lens style"]
[null,null,null,"• Anti-mist performance due to indirect vents and anti-fog/anti-scratch coating"]
[null,1028640,null,"SP10002G Clear ","2C-1.2 \n1 BT 3 KN",null,"10 units","BOX","EA",12.598484848484848,4157.5]
[null,1028644,null,"SP10002G HDL Yellow","2C-1.2\n1 BT 3 KN",null,"10 units","BOX","EA",12.969696969696971,4280]
[null,1028643,null,"SP10002G HDL Grey","2C-2.5\n5-2.5 \n1 BT 3 KN",null,"10 units","BOX","EA",12.969696969696971,4280]
[null,null,null,null,null,null,""]
[null,"XC",null,null,null,null,""]
[null,"X-Tra Comfort, X-Tra Coverage, X-Tra Control"]
[null,"● MMT - Multi-Material Technology for all day comfort"]
[null,"● 9 base-curved lens for total wrap-around coverage and exceptional peripheral vision"]
[null,"● Adjustable temples and lenses with a flexible nose bridge to ensure an excellent fit"]
[null,"XC with new Hydroshield lens (K&N marking on both side of the lens)"]
[null,"1011027HS",null,"XC blue frame, Clear Hydroshield lens","2C-1,2 1 FT KN",null,"1 db","BOX","EA",9.3409090909090899,3082.4999999999995]
[null,"1011025HS",null,"XC blue frame, TSR Gray Hydroshield lens","5C-2,2 1FT KN",null,"10 units","BOX","EA",10.954545454545455,3615]
[null,"1012900HS",null,"XC blue frame, HDL yellow Hydroshield lens","2C-1,2 1 FT KN",null,"1 db","BOX","EA",10.954545454545455,3615]
[null,1010950,null,"XC blue frame, Clear abrasion resistant lens","2C-1.2 \n1 FT",null,"10 units","BOX","EA",8.0303030303030294,2649.9999999999995]
[null,1018270,null,"XC blue frame, Clear lens with Dura-streme™ coating technology","2C-1.2\n1 FT KN",null,"10 units","BOX","EA",10.719696969696969,3537.4999999999995]
[null,1011026,null,"XC blue frame, TSR Grey lens","5-2.5\n1 FT",null,"10 units","BOX","EA",9.6439393939393945,3182.5]
[null,1011025,null,"XC blue frame, TSR Grey Fog-Ban lens","5-2.5\n1 FT",null,"10 units","BOX","EA",10.954545454545455,3615]
[null,1012879,null,"XC blue frame Cappucino Fog-Ban lens","5-2.5\n1 FT",null,"10 units","BOX","EA",10.954545454545455,3615]
[null,1012100,null,"XC blue frame Green 6-2.5 lens","6-2.5\n1 FTK",null,"10 units","BOX","EA",11.825757575757574,3902.4999999999995]
[null,1011022,null,"XC blue frame Silver mirror lens","5-3.1\n1 FT",null,"10 units","BOX","EA",11.363636363636363,3750]
[null,1012910,null,"XC blue frame Dark Grey TCG lens","5-3.1\n1 FT",null,"10 units","BOX","EA",9.6439393939393945,3182.5]
[null,1011024,null,"XC blue frame, HDL Yellow abrasion resistant lens","2-1.2\n1 FT",null,"10 units","BOX","EA",9.6439393939393945,3182.5]
[null,1012900,null,"XC blue frame, HDL Yellow Fog-Ban lens","2-1.2\n1 FT",null,"10 units","BOX","EA",10.954545454545455,3615]
[null,1011023,null,"XC blue frame, I/O Silver lens","5-1.7\n1 FT",null,"1 db","BOX","EA",11.363636363636363,3750]
[null,null,null,null,null,null,""]
[null,"Eye & Face Protection |  OVERSPECS, ACCESSORIES",null,null,null,null,""]
[null,1012877,null,"XC blue frame, IR 1.7 abrasion res. lens","1.7 \n1 FT",null,"10 units","BOX","EA",11.825757575757574,3902.4999999999995]
[null,1011021,null,"XC blue frame, IR 3 abrasion resistant lens","3.0\n1 FT",null,"10 units","BOX","EA",11.825757575757574,3902.4999999999995]
[null,1012901,null,"XC blue frame, IR 4 abrasion resistant lens","4.0\n1 FT",null,"10 units","BOX","EA",11.825757575757574,3902.4999999999995]
[null,1011020,null,"XC blue frame, IR 5 abrasion resistant lens","5.0\n1 FT",null,"1 db","BOX","EA",11.825757575757574,3902.4999999999995]
[null,1012902,null,"XC blue frame, IR 6 abrasion resistant lens","6.0\n1 FT",null,"10 units","BOX","EA",11.825757575757574,3902.4999999999995]
[null,"REPLACEMENT LENSES",null,null,null,null,""]
[null,1011013,null,"XC Clear abrasion resistant replacement lens",null,null,"10 units","BOX","EA",3.6439393939393936,1202.4999999999998]
[null,1011015,null,"XC Clear Fog-Ban replacement lens",null,null,"10 units","BOX","EA",4.9469696969696972,1632.5]
[null,1011017,null,"XC TSR Grey Fog-Ban replacement lens",null,null,"10 units","BOX","EA",6.5681818181818175,2167.4999999999995]
[null,1011018,null,"XC HDL Yellow abrasion res. replacement lens",null,null,"1 db","BOX","EA",5.2575757575757578,1735]
[null,1011019,null,"XC HDL I/O Silver abrasion res. replacement lens",null,null,"10 units","BOX","EA",6.9696969696969688,2299.9999999999995]
[null,1011010,null,"XC IR shade 3 abrasion resistant replacement lens",null,null,"10 units","BOX","EA",7.3712121212121211,2432.5]
[null,1010949,null,"XC IR shade 5 abrasion resistant replacement lens",null,null,"10 units","BOX","EA",7.3712121212121211,2432.5]
[null,1011410,null,"XC RX INSERT",null,null,"1 db","BOX","EA",18.189393939393941,6002.5000000000009]
[null,1015250,null,"XC R-L SHADE 1.7",null,null,"10 units","BOX","EA",6.8181818181818175,2249.9999999999995]
[null,"OVERSPEC",null,null,null,null,""]
[null,"Overspec provides over-the-glass coverage, offering workers full protection while wearing their own prescription spectacles"]
[null,"Medium frame size now available"]
[null,1028500,null,"Clear hard coating, Medium frame","2C-1.2\n1 F",null,"10 units","BOX","EA",6.2803030303030294,2072.4999999999995]
[null,1028501,null,"Clear Fog-Ban, Medium frame","2C-1.2\n1 F",null,"10 units","BOX","EA",6.378787878787878,2104.9999999999995]
[null,1028502,null,"TSR Grey, Medium frame","5-2.5\n1 F",null,"1 db","BOX","EA",6.462121212121211,2132.4999999999995]
[null,1027608,null,"Clear hard coating, Large frame","2C-1.2\n1 F",null,"10 units","BOX","EA",6.2803030303030294,2072.4999999999995]
[null,1027613,null,"Clear Fog-Ban, Large frame","2C-1.2\n1 F",null,"10 units","BOX","EA",6.378787878787878,2104.9999999999995]
[null,1027611,null,"TSR Grey, Large frame","5-2.5\n1 F",null,"10 units","BOX","EA",6.462121212121211,2132.4999999999995]
[null,1027610,null,"Amber lens, Large frame","2C-1.2\n1 F",null,"10 units","BOX","EA",6.462121212121211,2132.4999999999995]
[null,1027612,null,"I/O silver lens, Large frame","5-1.7\n1 F",null,"10 units","BOX","EA",7.2878787878787872,2404.9999999999995]
[null,"POLYSAFE",null,null,null,null,""]
[null,1002550,null,"POLYSAFE. Visitor spec. Fits over prescription glasses .General use and protection against impact (45m/s).Mechanic work: grinding, turning, milling","2C-1.2\n1 F",null,"10 units","BOX","EA",2.0303030303030303,670]
[null,1002549,null,"POLYSAFE PLUS CLEAR . Clear Frame (Polysafe Plus) Clear Lens, Anti-scratch Coating,",null,null,"10 units","BOX","EA",3.143939393939394,1037.5]
[null,1015744,null,"POLYSAFE. Black temples. Visitor spec. Fits over prescription glasses .",null,null,"200 units","CAS","EA",1.7727272727272725,584.99999999999989]
[]
[null,"Eye & Face Protection |  OVERSPECS, ACCESSORIES",null,null,null,null,""]
[null,"ARMAMAX",null,null,null,null,""]
[null,1002221,null,"AX1H Clear polycarbonate eyeshield","1 FK",null,"10 units","BOX","EA",6.416666666666667,2117.5]
[null,1002223,null,"AX4H green shade 1.7 polycarbonate eyeshield","1 FK",null,"10 units","BOX","EA",8.7424242424242422,2885]
[null,1002224,null,"AX Clear polycarbonate eyeshield","1 F",null,"10 units","BOX","EA",4.4924242424242422,1482.5]
[null,1002163,null,"Armamax 520 clip on square shape with flip up mechanism clear abresion resisatnt","1FK",null,"10 units","BOX","EA",10.060606060606059,3319.9999999999995]
[null,1002166,null,"Armamax 520 clip on square shape with flip up mechanism green IR1.7 abresion resisatnt","1FK",null,"10 units","BOX","EA",10.878787878787877,3589.9999999999995]
[null,"SPECTACLE CASES",null,null,null,null,""]
[null,1008060,null,"Soft spectacle case with zip fastener and belt clip, suits all styles inc. wrap-around spectacles",null,null,"10 units","BOX","EA",3.4318181818181817,1132.5]
[null,1013418,null,"Rigid spectacle case with zip fastener and belt clip, suits all styles inc. wrap-around spectacles",null,null,"1 db","BOX","EA",4.9999999999999991,1649.9999999999998]
[null,1008061,null,"SOFT PVC CASE.",null,null,"10 units","BOX","EA",1.9469696969696968,642.49999999999989]
[null,"SPECTACLE CORDS",null,null,null,null,""]
[null,1002436,null,"SC2 black spectacle cord retainer",null,null,"12 units","BOX","EA",1.1363636363636362,374.99999999999994]
[null,1005771,null,"Flexi-Cord spectacle retainer",null,null,"100 units","BOX","EA",0.83333333333333337,275]
[null,"LENS CLEANER",null,null,null,null,""]
[null,1011378,null,"Lens cleaning solution 500ml spray bottle, contains no alcohol or silicone",null,null,"1 unit","EA","EA",5.416666666666667,1787.5]
[null,1011379,null,"Lens cleaning tissues, 500 per box, non-abrasive",null,null,"500 tissues","BOX","BOX",4.0606060606060606,1340]
[null,1011380,null,"Box contains : Lens cleaning station, contains 500ml spray bottle of lens cleaning solution and 1500 tissues",null,null,"1 unit","BOX","BOX",18.18181818181818,5999.9999999999991]
[null,1011332,null,"Box contains: Lens cleaning towelettes, pre-moistened in pocket size sachets, Box contains 100 towlettes. ",null,null,"100  tissues","BOX","BOX",8.3333333333333321,2749.9999999999995]
[null,null,null,null,null,null,""]
[null,"Eye & Face Protection |  GOGGLES",null,null,null,null,""]
[null,"SUB-ZERO"]
[null,"Sub-Zero™ goggles provide superior protection in cold, extreme environments."]
[null,"Soft face foam for superior comfort and warmth. "]
[null,"HydroShield anti-fog coating reduces fogging, and provide anti-scratch performances to keep lenses clear and workers safe. "]
[null,1111001,null,"Honeywell Sub-Zero Goggle, Clear lens, HydroShield Clear HydroShield","2C-1.2 HON 1FT/BKN",null,"1 unit","BOX","EA",39.393939393939391,12999.999999999998]
[null,1111002,null,"Honeywell Sub-Zero Goggle, Grey lens, HydroShield Grey HydroShield 2C-3 / 5-3.1 HON 1 FT / BKN","2C-3 HON 1FT/BKN",null,"1 unit","BOX","EA",39.393939393939391,12999.999999999998]
[null,"DURAMAXX",null,null,null,null,""]
[null,"DuraMaxx™ goggle with Dura-streme™ coating technology"]
[null,"● Dura-streme™ delivers tough, anti-scratch coating on the outside, and anti-fog coating on the inside, for lenses that last "]
[null,"up to 3 times* longer"]
[null,"● Soft, elastomer body flexes and conforms to the face for a comfortable, gap-free fit"]
[null,"● Fits comfortably over most prescription spectacles"]
[null,"*Comparative lens life test performed using Bayer Abrasion Test method and may vary between environment and application"]
[]
[null,1017751,null,"DURAMAXX goggle with Clear lens and neoprene strap","2C-1.2\n1 BT 34 KN",null,"1 unit","","EA",11.772727272727272,3884.9999999999995]
[null,1017750,null,"DURAMAXX goggle with Clear lens and fabric strap","2C-1.2\n1 BT 34 KN",null,"1 unit","","EA",11.772727272727272,3884.9999999999995]
[null,1017737,null,"DURAMAXX goggle with TSR Grey lens and neoprene strap","5-2.5\n1 BT 34 KN",null,"1 unit","","EA",12.25,4042.5]
[null,1017738,null,"DURAMAXX goggle with TSR Grey lens and fabric strap","5-2.5\n1 BT 34 KN",null,"1 unit","","EA",12.25,4042.5]
[null,1017752,null,"DURAMAXX goggle with HDL Yellow lens and neoprene strap","2C-1.2\n1 BT 34 KN",null,"1 unit","","EA",12.25,4042.5]
[null,1017753,null,"DURAMAXX goggle with HDL Yellow lens and fabric strap","2C-1.2\n1 BT 34 KN",null,"1 unit","","EA",12.25,4042.5]
[null,1017739,null,"DURAMAXX goggle with Shade 5 Green lens and neoprene strap","5.0\n1 BT 34 KN",null,"1 unit","","EA",16.780303030303028,5537.4999999999991]
[null,1028135,null,"Replacement Clear lens",null,null,"1 unit","","EA",5.6515151515151514,1865]
[null,"Eye & Face Protection |  GOGGLES",null,null,null,null,""]
[]
[null,1028136,null,"Replacement TSR Grey lens",null,null,"1 unit","","EA",6.2272727272727275,2055]
[null,1028137,null,"Replacement HDL Yellow lens",null,null,"1 unit","","EA",6.2272727272727275,2055]
[null,1028140,null,"Replacement Shade 5 Green lens",null,null,"1 unit","","EA",7.5378787878787872,2487.4999999999995]
[null,null,null,null,null,null,""]
[null,"MAXX-PRO",null,null,null,null,""]
[null,"Low profile goggle compatible with welding helmets, faceshields and other protective equipment"]
[null,"New hydroshield lens"]
[null,"1011071HS",null,"MAXX-PRO GOGGLE CLEAR Hydroshield LENS NEOPRENE HB","2C-1.2 1FT 349 KN",null,"1 unit",null,"EA",10.15151515151515,3349.9999999999995]
[null,"1011072HS",null,"MAXX-PRO GOGGLE CLEAR Hydroshiled LENS FABRIC HB","2C-1.2 1FT 349 KN",null,"1 unit",null,"EA",9.8484848484848477,3249.9999999999995]
[null,"1011070HS",null,"MAXX-PRO GOGGLE CLEAR Hydroshield REPL LENS",null,null,"10 units",null,"EA",4.545454545454545,1499.9999999999998]
[null,1011071,null,"MAXX-PRO goggle with Clear Fog-Ban lens and neoprene headband","2C-1.2 \n1 FT 349 K",null,"1 unit","","EA",8.9848484848484844,2965]
[null,1011070,null,"MAXX-PRO GOGGLE CLEAR F-B REPL LNS",null,null,10,null,"EA",3.6969696969696968,1220]
[null,"FLEX-SEAL",null,null,null,null,""]
[null,"Ultimate comfort and performance - Soft silicone body for a perfect fit and exceptional comfort, combined with a large "]
[null,"wrap-around lens for excellent panoramic vision",null,null,null,null,""]
[null,1011381,null,"FLEXSEAL goggle with Clear Fog-Ban lens and neoprene strap","2C-1.2 \n1 BT 349",null,"1 unit","","EA",12.128787878787879,4002.5]
[null,1011333,null,"FLEXSEAL goggle with Clear Fog-Ban lens and fabric strap","2C-1.2\n1 BT 349",null,"1 unit","","EA",12.128787878787879,4002.5]
[null,1011384,null,"FLEXSEAL goggle with Shade 5 Green Fog-Ban lens and neoprene strap","5.0\n1 FT 349",null,"1 unit","","EA",16.871212121212121,5567.5]
[null,1011385,null,"Replacement Clear Fog-Ban lens",null,null,"10 units","BOX","EA",5.8106060606060606,1917.5]
[null,"V-MAXX",null,null,null,null,""]
[null,"Sport style goggle with distortion-free 100% peripheral vision",null,null,null,null,""]
[null,1006192,null,"V-MAXX goggle with indirect vent, polycarbonate lens and elastic strap","2C-1.2\n1 349 B",null,"1 db","BOX","EA",5.8636363636363633,1935]
[null,1006193,null,"V-MAXX goggle with indirect vent, polycarbonate non-mist lens and elastic strap","2C-1.2\n1 B 349",null,"10 units","BOX","EA",7.0227272727272725,2317.5]
[null,1006194,null,"V-MAXX goggle with indirect vent, polycarbonate non-mist lens and neoprene strap","2C-1.2\n1 B 349",null,"10 units","BOX","EA",8.1818181818181817,2700]
[null,1006195,null,"V-MAXX goggle with polycarbonate non-mist lens and elastic strap, no vent","2C-1.2\n1 B 3459",null,"10 units","BOX","EA",7.4242424242424248,2450]
[null,1006196,null,"V-MAXX goggle with polycarbonate non-mist lens, foam surround and elastic strap, no vent","2C-1.2\n1 B 3459",null,"10 units","BOX","EA",8.7424242424242422,2885]
[null,1007506,null,"V-MAXX goggle with indirect vent, acetate non-mist lens, neoprene strap and 2 protective lens covers","1 F 34",null,"10 units","BOX","EA",8.0833333333333321,2667.4999999999995]
[null,1008111,null,"V-MAXX welding goggle with black frame and green shade 5 lens","5.0\n1 F 349",null,"10 units","BOX","EA",11.613636363636363,3832.5]
[null,1006437,null,"Protective Lens Covers",null,null,"10 units","BOX","EA",1.9772727272727271,652.49999999999989]
[null,null,null,null,null,null,""]
[null,"VISTAMAX 2000",null,null,null,null,""]
[null,"Deep frame profile provides protection over most prescription eyewear",null,null,null,null,""]
[null,1002755,null,"VX2031 goggle with abrasion resistant, anti-mist polycarbonate lens and high flow vents","1 B 349",null,"10 units","BOX","EA",14.65151515151515,4835]
[null,1002757,null,"VX2131 goggle with indirect vents and abrasion resistant, anti-mist polycarbonate lens","1 B 349",null,"10 units","BOX","EA",16.166666666666664,5334.9999999999991]
[null,"VISTAMAX VNC",null,null,null,null,""]
[null,"Breathable 'twin-lens' system with aluminium condensers for exceptional anti-mist performance"]
[null,1002759,null,"VNC21 unvented goggle with dual lenses; Front lens is acetate for chemical resistance and rear lens is polycarbonate for impact resistance","1 B 345",null,"10 units","BOX","EA",9.3409090909090899,3082.4999999999995]
[null,1004066,null,"VNC21FC unvented goggle with dual lenses; Front lens is acetate for chemical resistance and rear lens is polycarbonate for impact resistance, foam comfort surround fitted","1 B 345",null,"10 units","BOX","EA",11.969696969696969,3949.9999999999995]
[null,"LG ",null,null,null,null,""]
[null,"Excellent value in a lightweight comfortable design",null,null,null,null,""]
[null,1005504,null,"LG10 goggle with direct vent and polycarbonate lens","1 B",null,"50 units","CAS","CAS",1.4206060606060604,468.79999999999995]
[null,1005507,null,"LG20 goggle with indirect vent and polycarbonate lens","1 B 3",null,"50 units","CAS","CAS",1.8939393939393938,625]
[null,1005509,null,"LG20 AF goggle with indirect vent and anti-mist polycarbonate lens","1 B 3",null,"50 units","CAS","CAS",2.6666666666666665,880]
[null,1008112,null,"LG20 Chemistry goggle with indirect vent and anti-mist acetate Lens","1 F 34",null,"50 units","CAS","CAS",3.4545454545454541,1139.9999999999998]
[null,"Eye & Face Protection |  NORTH",null,null,null,null,""]
[null,"Tactile T2400"]
[null,"Square shaped ultra lightweight PC lens - soft touch black temples & nose bridge - 'lollipop' packaging"]
[null,908730,null,"Clear - 3A",null,null,"12 units","BOX","EA",3.1818181818181817,1050]
[null,908731,null,"Blue Mirror Smoke - 3A",null,null,"12 units","BOX","EA",3.4090909090909087,1124.9999999999998]
[null,908736,null,"In / Outdoor - 3A",null,null,"12 units","BOX","EA",3.4090909090909087,1124.9999999999998]
[null,"N - Vision T5655"]
[null,"Beyond the Edge - full frame - extensible temples - regular curved and straight temple included - 2 size flexi-fit nose bridge included - PC lens- RX-Insert available"]
[]
[null,906600,null,"Black - Clear - 4A",null,null,"10 units","BOX","EA",7.7045454545454541,2542.5]
[null,906601,null,"Black - Smoke - 4A",null,null,"10 units","BOX","EA",8.5227272727272716,2812.4999999999995]
[null,906602,null,"Black - Amber - 4A",null,null,"10 units","BOX","EA",8.5227272727272716,2812.4999999999995]
[null,906606,null,"Black - In / Outdoor - 3A",null,null,"10 units","BOX","EA",8.5227272727272716,2812.4999999999995]
[null,"Accessories"]
[null,"For N-vision & Lightning series"]
[null,606790,null,"N-Vision Clear lens - 4A",null,null,"10 units","BOX","EA",4.3106060606060606,1422.5]
[null,606791,null,"N-Vision Smoke lens - 4A",null,null,"10 units","BAG","EA",4.7424242424242422,1565]
[null,606792,null,"N-Vision Amber lens - 4A",null,null,"10 units","","EA",4.7424242424242422,1565]
[null,"493HRL",null,"N-Vision I/O lens - 3A",null,null,"10 units","BOX","EA",4.7424242424242422,1565]
[null,"The EDGE T5600"]
[null,"Sporty glasses - full frame - extensible temples - regular curved temple and straight temple included - revolutionary replacement lens system - PC lens"]
[null,908300,null,"Grey - Clear - 4A",null,null,"10 units","BOX","EA",7.6060606060606046,2509.9999999999995]
[null,908304,null,"Grey - Amber - 4A",null,null,"10 units","BOX","EA",8.4015151515151505,2772.4999999999995]
[null,908310,null,"Blue - Clear - 4A",null,null,"10 units","BOX","EA",7.6060606060606046,2509.9999999999995]
[null,908311,null,"Blue - Smoke - 4A",null,null,"10 units","BOX","EA",8.4015151515151505,2772.4999999999995]
[null,908320,null,"Black - Clear - 4A",null,null,"10 units","BOX","EA",7.6060606060606046,2509.9999999999995]
[null,908321,null,"Black - Smoke - 4A",null,null,"10 units","BOX","EA",8.4015151515151505,2772.4999999999995]
[null,908324,null,"Black - Amber - 4A",null,null,"10 units","BOX","EA",8.4015151515151505,2772.4999999999995]
[null,"Amigo"]
[null,"Flip-up welding goggle - with welding lens"]
[null,805635,null,"Xanthos 5",null,null,"24 units","BOX","EA",9.5757575757575761,3160]
[null,"Clips-Ons"]
[null,"Flip-up clip for RX-frames"]
[null,204540,null,"Brown polarized",null,null,"1 unit","","EA",11.174242424242424,3687.5]
[null,204524,null,"Clear PC - 3A",null,null,"1 unit","","EA",5.4848484848484844,1809.9999999999998]
[null,"Eye & Face Protection |  NORTH",null,null,null,null,""]
[null,204525,null,"Green 3 PC - 3A",null,null,"1 unit","","EA",5.4848484848484844,1809.9999999999998]
[null,204527,null,"Green 5 PC - 3A",null,null,"1 unit","","EA",5.4848484848484844,1809.9999999999998]
[null,"Tube case"]
[null,"Soft shell tube lens protector - fits all styles"]
[null,204513,null,"Black",null,null,"1 unit","","EA",1.9848484848484849,655]
[null,"Perforama Nova"]
[null,"Clear crown - chin gard - 17 cm screen - ratchet adjustment headgear"]
[null,820140,null,"Clear PC - 3A",null,null,"16 units","BOX","EA",25.424242424242426,8390]
[null,"820144.6",null,"Clear CP - 4A",null,null,"16 units","BOX","EA",28.037878787878785,9252.5]
[null,520160,null,"Screen Clear PC - 3A",null,null,"5 units","BOX","EA",16.196969696969695,5344.9999999999991]
[null,520164,null,"Screen Clear CP - 4A",null,null,"5 units","BOX","EA",18.954545454545453,6255]
[null,"Eye & Face Protection |  FACESHIELDS",null,null,null,null,""]
[null,"NEW TURBOSHIELD",null,null,null,null,""]
[null,"Turboshield faceshield  integrates an array of features for ease of use and wearer comfort"]
[null,"● Patented, secure visor attachment system for quick, easy visor replacement"]
[null,"● Toric lens (curved on two planes) provides excellent optics, increased field of view and chin coverage without attachments"]
[null,"● Ergonomic, easy-to-use adjustment\nknobs – even when wearing gloves"]
[null,"● Patent-pending suspension with comfort-designed headgear features dual material technology for cushioned comfort"]
[null,"● Smooth-pivoting action with positive stops secures visor in raised and lowered positions"]
[null,"TURBOSHIELD HEADGEAR AND HELMET ATTACHMENT"]
[null,1031740,null,"Turboshield Ratcheted Headgear, Black","166 3 9 BT",null,"1 unit","","EA",17.939393939393938,5919.9999999999991]
[null,1031749,null,"Turboshield Hard Hat Adapter, Black\nTested and approved for use on these hard hats: North A59, A69, A79, A89; MSA V-Gard; Centurion Concept Full Peak, 1100; Schuberth Baumeister 80, Euroguard 4; Peltor G2000; JSP MK2","166 3 9 BT",null,"1 unit","","EA",17.977272727272727,5932.5]
[null,"TURBOSHIELD VISORS",null,null,null,null,""]
[null,1031743,null,"Clear Polycarbonate Visor, uncoated","2C-1.2\n1 BT 9",null,"1 unit","","EA",8.5303030303030294,2814.9999999999995]
[null,1031744,null,"Clear Polycarbonate Visor, hard-coat and anti-fog","2C-1.2\n1 BT 9KN",null,"1 unit","","EA",20.696969696969695,6829.9999999999991]
[null,1031745,null,"Grey Polycarbonate Visor, uncoated","2C-2.5\n5-2.5\n1 BT 9",null,"1 unit","","EA",9.6969696969696972,3200]
[null,1031746,null,"Grey Polycarbonate Visor, hard-coat and anti-fog","2C-2.5\n5-2.5\n1 BT 9KN",null,"1 unit","","EA",21.651515151515149,7144.9999999999991]
[null,1031747,null,"IR Shade 3 Visor, uncoated","3\n1 BT 9",null,"1 unit","","EA",20.068181818181817,6622.4999999999991]
[null,1031748,null,"IR Shade 5 Visor, uncoated","5\n1 BT 9",null,"1 unit","","EA",22.992424242424242,7587.5]
[null,null,null,null,null,null,""]
[null,"BIONIC",null,null,null,null,""]
[null,"Extremely adjustable fit, position and tilt control plus extended top of head and chin protection"]
[null,"Now available with High Energy Impact visor EN166-A"]
[null,1011933,null,"BIONIC complete with Clear acetate visor","1 FT 3",null,"1 unit","","EA",30.303030303030301,10000]
[null,1011624,null,"BIONIC complete with Clear polycarbonate Fog-Ban anti-scratch visor","2C-1.2 \n1 BT 39",null,"1 unit","","EA",38.43181818181818,12682.5]
[null,1011623,null,"BIONIC complete with Clear polycarbonate uncoated visor","2C-1.2 \n1 BT 39",null,"1 unit","","EA",27.022727272727273,8917.5]
[null,"BIONIC SHELL WITH HEADBAND (NO VISOR)",null,null,null,null,""]
[null,1015113,null,"BIONIC frame and headband without visor",null,null,"1 unit","","EA",22.984848484848484,7585]
[null,"REPLACEMENT VISORS",null,null,null,null,""]
[null,1011626,null,"Clear acetate visor","1 FT 3",null,"1 unit","","EA",7.3257575757575752,2417.5]
[null,1011627,null,"Clear Fog-Ban anti-scratch polycarbonate visor","2C-1.2\n1 BT 39",null,"1 unit","","EA",16.772727272727273,5535]
[null,1011625,null,"Clear uncoated polycarbonate visor","2C-1.2\n1 BT 39",null,"1 unit","","EA",6.5151515151515147,2150]
[null,1011628,null,"Shade 3 polycarbonate visor","3\n1 BT 39",null,"1 unit","","EA",18.386363636363637,6067.5]
[null,1011629,null,"Shade 5 polycarbonate visor","5\n1 BT 39",null,"1 unit","","EA",20.212121212121211,6670]
[null,1015112,null,"Clear polycarbonate electric arc visor approved to EN166-A for high energy impact","2C-1.2\n1 A 389",null,"10 units","BOX","EA",9.6439393939393945,3182.5]
[null,"ACCESSORIES",null,null,null,null,""]
[null,1015240,null,"Protective visor covers",null,null,"10 units","BOX","EA",10.106060606060606,3335]
[null,1011934,null,"Sweatband",null,null,"1 unit","","EA",2.0303030303030303,670]
[null,1015161,null,"Helmet adapter",null,null,"1 unit","","EA",11.037878787878787,3642.4999999999995]
[null,"CLEARWAYS",null,null,null,null,""]
[null,"BROWGUARDS",null,null,null,null,""]
[null,1002341,null,"CB20 browguard with ratchet headband","B 3",null,"10 units","BOX","EA",10.454545454545455,3450]
[null,1002346,null,"CB14 browguard with elasticated headband","B 3 ",null,"10 units","BOX","EA",7.2196969696969688,2382.4999999999995]
[null,"VISORS",null,null,null,null,""]
[null,1002360,null,"CV84A  200mm clear acetate visor","1 F 3",null,"10 units","BOX","EA",5.9621212121212119,1967.5]
[null,1002354,null,"CV84A/CG  200mm clear acetate visor for use with CG7 chinguard","1 F 3",null,"10 units","BOX","EA",6.8712121212121211,2267.5]
[null,1002353,null,"CV83P  200mm clear polycarbonate visor","1 B 3",null,"10 units","BOX","EA",5.3030303030303028,1750]
[null,1002359,null,"CV83P/CG  200mm clear polycarbonate visor for use with CG7 chinguard","1 B 3",null,"10 units","BOX","EA",6.0151515151515156,1985.0000000000002]
[null,1002365,null,"CV84AG  200mm green acetate shade 1.7 visor","1 F 3",null,"10 units","BOX","EA",6.7803030303030294,2237.4999999999995]
[null,1002369,null,"CV85/3W  200mm green acetate shade 3 visor","3.0\n1 F 3",null,"10 units","BOX","EA",13.583333333333332,4482.5]
[null,1002370,null,"CV85/5W  200mm green acetate shade 5 visor","5.0\n1 F 3",null,"10 units","BOX","EA",14.901515151515152,4917.5]
[null,1002294,null,"CG7 chinguard for use with 1002354, 1002359",null,null,"10 units","BOX","EA",6.1060606060606064,2015.0000000000002]
[null,1002366,null,"Clearways Visor CV84AN",null,null,"10 units","BOX","EA",9.4015151515151505,3102.4999999999995]
[null,"FACE SCREENS FOR ELECTRICAL WORK"]
[null,"Protection against hazards related to electric arc short -circuits and mechanical and chemical hazards. "]
[null,3697094,null,"ELECTRICAL FACESHIELDS CLEAR SCHUBERT. Clear acetate fogban screen (Height 24 mm)","3.1,2D.1.B.8.N",null,"10 units","BOX","EA",27.871212121212118,9197.4999999999982]
[null,"Eye & Face Protection |  FACESHIELDS",null,null,null,null,""]
[null,3697095,null,"ELECTRICAL FACESHIELDS CLEAR PROTECTOR. Clear acetate fogban screen (Height 24 mm)\n","3.1,2D.1.B.8.N",null,"10 units","BOX","EA",27.871212121212118,9197.4999999999982]
[null,3697080,null,"ELECTR FACESHIELDS CLEAR POLY PROTECTOR. Clear polycarbonate screen (height 24mm)\n","3.1,2.D.1.B.8",null,"10 units","BOX","EA",24.462121212121211,8072.5]
[null,"SUPERVIZOR HEAVY DUTY FACE PROTECTION",null,null,null,null,""]
[null,"BROWGUARD AND HELMET ATTACHMENTS (HELMET NOT INCLUDED)",null,null,null,null,""]
[null,1002297,null,"SB600 browguard with ratchet headband","B 39",null,"10 units","BOX","EA",16.227272727272727,5355]
[null,1002302,null,"SA660 plastic safety helmet attachment","B 39",null,"10 units","BOX","EA",11.825757575757574,3902.4999999999995]
[null,1002305,null,"SA66 metal safety helmet attachment","B 39",null,"1 db","BOX","EA",17.121212121212121,5650]
[null,1002304,null,"SA66M molten metal safety helmet attachment","B 39",null,"10 units","BOX","EA",20.053030303030301,6617.4999999999991]
[null,"POLYCARBONATE VISORS",null,null,null,null,""]
[null,1002312,null,"SV9PC 230mm clear polycarbonate visor","1 B 39",null,"10 units","BOX","EA",8.2424242424242422,2720]
[null,1002310,null,"SV9PC/CG clear polycarbonate visor for use with VS7 chinguard","1 B 39",null,"10 units","BOX","EA",8.9469696969696972,2952.5]
[null,1002316,null,"SV9PCH 230mm clear abrasion resistant polycarbonate visor","1 B 39",null,"10 units","BOX","EA",24.143939393939394,7967.5]
[null,1002328,null,"SV9PG  230mm green shade 1.7 polycarbonate visor, EN170","3-1.7\n1 B 39",null,"10 units","BOX","EA",13.734848484848483,4532.4999999999991]
[null,1002325,null,"SV9PGFH  230mm gold coated abrasion resistant polycarbonate visor, EN170, EN171","4-5,",null,"1 unit","","EA",133.36363636363635,44009.999999999993]
[null,"ACETATE VISORS",null,null,null,null,""]
[null,1002307,null,"SV9AC 200mm clear acetate visor","1 F 3",null,"10 units","BOX","EA",9.0378787878787872,2982.4999999999995]
[null,1002309,null,"SV9AC/CG clear acetate visor for use with VS7 chinguard","1 F 3",null,"10 units","BOX","EA",10.303030303030303,3400]
[null,1002329,null,"SV9A3W  200mm green shade 3 acetate visor","3.0\n1 F 3",null,"10 units","BOX","EA",26.27272727272727,8669.9999999999982]
[null,1002330,null,"SV9A5W  200mm green shade 5 acetate visor","5.0\n1 F 3",null,"10 units","BOX","EA",28.287878787878789,9335]
[null,1002308,null,"SV9EK clear acetate visor for electrical hazards","3-1.2\n1 F 38",null,"1 db","BOX","EA",13.083333333333332,4317.5]
[null,"TRI-ACETATE VISORS",null,null,null,null,""]
[null,1002318,null,"SV9TC 200mm clear tri-acetate visor","1 F 39",null,"10 units","BOX","EA",22.477272727272727,7417.5]
[null,1002321,null,"SV9TC3WP  200mm part shaded green / clear shade 3 tri-acetate visor","BS2092-2CM",null,"10 units","BOX","EA",40.409090909090907,13335]
[null,1002323,null,"SV9TC5WP  200mm part shaded green / clear shade 5 tri-acetate visor","BS2092-2CM",null,"10 units","BOX","EA",40.409090909090907,13335]
[null,"METAL MESH VISOR",null,null,null,null,""]
[null,1002337,null,"SAM9 metal wire mesh visor (suits SA66M helmet attachment only) for molten metal protection and forestry work","F",null,"10 units","BOX","EA",14.242424242424242,4700]
[null,"CHINGUARD",null,null,null,null,""]
[null,1002295,null,"VS7  Chinguard for use with 1002310, 1002309",null,null,"10 units","BOX","EA",5.4393939393939386,1794.9999999999998]
[null,"SUPERVIZOR HELMET / EARMUFF SYSTEM ",null,null,null,null,""]
[null,"Combined helmet mounted hearing and face protection (helmet earmuffs and adapters are also required)"]
[null,"HELMET ATTACHMENT",null,null,null,null,""]
[null,1004583,null,"SHA66M helmet mounted visor carrier","B 39",null,"10 units","BOX","EA",19.492424242424242,6432.5]
[null,"VISORS",null,null,null,null,""]
[null,1004584,null,"SHV9PC 200mm clear polycarbonate visor","1 B 39",null,"10 units","BOX","EA",9.9469696969696972,3282.5]
[null,1004587,null,"SHV9AC 200mm clear acetate visor","1 F 3",null,"10 units","BOX","EA",9.7499999999999982,3217.4999999999995]
[null,"VULCAN FIBRE WELDING HELMETS & HEAD SHIELDS"]
[null,"Prota Shell Baby"]
[null,"Small size helmet - full adjustable head gear - fixed and flip up glass holder"]
[null,810310,null,"Fixed 50x108 - no lens",null,null,"14 units","BOX","EA",25.007575757575754,8252.4999999999982]
[null,810314,null,"Fixed 50x108 - lens 10",null,null,"14 units","BOX","EA",26.378787878787879,8705]
[null,810300,null,"Flip up 50x108 - no lens",null,null,"14 units","BOX","EA",31.674242424242426,10452.5]
[null,810304,null,"Flip up 50x108 - lens 10",null,null,"14 units","BOX","EA",32.992424242424242,10887.5]
[null,810320,null,"Fixed 3 1/4 x 4 1/4 - no lens",null,null,"14 units","BOX","EA",25.772727272727273,8505]
[null,810330,null,"Fixed 85 x 110 - no lens",null,null,"14 units","BOX","EA",27.810606060606059,9177.5]
[null,810340,null,"Fixed 90 x 110 - no lens",null,null,"1 unit","","EA",25.772727272727273,8505]
[null,810344,null,"Fixed 90 x 110 - lens 10",null,null,"1 unit","","EA",27.810606060606059,9177.5]
[null,810394,null,"Flip up 50 x 108 chinflap - 10",null,null,"14 units","BOX","EA",54.537878787878782,17997.499999999996]
[]
[null,"Eye & Face Protection |  WELDING",null,null,null,null,""]
[null,"Spare parts Prota Shell (Baby)"]
[null,"Curved glass holders with springs - without o with clamps - no lenses supplied"]
[null,514032,null,"Flip up 50x108",null,null,"10 units","BOX","EA",9.9318181818181817,3277.5]
[null,514120,null,"Clamps 50x108",null,null,"10 units","BOX","PR",1.0454545454545454,345]
[null,"Shellfo"]
[null,"Light weight and comfortable - hand shield - fixed lens"]
[null,812210,null,"50x108 no lens",null,null,"15 units","BOX","EA",18.060606060606059,5959.9999999999991]
[null,812214,null,"50x108 lens",null,null,"15 units","BOX","EA",19.106060606060606,6305]
[null,812224,null,"3 1/4 x 4 1/4  lens 10",null,null,"15 units","","EA",20.742424242424242,6845]
[null,812244,null,"90x110  lens",null,null,"15 units","BOX","EA",20.742424242424242,6845]
[null,812250,null,"100x120 no lens",null,null,"15 units","BOX","EA",20.742424242424242,6845]
[null,812254,null,"100x120 lens",null,null,"15 units","BOX","EA",21.833333333333332,7205]
[null,"Spare parts Shekllfo"]
[null,"Fixed glass holders - no lenses supplied - handles"]
[null,515500,null,"100x120",null,null,"10 units","BOX","EA",4.6136363636363633,1522.5]
[null,512275,null,"110x120 handle",null,null,"10 units","","EA",3.75,1237.5]
[null,"Prota Shell"]
[null,"Full size helmet - full adjustable head gear - fixed and flip up glass holder"]
[null,810910,null,"Fixed 50x108 - no lens",null,null,"12 units","BOX","EA",26.378787878787879,8705]
[null,810914,null,"Fixed 50x108 - lens 10",null,null,"12 units","BOX","EA",27.537878787878789,9087.5]
[null,810920,null,"Fixed 3 1/4 x 4 1/4 - no lens",null,null,"12 units","BOX","EA",26.924242424242422,8885]
[null,810930,null,"Fixed 85 x 110 - no lens",null,null,"12 units","BOX","EA",28.954545454545453,9555]
[null,810940,null,"Fixed 90 x 110 - no lens",null,null,"12 units","BOX","EA",26.924242424242422,8885]
[null,810944,null,"Fixed 90 x 110 - lens 10",null,null,"12 units","BOX","EA",28.909090909090907,9540]
[null,810900,null,"Flip up 50x108 - no lens",null,null,"12 units","BOX","EA",33.030303030303031,10900]
[null,810904,null,"Flip up 50x108 - lens 10",null,null,"12 units","BOX","EA",34.378787878787882,11345.000000000002]
[null,810994,null,"Flip up 50 x 108 chinflap - lens 10",null,null,"12 units","BOX","EA",50.977272727272727,16822.5]
[null,"THERMO PLASTIC WELDING HELMETS & HAND SHIELDS"]
[null,"Lamador"]
[null,"Small size helmet - full adjustable head gear - flip-up glass holder"]
[null,810504,null,"50x108 lens 10",null,null,"14 units","BOX","EA",21.121212121212121,6970]
[null,810520,null,"60x110 no lens",null,null,"14 units","","EA",30.113636363636363,9937.5]
[null,810550,null,"85x110 no lens",null,null,"14 units","","EA",21.795454545454543,7192.4999999999991]
[null,"Gamador"]
[null,"Full size helmet - full adjustable head gear - fl8ip up glass holder"]
[null,810400,null,"50x108 no lens",null,null,"12 units","BOX","EA",21.121212121212121,6970]
[null,810440,null,"85x110 no lens",null,null,"12 units","BOX","EA",22.765151515151516,7512.5]
[null,810450,null,"90x110 no lens",null,null,"12 units","BOX","EA",22.765151515151516,7512.5]
[]
[null,"Eye & Face Protection |  WELDING",null,null,null,null,""]
[null,"Spare Parts Lamador / Gamador"]
[null,"Glass holders - glass retaining springs"]
[null,510490,null,"Glassholder 50x108",null,null,"10 units","BOX","EA",6.8863636363636358,2272.5]
[null,510495,null,"Glassholder 90x110",null,null,"10 units","BOX","EA",6.8863636363636358,2272.5]
[null,214112,null,"Spring 50x108",null,null,"1 unit","","EA",0.89393939393939381,294.99999999999994]
[null,"Shelfo Nova"]
[null,"Hand shield - lightweight - green"]
[null,812810,null,"50x108 no lens",null,null,"1 unit","","EA",11.893939393939393,3924.9999999999995]
[null,812814,null,"50x108 lens",null,null,"10 units","","EA",13.128787878787877,4332.4999999999991]
[null,"Popweld Nova"]
[null,"Hand shield - fixed glass holder"]
[null,812614,null,"50x108 lens 10",null,null,"15 units","BOX","EA",9.6060606060606055,3170]
[null,"FIBRE METAL THERMO PLASTIC WELDING HELMETS"]
[null,"Tigerhood Futura 2006"]
[null,"Streamlined shape - high performance material - extremely lightweight - 3C head gear - lift front- black - glass lens"]
[null,812932,null,"50x108 lens 10",null,null,"1 unit","","EA",34.234848484848484,11297.5]
[null,"Tigerhood 2999"]
[null,"Streamlined shape - high performance material - extreme - fixed front - black"]
[null,812930,null,"90x110 lens 10",null,null,"1 unit","","EA",34.492424242424242,11382.5]
[null,"Spare parts"]
[null,"For tiguerhood 2006 - Tigerhood 2999 - Pipeliner"]
[null,"3C",null,"3C headgear",null,null,"6 units","BOX","EA",9.6515151515151505,3184.9999999999995]
[null,"FM633171",null,"Speedy Loop headgear",null,null,"96 units","CAS","EA",9.4469696969696972,3117.5]
[null,"WELDING IN COMBINATION WITH NORTH HARD HATS"]
[null,"Gamador Combi North"]
[null,"Black carrier CP5005 - supplied without hard hat and lenses"]
[null,"810400.2",null,"50x108",null,null,"8 units","","EA",22.106060606060606,7295]
[null,"Lamador Combi North"]
[null,"Black carrier CP85005 - supplied without hard had and lenses"]
[null,"810550.2",null,"90x110",null,null,"8 units","BOX","EA",22.818181818181817,7529.9999999999991]
[null,"ACCESSORIES"]
[null,"Headgear North"]
[null,"For welding helmets - \"stop attachment\""]
[null,513556,null,"Headgear",null,null,"10 units","BOX","EA",8.1212121212121211,2680]
[null,613506,null,"Nomaz sweatband",null,null,"10 units","","BOX",9.5530303030303028,3152.5]
[null,"Spare parts"]
[null,"Glass retaining springs"]
[null,514110,null,"Spring 50x108",null,null,"10 units","BOX","EA",0.86363636363636354,284.99999999999994]
[null,"LEATHER WELDING MASKS WITHOUT LENSES"]
[null,"Mask"]
[null,"2 sizes"]
[null,813000,null,"30 cm",null,null,"1 unit","","EA",44.93181818181818,14827.5]
[null,813010,null,"45 cm",null,null,"5 units","BOX","EA",49.962121212121211,16487.5]
[null,"Mask 1"]
[null,"2 sizes with extra side flaps"]
[null,813001,null,"30 cm",null,null,"1 unit","","EA",51.446969696969695,16977.5]
[null,813011,null,"45 cm",null,null,"1 unit","","EA",56.446969696969695,18627.5]
[null,"Mask 2"]
[null,"2 sizes with leather cap"]
[null,813002,null,"30 cm",null,null,"5 units","BOX","EA",64.901515151515156,21417.5]
[null,813012,null,"45 cm",null,null,"5 units","BOX","EA",69.886363636363626,23062.499999999996]
[null,"Mask 3"]
[null,"2 sizes with cap and extra side flaps"]
[null,813003,null,"30 cm",null,null,"1 unit","","EA",76.931818181818173,25387.499999999996]
[null,813013,null,"45 cm",null,null,"5 units","BOX","EA",81.931818181818187,27037.5]
[null,"FIBRE METAL WELDING HELMETS WITH ADF LENSES"]
[null,"Tigerhood 2006"]
[null,"Streamlined shape - high performance material - extremely lightweight - 3C headgear - lift front - black - 50x108"]
[null,812924,null,"DIN 3-10",null,null,"1 unit","","EA",132.75,43807.5]
[null,812928,null,"DIN 3-11",null,null,"1 unit","","EA",132.75,43807.5]
[]
[null,"Tigerhood 2999"]
[null,"Streamlined shape - high performance material - extreme - lift front - black - 90x110"]
[null,812922,null,"DIN3-10",null,null,"1 unit","","EA",153.2348484848485,50567.500000000007]
[null,812926,null,"DIN 3-11",null,null,"1 unit","","EA",153.2348484848485,50567.500000000007]
[null,812920,null,"DIN 4/9 -13",null,null,"1 unit","","EA",213.81060606060606,70557.5]
[null,"ADF Lenses"]
[null,"For North Fibre Metal Tigerhood & FMX welding helmets"]
[null,212920,null,"90x110 DIN4/9 13",null,null,"1 unit","","EA",173.68181818181816,57314.999999999993]
[null,212921,null,"90X110 DIN 6 13 ADC",null,null,"1 unit","","EA",322.22727272727269,106334.99999999999]
[null,"Master Edition ADC Plus"]
[null,"New lightweight welding helmet - ADF lens with unique delay system - switch for grinding facility - multi shade selection - 3C head gear - including Slimline safety Spectacle - "]
[null,812921,null,"DIN 6-8/9 - 13",null,null,"1 unit","","EA",355.45454545454544,117300]
[null,"WELDING & COVER LENSES"]
[null,"Lenses 50"]
[null,"Mineral lenses - colour green - 50mm"]
[null,618804,null,"Xanthos 50mm Nº 4",null,null,"50 units","","EA",0.53030303030303028,175]
[null,618805,null,"Xanthos 50mm Nº 5",null,null,"50 units","","EA",0.53030303030303028,175]
[null,618806,null,"Xanthos 50mm Nº 6",null,null,"50 units","","EA",0.53030303030303028,175]
[null,618809,null,"Xanthos 50mm Nº 9",null,null,"50 units","","EA",0.53030303030303028,175]
[null,618810,null,"Xanthos 50mm Nº 10",null,null,"50 units","","EA",0.53030303030303028,175]
[null,618811,null,"Xanthos 50mm Nº 11",null,null,"50 units","","EA",0.53030303030303028,175]
[null,618812,null,"Xanthos 50mm Nº 12",null,null,"50 units","","EA",0.53030303030303028,175]
[null,618813,null,"Xanthos 50mm Nº 13",null,null,"50 units","","EA",0.53030303030303028,175]
[null,"Lenses 50 x 108"]
[null,"Mineral lenses - colour green - 50x108"]
[null,619004,null,"Xanthos 2x4 1/4 nº 4",null,null,"100 units","","EA",0.52272727272727271,172.5]
[null,619005,null,"Xanthos 2x4 1/4 nº 5",null,null,"100 units","CAS","EA",0.52272727272727271,172.5]
[null,619006,null,"Xanthos 2x4 1/4 nº 6",null,null,"10 units","BOX","EA",0.52272727272727271,172.5]
[null,619008,null,"Xanthos 2x4 1/4 nº 8",null,null,"100 units","","EA",0.52272727272727271,172.5]
[null,619009,null,"Xanthos 2x4 1/4 nº 9",null,null,"100 units","","EA",0.52272727272727271,172.5]
[null,619010,null,"Xanthos 2x4 1/4 nº 10",null,null,"100 units","","EA",0.52272727272727271,172.5]
[null,619011,null,"Xanthos 2x4 1/4 nº 11",null,null,"100 units","","EA",0.52272727272727271,172.5]
[null,619012,null,"Xanthos 2x4 1/4 nº 12",null,null,"100 units","","EA",0.52272727272727271,172.5]
[null,619013,null,"Xanthos 2x4 1/4 nº 13",null,null,"100 units","","EA",0.52272727272727271,172.5]
[null,"Lenses  90 x 110"]
[null,"Mineral lenses - colour green - 90x110"]
[null,619307,null,"Xanthos 90x110 nº 7",null,null,"100 units","BOX","EA",0.97727272727272729,322.5]
[null,619308,null,"Xanthos 90x110 nº 8",null,null,"100 units","BOX","EA",0.97727272727272729,322.5]
[null,619309,null,"Xanthos 90x110 nº 9",null,null,"100 units","BOX","EA",0.97727272727272729,322.5]
[null,619310,null,"Xanthos 90x110 nº 10",null,null,"100 units","BOX","EA",0.97727272727272729,322.5]
[null,619311,null,"Xanthos 90x110 nº 11",null,null,"100 units","BOX","EA",0.97727272727272729,322.5]
[null,619312,null,"Xanthos 90x110 nº 12",null,null,"100 units","BOX","EA",0.97727272727272729,322.5]
[null,619313,null,"Xanthos 90x110 nº 13",null,null,"100 units","BOX","EA",0.97727272727272729,322.5]
[null,"Eye & Face Protection |  WELDING",null,null,null,null,""]
[null,619409,null,"Xanthos 100x120 Nº 9",null,null,"100 units","BOX","EA",1.106060606060606,364.99999999999994]
[null,619410,null,"Xanthos 100x120 Nº 10",null,null,"100 units","BOX","EA",1.106060606060606,364.99999999999994]
[null,619411,null,"Xanthos 100x120 Nº 11",null,null,"100 units","BOX","EA",1.106060606060606,364.99999999999994]
[null,619412,null,"Xanthos 100x120 Nº 12",null,null,"100 units","BOX","EA",1.106060606060606,364.99999999999994]
[null,"Gold Coated 50 x108"]
[null,"Mineral lenses - fixed shades - 50x108"]
[null,618710,null,"2x4 1/4 Nº 10",null,null,"10 units","BOX","EA",2.3636363636363638,780]
[null,618711,null,"2x4 1/4 Nº 11",null,null,"10 units","BOX","EA",2.3636363636363638,780]
[null,618712,null,"2x4 1/4 Nº 12",null,null,"10 units","BOX","EA",2.3636363636363638,780]
[null,"Cover Lenses Mineral"]
[null,"Mineral lenses - Clear"]
[null,618100,null,"50 1,8 mm glass",null,null,"50 units","","EA",0.17424242424242425,57.500000000000007]
[null,618110,null,"50x108",null,null,"100 units","","EA",7.575757575757576E-2,25]
[null,618140,null,"90x110",null,null,"100 units","","EA",0.15151515151515152,50]
[null,618150,null,"100x120",null,null,"100 units","","EA",0.17424242424242425,57.500000000000007]
[null,"Cover Lenses Vinylite"]
[null,"CP - Plastic lenses - clear"]
[null,517800,null,50,null,null,"50 units","BOX","EA",0.26515151515151514,87.5]
[null,517810,null,"50x108",null,null,"50 units","BOX","EA",0.45454545454545453,150]
[null,517840,null,"Cover lens",null,null,"50 units","BOX","EA",0.68181818181818177,224.99999999999997]
[null,517850,null,"100x120",null,null,"50 units","BOX","EA",0.90909090909090906,300]
[null,"Chipping Lenses Focar"]
[null,"PC - plastic lenses - clear"]
[null,517500,null,50,null,null,"50 units","BOX","EA",0.66666666666666663,220]
[null,517510,null,"50x108",null,null,"250 units","BOX","EA",0.90909090909090906,300]
[null,517540,null,"Inner lens",null,null,"100 units","BOX","EA",1.4772727272727271,487.49999999999994]

{"sheet":"Head Protection","index":3,"n_rows":88,"n_cols":11,"rows_kept":88,"cut":false,"hidden":false,"merged":[]}
[null,"Head Protection | Hard Hats PEAK RANGE "]
[null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per","NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,"NEW!! PEAK RANGE"]
[null,null,"NEW - OUTER SHELL IN ABS MATERIAL "]
[null,"·          Tough, hard and rigid material with good chemical resistance, very high strength to impacts and excellent performance in high and low temperatures (+50°C to -30°C)."]
[null,null,"PERSONALISING HARD HATS "]
[null,"·          High definition pad printing gives the hard hat a professional customised look. Highly durable ink to print the logo on certain parts of the shell."]
[null,null,"AVAILABLE WITH TWO ADJUSTEMENT SYSTEMS "]
[null,"·  Pin-lock: easy to adjust system of interlocking teeth for a firm hold. Simply squeeze the buckle tabs to loosen the band and slide to tighten. "]
[null,"·          Ratchet: features an extra secure and comfortable grip that allows the wearer to place in any position without slipping. Simply twist the ratchet to adjust."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"A79"]
[null,"4-point nylon suspension - HDPE shell - replacement suspension 633160"]
[null,933160,null,"White",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,933161,null,"Yellow",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,933162,null,"Red",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,933163,null,"Green",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,"933164.1",null,"Blue",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,"933164.2",null,"Sky Blue",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,933165,null,"Orange",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,933166,null,"Grey",null,null,"20 units","BOX","EA",7.916666666666667,2612.5]
[null,"A69"]
[null,"6-point nylon suspension - HDPE shell - replacement suspension 633170"]
[null,933170,null,"White",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,933171,null,"Yellow",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,933172,null,"Red",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,933173,null,"Green",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,"933174.1",null,"Blue",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,"933174.2",null,"Sky Blue",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,933175,null,"Orange",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,933176,null,"Grey",null,null,"20 units","BOX","EA",8.75,2887.5]
[null,"SMOOTH LOCK RATCHET SYSTEM PEAK SERIES"]
[null,"A79R"]
[null,"4-point nylon suspension - HDPE shell - replacement suspension 633192"]
[null,933190,null,"White",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,933191,null,"Yellow",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,933192,null,"Red",null,null,"20 units",null,"EA",9.65,3184.5]
[null,933193,null,"Green",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,"933194.1",null,"Blue",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,"933194.2",null,"Sky Blue",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,933195,null,"Orange",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,933196,null,"grey",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,933197,null,"pink",null,null,"20 units","BOX","EA",9.65,3184.5]
[null,"A69R"]
[null,"6-point nylon suspension - HDPE shell - replacement suspension 633180"]
[null,933180,null,"White",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[null,933181,null,"Yellow",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[null,933182,null,"Red",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[null,933183,null,"Green",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[null,"933184.1",null,"Blue",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[null,"933184.2",null,"Sky Blue",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[null,933185,null,"Orange",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[null,933186,null,"Grey",null,null,"20 units","BOX","EA",11.366666666666667,3751]
[]
[]
[null,"Head Protection | Accessories "]
[null,"Easy replacement - for Peak and K2 series"]
[null,633105,null,"Chainstrap protection",null,null,null,null,null,6.05,1996.5]
[null,633103,null,"A79C100 CHINSTRAP 2PTS WHITE",null,null,null,null,null,3.4833333333333329,1149.4999999999998]
[null,"633130.1",null,"GC2000 GOGGLE CLIP/HATS",null,null,null,null,null,3.8500000000000005,1270.5000000000002]
[null,633150,null,"Plastic 4 - point",null,null,"10 units","","EA",2.2749999999999999,750.75]
[null,633160,null,"Terylene 4 - point",null,null,"10 units","","EA",2.5833333333333335,852.5]
[null,633170,null,"Terylene 6 - point",null,null,"10 units","BOX","EA",3.4583333333333335,1141.25]
[null,633180,null,"Terylene 6 - point ratchet",null,null,"10 units","BOX","EA",7.65,2524.5]
[null,633192,null,"Terylene 4 - point ratchet",null,null,"1 unit","","EA",6.866666666666668,2266.0000000000005]
[null,"ACCESSORIES"]
[null,"For hard hats - fit all hard hats - 3 pieces"]
[null,"633130.1",null,"Black - 3pcs",null,null,"10 units","","SET",3.8500000000000005,1270.5000000000002]
[null,"Sweatband"]
[null,"Fits Peak and K2 hard hats"]
[null,633122,null,"Nomaz",null,null,"10 units","BOX","EA",1.5833333333333333,522.5]
[null,633123,null,"Terry cloth with velcro",null,null,"1 unit","","BAG",1.4750000000000001,486.75000000000006]
[null,"WINTER LINERS"]
[null,"WL12"]
[null,633104,null,"WL12",null,null,"12 units","BOX","EA",12.5,4125]
[null,"WL12FP"]
[null,"WL12FP",null,"WL12FP",null,null,"12 units","BOX","EA",16.666666666666664,5499.9999999999991]
[null,"Baseball cap - foam liner - (min order qty for cap with your logo: 100 pcs)"]
[null,"A168199-00",null,"Dark Blue ",null,null,"10 units","BOX","BOX",19.062121212121209,6290.4999999999991]

{"sheet":"Respiratory Protection","index":4,"n_rows":646,"n_cols":11,"rows_kept":646,"cut":false,"hidden":false,"merged":[]}
[null,"Respiratory Protection |  SINGLE-USE PREMIUM RANGE",null,null,null,null,""]
[null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per","NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null," 5000 PREMIUM RANGE "]
[null,"Ergonomically designed for a high additional comfort"]
[null,"Range of highly comfortable and ergonomically designed single-use respirators. Leverages the Willtech™ soft seal technology for an improved fit and exceptional comfort. "]
[null,"Ideal for demanding environment. Available in moulded and flat-fold versions. Available in FFP1, FFP2, FFP3. Dolomite tested."]
[null,1005580,null,"Honeywell 5110 M/L - FFP1 NR D\nFFP1 Non Reusable Moulded EN particulate respirator with a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units ","CAS","EA",0.73636363636363633,243]
[null,1005113,null,"Honeywell 5110 XL - FFP1 NR D\nFFP1 Non Reusable Moulded EN particulate respirator with a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Extra-Large. Boxes of 20.",null,null,"200 units ","CAS","EA",0.73636363636363633,243]
[null,1005582,null,"Honeywell 5111 M/L - FFP1 NR D\nFFP1 Non Reusable Moulded EN particulate respirator, with a valve, a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units ","CAS","EA",1.209090909090909,398.99999999999994]
[null,1005584,null,"Honeywell 5210 M/L - FFP2 NR D\nFFP2 Non Reusable Moulded EN particulate respirator with a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units ","CAS","EA",1,330]
[null,1005586,null,"Honeywell 5211 M/L - FFP2 NR D \nFFP2 Non Reusable Moulded EN particulate respirator, with a valve, a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units ","CAS","EA",1.427272727272727,470.99999999999994]
[null,1005099,null,"Honeywell 5211 XL - FFP2 NR D \nFFP2 Non Reusable Moulded EN particulate respirator, with a valve, a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Extra Large. Boxes of 20.",null,null,"200 units ","CAS","EA",1.427272727272727,470.99999999999994]
[null,1005588,null,"Honeywell 5221 M/L - FFP2 NR D \nFFP2 Non Reusable Moulded EN particulate respirator, with a valve, a Willtech™ full-face seal and adjustable braids. Dolomite tested. Size Medium-Large. Boxes of 5.",null,null,"50 units","CAS","EA",2.8818181818181814,950.99999999999989]
[null,1005120,null,"Honeywell 5221 XL - FFP2 NR D \nFFP2 Non Reusable Moulded EN particulate respirator, with a valve, a Willtech™ full-face seal and adjustable braids. Dolomite tested. Size Extra-Large. Boxes of 5.",null,null,"50 units","CAS","EA",2.8818181818181814,950.99999999999989]
[null,1005602,null,"Honeywell 5321 M/L - FFP3 NR D \nFFP3 Non Reusable Moulded EN particulate respirator, with a valve, a Willtech™ full-face seal and adjustable braids. Dolomite tested. Size Medium-Large. Boxes of 5.",null,null,"50 units","CAS","EA",3.7272727272727262,1229.9999999999995]
[null,1005126,null,"Honeywell 5321 XL - FFP3 NR D \nFFP3 Non Reusable Moulded EN particulate respirator, with a valve, a Willtech™ full-face seal and adjustable braids. Dolomite tested. Size Extra-Large. Boxes of 5.",null,null,"50 units","BOX","EA",3.7272727272727262,1229.9999999999995]
[null,"HONEYWELL 4000 PREMIUM SERIES RESPIRATORS"]
[null,"Individually packaged single-use respirators in an instruction-marked sachet for convenience, fold flat to fit easily into a pocket"]
[null,"Features the Willtech® ultra soft triple seal which provides a high level of comfort and fit"]
[null,"Dolomite tested demonstrating the respirators’ resistance to clogging over time"]
[null,1005605,null,"Honeywell 4110 - FFP1 NR D\nFFP1 Non Reusable Foldable EN particulate respirator, with a Willtech™ half-face seal and a sliding elastic ring. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units ","CAS","EA",0.76363636363636356,251.99999999999997]
[null,1005608,null,"Honeywell 4111 - FFP1 NR D\nFFP1 Non Reusable Foldable EN particulate respirator, with a valve, a Willtech™ half-face seal and a sliding elastic ring. Dolomite tested. Size Medium-Large. Boxes of 10.",null,null,"10 db","CAS","EA",1.1272727272727272,372]
[null,1005611,null,"Honeywell 4210 - FFP2 NR D\nFFP2 Dolomite tested. Foldable EN particulate respirator mask, Willtech™ half-face seal and sliding elastic ring. Size Medium-Large. Boxes of 20.",null,null,"200 units ","CAS","EA",0.99090909090909085,327]
[null,1005614,null,"Honeywell 4211 - FFP2 NR D\nFFP2 Dolomite tested. Foldable EN particulate respirator mask, with valve, Willtech™ half-face seal and sliding elastic ring. Size Medium Large. Boxes of 10.",null,null,"100 units","CAS","EA",1.3454545454545455,444]
[null,1005630,null,"Honeywell 4311 - FFP3 NR D\nFFP3 Dolomite tested. Foldable EN particulate respirator mask, Willtech™ half-face seal and sliding elastic ring. Size Medium-Large. Boxes of 10.",null,null,"10 db","CAS","EA",3.2727272727272729,1080]
[null,"Respiratory Protection |  SINGLE-USE RESPIRATORS",null,null,null,null,""]
[null,"HONEYWELL 2000 COMFORT SERIES RESPIRATORS"]
[null,"Fold-flat respirator packed in an individually sealed bag for easy transportation and storage"]
[null,"Ergonomic design delivers outstanding levels of comfort and adjustment"]
[null,"Cut out shape provides excellent compatability with goggles"]
[null,"Dolomite tested demonstrating the respirators’ resistance to clogging over time"]
[]
[null,"NEW DESIGN AND BETTER PERFORMANCE WITH UPGRADED VERSION OF 2000 SERIES"]
[]
[null,1031590,null,"2110 FFP1 without valve","EN149:\nFFP1\nNR D",null,"400 units","CAS","EA",0.7,230.99999999999997]
[null,1031591,null,"2111 FFP1 with valve","EN149:\nFFP1\nNR D",null,"320 units","CAS","EA",0.96363636363636362,318]
[null,1031592,null,"2210 FFP2 without valve","EN149:\nFFP2\nNR D",null,"400 units","CAS","EA",0.79090909090909089,261]
[null,1031593,null,"2211 FFP2 with valve","EN149:\nFFP2\nNR D",null,"320 units","CAS","EA",1.1272727272727272,372]
[null,1031594,null,"2311 FFP3 with valve","EN149:\nFFP3\nNR D",null,"320 units","CAS","EA",1.5909090909090908,525]
[null,null,null,null,null,null,""]
[null,"COMFORT SERIES 5000 "]
[null,"The best combination in terms of performance for standard working conditions. Good fit and comfort thoroughout the day. "]
[null,1007221,null,"Honeywell 5185 M/L - FFP1 NR \nFFP1 Non Reusable Moulded EN particulate respirator mask, with a nose seal and twin-stapled elastics. Size Medium/Large. Boxes of 20.",null,null,"20 db","CAS","EA",0.53636363636363626,176.99999999999997]
[null,1007222,null,"Honeywell 5186 M/L- FFP1 NR\nFFP1 Non Reusable Moulded EN particulate respirator mask, with a valve, a nose seal and twin-stapled elastics. Size Medium/Large. Boxes of 20.",null,null,"200 units ","CAS","EA",0.88181818181818172,290.99999999999994]
[null,1007223,null,"Honeywell 5208 M/L - FFP2 NR\nFFP2 Non Reusable Moulded EN particulate respirator mask, with a nose seal and twin-stapled elastics. Size Medium/Large. Boxes of 20.",null,null,"200 units ","CAS","EA",0.64545454545454539,212.99999999999997]
[null,1007224,null,"Honeywell 5209 M/L - FFP2 NR\nFFP2 Non Reusable Moulded EN particulate respirator mask, with a valve, a nose seal and twin-stapled elastics. Size Medium/Large. Boxes of 20.",null,null,"200 units ","CAS","EA",1.1454545454545455,378]
[null,1015635,null,"Honeywell 5311 M/L - FFP3 NR D\nFFP3 Non Reusable Moulded EN particulate respirator mask, with a valve, a full-face seal and twin-stapled elastics. Dolomite tested. Size Medium/Large. Boxes of 10.",null,null,"200 units ","CAS","EA",1.6636363636363636,549]
[null,"Respiratory Protection |  SINGLE-USE RESPIRATORS",null,null,null,null,""]
[null,"SPECIALITY SERIES 5000 "]
[null,"Enhanced comfort against specific odours. Range of moulded masks specifically designed to deal with nuisance level organic & acid gases. "]
[null,"Superior odour removal capabilities. Excellent comfort with adjustable straps and the Willtech™ soft seal technology with high moisture absorption properties. "]
[null,"Available in FFP1 and FFP2. Dolomite tested."]
[null,1005591,null,"Honeywell 5140 M/L - FFP1 NR D\nFFP1 Non Reusable Moulded EN particulate respirator against nuisance level organic vapours, a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units","CAS","EA",1.2545454545454544,413.99999999999994]
[null,1005593,null,"Honeywell 5141 M/L - FFP1 NR D\nFFP1 Non Reusable Moulded EN particulate respirator against nuisance level organic vapours, with a valve, a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units","CAS","EA",2,660]
[null,1005595,null,"Honeywell 5251 M/L - FFP2 NR D\nFFP2 Non Reusable Moulded EN particulate respirator against nuisance level organic vapours, with a valve, a Willtech™ full-face seal and adjustable braids. Dolomite tested. Size Medium-Large. Boxes of 5.",null,null,"50 units","CAS","EA",3.9727272727272722,1310.9999999999998]
[null,1005122,null,"Honeywell 5251 XL - FFP2 NR D\nFFP2 Non Reusable Moulded EN particulate respirator against nuisance level organic vapours, with a valve, a Willtech™ full-face seal and adjustable braids. Dolomite tested. Size Extra-Large. Boxes of 5.",null,null,"50 units","CAS","EA",3.9727272727272722,1310.9999999999998]
[null,1005598,null,"Honeywell 5161 M/L - FFP1 NR D\nFFP1 Non Reusable Moulded EN particulate respirator against nuisance level acid gases, with a valve, a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units","CAS","EA",1.9909090909090905,656.99999999999989]
[null,1005600,null,"Honeywell 5261 M/L - FFP2 NR D\nFFP2 Non Reusable Moulded EN particulate respirator against nuisance level acid gases, with a valve, a Willtech™ half-face seal and twin-stapled elastics. Dolomite tested. Size Medium-Large. Boxes of 20.",null,null,"200 units","CAS","EA",2.3272727272727272,768]
[]
[null,"SUPERONE  SERIES ",null,null,null,null,""]
[null,"Economic, simple and effective",null,null,null,null,""]
[null,"Value single-use respirators",null,null,null,null,""]
[null,1013203,null,"SuperOne 3203 - FFP1 NR\nFFP1 Non Reusable Moulded EN particulate respirator mask with a pre-shaped nose area and twin-stapled elastics. A \"one size fits all\" design. Boxes of 30 masks.","EN149:\nFFP1\nNR D",null,"300 units","CAS","EA",0.40909090909090912,135]
[null,1013204,null,"SuperOne 3204 - FFP1 NR\nFFP1 Non Reusable Moulded EN particulate respirator with a valve, a pre-shaped nose area and twin-stapled elastics. A \"one size fits all\" design. Boxes of 20 masks.","EN149:\nFFP1\nNR D",null,"200 units ","CAS","EA",0.68181818181818177,224.99999999999997]
[null,1013205,null,"SuperOne 3205 - FFP2 NR\nFFP2 Non Reusable Moulded EN particulate respirator with a pre-shaped nose area and twin-stapled elastics. A \"one size fits all\" design. Boxes of 30 masks.","EN149:\nFFP2\nNR D",null,"300 units","CAS","EA",0.50909090909090915,168.00000000000003]
[null,1013206,null,"SuperOne 3206 - FFP2 NR\nFFP2 Moulded EN particulate respirator with a valve, a pre-shaped nose area and twin-stapled elastics. A \"one size fits all\" design. Boxes of 20 masks.","EN149:\nFFP2\nNR D",null,"200 units ","CAS","EA",0.71818181818181814,237]
[null,1032501,null,"SuperOne 3207\nFFP3 Non Reusable Moulded EN particulate respirator mask with a pre-shaped nose area and twin-stapled elastics. A \"one size fits all\" design. Boxes of 30 masks.",null,null,"300 units","CAS","EA",0.64545454545454539,212.99999999999997]
[null,1032502,null,"SuperOne 3208\nFFP3 Moulded EN particulate respirator with a valve, a pre-shaped nose area and twin-stapled elastics. A \"one size fits all\" design. Boxes of 20 masks.",null,null,"200 units ","CAS","EA",0.89090909090909087,294]
[null,1015639,null,"EasyFit 300 - FFP3 NR\nFFP3 Foldable EN particulate respirator mask with a single welded elastic. Size Medium-Large. Boxes of 30.",null,null,"300 units","CAS","EA",0.51818181818181808,170.99999999999997]
[null,1018921,null,"EasyFit 200 - FFP2 NR\nFFP2 Foldable EN particulate respirator mask with a single welded elastic. Size Medium-Large. Boxes of 30.",null,null,"300 units","CAS","EA",0.36363636363636359,119.99999999999999]
[null,"Respiratory Protection |  FIT TEST KIT"]
[null,"FIT-TEST KIT",null,null,null,null,""]
[null,"Bitrex fit test kit is used to test the fit of a respirator on an individual - Legislation requires that all of the preceding respirators"]
[null,"(single-use, half and full-face respirators) are face-fit-tested to the user"]
[null,"● Fit-Test kit is suitable for the testing of single-use disposable and half-mask respirators"]
[null,1010051,null,"Bitrex Fit Test kit",null,null,"1 unit","EA","KIT",157.41818181818181,51948]
[null,1010052,null,"Sensitazation test solution (6 ampoules) duration 1 day after opening - storage shelf life : 2 years",null,null,"1 unit","","EA",15.299999999999997,5048.9999999999991]
[null,1010053,null,"Fit test solution (6 ampoules) duration 1 day after opening - storage shelf life : 2 years",null,null,"1 unit","","KIT",15.963636363636363,5268]
[]
[null,"Respiratory Protection |  HALF MASKS AND FULL FACE MASKS "]
[null,"FREEDOM HALF-MASKS",null,null,null,null,""]
[null,"Maintenance free, semi-disposable half mask for occasional or frequent exposures to gases, vapours and particulates. Available in one size fitting all."]
[null,1001597,null,"Freedom P3","EN405",null,"10 units","BOX","EA",13.809090909090907,4556.9999999999991]
[null,1001591,null,"Freedom A1","EN405",null,"10 units","BOX","EA",11.136363636363635,3674.9999999999995]
[null,1001598,null,"Freedom A2","EN405",null,"10 units","BOX","EA",12.554545454545453,4142.9999999999991]
[null,1001607,null,"Freedom A1 + 10 pairs of protection prefilters","EN405",null,"10 units","BOX","EA",13.336363636363636,4401]
[null,1001592,null,"Freedom A1P1","EN405",null,"10 units","BOX","EA",11.772727272727272,3884.9999999999995]
[null,1001601,null,"Freedom A2P2","EN405",null,"1 db","BOX","EA",13.336363636363636,4401]
[null,1001602,null,"Freedom A2P3","EN405",null,"10 units","BOX","EA",17.263636363636362,5696.9999999999991]
[null,1001610,null,"Freedom disposable mask A1B1E1K1-P3  ","EN405",null,"10 units","BOX","EA",20.709090909090911,6834.0000000000009]
[null,"CLIP ON P1 AND P2 FILTER PADS AND RETAINERS FOR USE WITH FREEDOM GAS/VAPOUR FILTERS"]
[null,1002800,null,"P1 Pre-filter","EN143",null,"20 units","BOX","EA",2.0545454545454542,677.99999999999989]
[null,1002801,null,"P2 Pre-filter","EN143",null,"1 db","BOX","EA",2.1090909090909089,695.99999999999989]
[null,1001606,null,"RP78 Retainer for TP1S / TP2S filters, Freedom",null,null,"20 units","BOX","EA",0.96363636363636362,318]
[null,"TWIN FILTER RESPIRATORS",null,null,null,null,""]
[null,"Filters attach using 'click-fit' system to provide a secure fastening by 1/4 turn with a positive audible click"]
[null,"VALUAIR HALF MASK",null,null,null,null,""]
[null,1001573,null,"Valuair Half-mask, Twin.","EN140","M","10 units","BOX","EA",6.8909090909090907,2274]
[null,1001574,null,"Valuair Half-mask, Twin.","EN140","L","1 db","BOX","EA",7.7272727272727266,2550]
[null,"PREMIER HALF MASK"]
[null,1001575,null,"Premier Half-mask, Twin.","EN140","M","10 units","BOX","EA",17.127272727272725,5651.9999999999991]
[null,1001576,null,"Premier Half-mask, Twin. ","EN140","L","10 units","BOX","EA",17.127272727272725,5651.9999999999991]
[null,"MX/PF F950 HALF MASK"]
[null,1001558,null,"MX/PF 950 Half-mask, Twin. ","EN140","M","10 units","BOX","EA",31.527272727272724,10403.999999999998]
[null,"OPTIFIT TWIN full face respirator\n\n\n",null,null,null,null,""]
[null,"● high optical quality, impact and abrasion resistant polycarbonate visor ● comfortable silicone inner mask with easy maintenance valves, prevents misting of the visor"]
[null,1715231,null,"Opti-fit Full-face mask, Twin.","EN136","S","1 unit","","EA",76.61818181818181,25283.999999999996]
[null,1715241,null,"Opti-fit Full-face mask, Twin.","EN136","M","1 unit","","EA",76.61818181818181,25283.999999999996]
[null,1715251,null,"Opti-fit Full-face mask, Twin.","EN136","L","1 unit","","EA",76.61818181818181,25283.999999999996]
[null,"T-SERIES FILTERS",null,null,null,null,""]
[null,"Filters for use with all Twin Filter half and full-face respirators",null,null,null,null,""]
[null,1001619,null,"A1 Organic vapour","EN 14387, EN 143",null,"10 units","BOX","EA",2.8545454545454541,941.99999999999989]
[null,1001577,null,"A2 Organic vapour","EN 14387, EN 143",null,"10 units","BOX","EA",3.7181818181818178,1226.9999999999998]
[null,1001581,null,"ABEK1 ","EN 14387, EN 143",null,"10 units","BOX","EA",4.7545454545454549,1569]
[null,1001620,null,"A1P3 Organic / High Efficiency","EN 14387, EN 143",null,"6 units","BOX","EA",5.672727272727272,1871.9999999999998]
[null,1001583,null,"A2P3 Organic / High Efficiency","EN 14387, EN 143",null,"6 units","BOX","EA",6.1818181818181817,2040]
[null,1001587,null,"ABEK1P3","EN 14387, EN 143",null,"6 units","BOX","EA",6.6,2178]
[null,1003529,null,"Low Profile P3 Cartridge","EN 14387, EN 143",null,"1 db","BOX","EA",3.6181818181818177,1193.9999999999998]
[null,"Respiratory Protection |  HALF MASKS AND FULL FACE MASKS "]
[]
[null,1001609,null,"A1B1P3","EN 14387, EN 143",null,"6 units","BOX","EA",8.2272727272727284,2715.0000000000005]
[null,1001582,null,"P3 DUAL FILTER","EN 14387, EN 143",null,"10 units","BOX","EA",3.6636363636363636,1209]
[null,1001584,null,"B1P3 Click-Fit","EN 14387, EN 143",null,"6 units","BOX","EA",6.2454545454545451,2061]
[]
[null,"CLIP ON P1 AND P2 FILTER PADS AND RETAINERS FOR USE WITH TWIN GAS/VAPOUR FILTERS",null,null,null,null,""]
[null,1001590,null,"79900517 RP22 Retainer for TP1S / TP2S filters, Click-fit series",null,null,"20 units","BOX","EA",0.97272727272727266,321]
[null,null,null,null,null,null,""]
[null,"Respiratory Protection |  HALF-MASKS",null,null,null,null,""]
[]
[null,"N5500"]
[null,"N65550031",null,"N5500 Half-mask, Twin. Elastomer ","EN 140","S","12 units","BOX","EA",12.236363636363636,4038]
[null,"N65550032",null,"N5500 Half-mask, Twin.  Elastomer ","EN 140","M","12 units","BOX","EA",12.236363636363636,4038]
[null,"N65550033",null,"N5500 Half-mask, Twin.  Elastomer ","EN 140","L","12 units","BOX","EA",12.236363636363636,4038]
[null,"N7700"]
[null,"N65770031",null,"N7700 Half-mask, Twin.Silicone","EN 140","S","12 units","BOX","EA",19.77272727272727,6524.9999999999991]
[null,"N65770032",null,"N7700 Half-mask, Twin. Silicone","EN 140","M","12 units","BOX","EA",19.77272727272727,6524.9999999999991]
[null,"N65770033",null,"N7700 Half-mask, Twin. Silicone","EN 140","L","12 units","BOX","EA",19.77272727272727,6524.9999999999991]
[null,"N5400"]
[null,"N65754101",null,"5400 Full-face mask, Twin, Elastomer","EN 136","M/L","1 unit","EA","EA",47.063636363636363,15531]
[null,"Respiratory Protection |  N series filters",null,null,null,null,""]
[]
[null,"DUST FILTERS"]
[null,"N06575008",null,"P3  dust filter",null,null,"4 units","BOX","BOX",12.8,4224]
[null,"N7500P3",null,"Pancake P3 dust filter",null,null,"20 units","BOX","PR",5.7181818181818178,1886.9999999999998]
[null,"N7500P3O",null,"Pancake P30 - carbon dust filter",null,null,"20 units","BOX","PR",7.2636363636363628,2396.9999999999995]
[null,"N06575035",null,"Adapter Pancake filter",null,null,"24 units","EA","EA",2.7181818181818183,897]
[null,"PREFILTER"]
[null,"7506P2",null,"P2 prefilter for N series",null,null,"100 units","CASE","CASE",173.26363636363635,57176.999999999993]
[null,"GAS FILTERS"]
[null,"N06575001A2",null," A2 gas filter",null,null,"1 pár","BOX","PR",6.7181818181818169,2216.9999999999995]
[null,"N06575001L",null,"A1 gas filter ",null,null,"12 units","BOX","PR",3.8727272727272721,1277.9999999999998]
[null,"N06575003L",null,"A1B1E1 gas filter",null,null,"12 units","BOX","PR",7.0818181818181811,2336.9999999999995]
[null,"N06575004L",null,"K1 gas filter",null,null,"12 units","BOX","PR",7.5636363636363635,2496]
[null,"N06575009L",null,"ABEK1 gas filter",null,null,"12 units","BOX","PR",11.145454545454545,3677.9999999999995]
[null,"COMBINED FILTERS"]
[null,"N06575001A2P3",null," A2P3 combined filter",null,null,"8 units","BOX","PR",11.8,3894.0000000000005]
[null,"N06575081L",null,"A1P3 Combined filter",null,null,"8 units","BOX","PR",13.18181818181818,4349.9999999999991]
[null,"N06575084L",null,"K1P3 Combined filter",null,null,"8 units","BOX","PR",15.509090909090906,5117.9999999999991]
[null,"N06575083L",null,"A1B1E1P3 Combined filter",null,null,"8 units","BOX","PR",17.454545454545453,5760]
[null,"N06575089L",null,"A1B1E1K1P3 Combined filter",null,null,"8 units","BOX","PR",18.427272727272726,6081]
[null,"N750036A",null,"Filter cover",null,null,"12 units","CAS","EA",0.77272727272727271,255]
[null,"N7700 CLASS 2 "]
[null,"N65770015",null,"N7700 half-mask, Mono. ","EN 140","S","12 units","BOX","EA",24.472727272727273,8076]
[null,"N65770016",null,"N7700 half-mask, Mono.","EN 140","L","12 units","BOX","EA",24.472727272727273,8076]
[null,"N5400 CLASS 2 "]
[null,"N65754201",null,"5400 Full-face mask, Mono, Elastomer","EN 136","M/L","1 unit","EA","EA",47.063636363636363,15531]
[null,"N65754301",null,"5400 Full-face mask, Mono, Silicone","EN 136","M/L","1 unit","EA","EA",56.481818181818177,18639]
[null,"Respiratory Protection |  REUSABLE FULL FACE MASKS",null,null,null,null,""]
[null,"OPTIFIT SINGLE full face respirator",null,null,null,null,""]
[null,"● high optical quality, impact and abrasion resistant polycarbonate visor"]
[null,"● comfortable silicone inner mask with easy maintenance valves, prevents misting of the visor"]
[]
[null,1715001,null,"Optifit full-face mask, Mono","EN136","S","1 unit","EA","EA",75.672727272727258,24971.999999999996]
[null,1715011,null,"Opti-fit Full-face mask, Mono,","EN136","M","1 unit ","EA","EA",75.672727272727258,24971.999999999996]
[null,1715021,null,"Opti-fit Full-face mask, Mono","EN136","L","1 unit ","EA","EA",75.672727272727258,24971.999999999996]
[]
[null,"PANORAMASQUE",null,null,null,null,""]
[null,"Full-face respirator with extra-wide field of vision and chemical resistant visor",null,null,null,null,""]
[null,1710394,null,"Panoramasque EPDM (black) full face respirator with PMMA lens ","EN136",null,"1 unit","EA ","EA",74.890909090909076,24713.999999999996]
[null,1710987,null,"Panoramasque silicone full face respirator, PMMA lens and speech diaphragm ","EN136",null,"1 unit","EA ","EA",132.42727272727271,43700.999999999993]
[null,1710395,null,"Panoramasque EPDM full face respirator with PMMA lens and speech diaphragm","EN136",null,"1 unit","EA ","EA",89.872727272727261,29657.999999999996]
[null,1711000,null,"Panoramasque (black, EPDM) - Chlorine lenses + 5-point head-harness ","EN136",null,"1 unit ","EA ","EA",122.97272727272728,40581]
[null,1711001,null,"Panoramasque EPDM full face respirator with triple layer glass lens (Triplex)","EN136",null,"1 unit","EA ","EA",139.99999999999997,46199.999999999993]
[null,"Respiratory Protection |  REUSABLE FULL FACE MASKS",null,null,null,null,""]
[]
[null,1710980,null,"Panoramasque EPDM. Panoramasque in yellow silicone with PMMA (methacrylate) lens",null,null,"1 unit",null,"EA",132.42727272727271,43700.999999999993]
[null,1710372,null,"Panoramasque EPDM with polycarbonate lens and speech diaphgram",null,null,"1 unit",null,"EA",138.67272727272726,45761.999999999993]
[null,1728753,null,"Panoramasque EPDM with methacrylate lens and speech diaphgram",null,null,"1 unit",null,"EA",193.12727272727273,63732]
[null,"Respiratory Protection |  Filters  Class 2 ",null,null,null,null,""]
[]
[null,"ALUMINIUM FILTERS"]
[null,1785010,null,"A2 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",10.427272727272728,3441]
[null,1783010,null,"A2 P3 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",11.627272727272725,3836.9999999999991]
[null,1785040,null,"A2B2 aluminum  canister","EN 14387, EN 143",null,"1 unit","EA","EA",12.399999999999999,4091.9999999999995]
[null,1783040,null,"A2 B2 P3 - A3 B3 P TM3 TM2 / A2 B2 P TH2 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",16.936363636363634,5588.9999999999991]
[null,1785030,null,"B2 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",12.154545454545451,4010.9999999999986]
[null,1783030,null,"B2 P3 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",19.427272727272729,6411.0000000000009]
[null,1785080,null,"K2 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",12.363636363636363,4080]
[null,1781080,null,"K2 aluminium canister","EN 14387, EN 143",null,"1 unit","EA","EA",13.727272727272725,4529.9999999999991]
[null,1783080,null,"K2 P3 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",20.254545454545454,6684]
[null,1784000,null,"A2B2E2K2 P3 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",17.418181818181818,5748]
[null,1786730,null,"A2B2E2K1 NO P3  ","EN 14387, EN 143",null,"1 unit","EA","EA",38.463636363636361,12693]
[null,1781000,null,"A2B2E2K2 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",14.918181818181818,4923]
[null,1785025,null,"AX aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",13.018181818181818,4296]
[null,1785018,null,"AX P3 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",19.2,6336]
[null,1784140,null,"Hg (Mercury) P3 ","EN 14387, EN 143",null,"1 unit","EA","EA",26.172727272727268,8636.9999999999982]
[null,1786200,null,"RD40 AL - I.P.R.","EN 14387, EN 143",null,"1 unit","EA","EA",34.372727272727268,11342.999999999998]
[null,1785019,null,"A2B2E2K1 HgP3 aluminum canister","EN 14387, EN 143",null,"1 unit","EA","EA",19.381818181818179,6395.9999999999991]
[null,1785012,null,"AX B2 aluminum canister","EN371",null,"1 unit","EA","EA",13.718181818181819,4527]
[null,1783000,null,"A2B2E2K1 P3 aluminium filter canister","EN141/143",null,"1 unit","EA","EA",16.354545454545452,5396.9999999999991]
[null,1785000,null,"A2 B2 E2 K1 - A3 B3 E3 K2 TM3 TM2 / A2 B2 E2 K1  TH2  aluminum canister",null,null,"1 unit","EA","EA",14.18181818181818,4679.9999999999991]
[null,1785011,null,"AX aluminum canister",null,null,"1 unit","EA","EA",10.345454545454546,3414]
[null,1785014,null,"AXB2P3 aluminum  canister"," EN148, EN 143, EN 14387",null,"1 unit","EA","EA",21.318181818181817,7034.9999999999991]
[]
[null,"PLASTIC FILTER CANISTERS FOR SINGLE FILTER RESPIRATORS",null,null,null,null,""]
[null,1788000,null,"A2 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",7.5727272727272723,2499]
[null,1788005,null,"A2P3 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",10.390909090909091,3429]
[null,1788075,null,"A2B2 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",9.5636363636363626,3155.9999999999995]
[null,1788070,null,"A2B2P3 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",11.909090909090908,3929.9999999999995]
[null,1788010,null,"B2 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",10.081818181818182,3327]
[null,1788015,null,"B2P3 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",11.909090909090908,3929.9999999999995]
[null,1788020,null,"K2 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",11.027272727272727,3639]
[null,1788025,null,"K2P3 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",13.809090909090907,4556.9999999999991]
[null,1788150,null,"A2B2E2K2 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",13.281818181818181,4383]
[null,1788155,null,"A2B2E2K2P3 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",14.590909090909092,4815]
[null,1788161,null,"AX plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",10.081818181818182,3327]
[null,"BULK PACK PLASTIC & ALUMINUM FILTER CANISTERS FOR SINGLE FILTER RESPIRATORS"]
[null,"1783010-B",null,"A2P3 ALUMINIUM","EN 14387, EN 143",null,"27 units","CAS","EA",10.5,3465]
[null,"1784000-B",null,"ABEK2P3 ALUMINIUM","EN 14387, EN 144",null,"27 units","CAS","EA",15.254545454545454,5034]
[null,"1786000-B",null,"P3 PLASTIC","EN 14387, EN 145",null,"1 db","CAS","EA",4.545454545454545,1499.9999999999998]
[null,"1788070-B",null,"AB2P3 PLASTIC","EN 14387, EN 146",null,"27 units","CAS","EA",10.399999999999999,3431.9999999999995]
[null,"1788155-B",null,"ABEK2P3 PLASTIC","EN 14387, EN 147",null,"27 units","CAS","EA",12.527272727272726,4133.9999999999991]
[null,"1783040-B",null,"AB2P3 ALUMINIUM","EN 14387, EN 148",null,"27 units","CAS","EA",14.745454545454544,4866]
[null,"1788005-B",null,"A2P3 PLASTIC","EN 14387, EN 149",null,"27 units","CAS","EA",9.0818181818181802,2996.9999999999995]
[null,"1788150-B",null,"ABEK2 PLASTIC","EN 14387, EN 150",null,"27 units","CAS","EA",12.527272727272726,4133.9999999999991]
[null,"1788075-B",null,"A2B2 PLASTIC","EN 14387, EN 151",null,"27 units","CAS","EA",8.418181818181818,2778]
[null,"1785010-B",null,"A2 ALUMINIUM","EN 14387, EN 152",null,"27 units","CAS","EA",8.9272727272727277,2946]
[null,"1785040-B",null,"A2B2 ALUMINIUM","EN 14387, EN 153",null,"27 units","CAS","EA",10.981818181818181,3623.9999999999995]
[null,"1781000-B",null,"ABEK2 ALUMINIUM","EN 14387, EN 154",null,"27 units","CAS","EA",13.854545454545454,4572]
[]
[null,"Respiratory Protection |  Filters  Class 2 ",null,null,null,null,""]
[]
[null,1788166,null,"AXP3 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",10.536363636363635,3476.9999999999995]
[null,"Particules "]
[null,1786000,null,"P3 plastic canister","EN 14387, EN 143",null,"5 units","BOX","EA",5.1818181818181817,1710]
[null,1786110,null,"P3 double threading plastic",null,null,"5 units","BOX","EA",11.290909090909091,3726]
[]
[null,"Respiratory Protection |  Accesories",null,null,null,null,""]
[null,"Disposable visor covers, cases and googles"]
[null,1001557,null,"F38 adaptor for MX/PF 950",null,null,"12 units","BOX","EA",10.572727272727274,3489.0000000000005]
[null,1710088,null,"Box of 20 disposable lenses for Panoramasque",null,null,"1 unit","EA","EA",95.999999999999986,31679.999999999996]
[null,1710174,null,"Protective visor covers  OPTIFIT",null,null,"25 units","BOX","BOX",52.8,17424]
[null,"N80836A",null,"Disposable visors for 5400",null,null,"15 units ","BAG","BAG",15.363636363636362,5069.9999999999991]
[null,1772525,null,"X Pack Case ",null,null,"1 unit","EA","EA",25.454545454545453,8400]
[null,1772526,null,"X pack case, easyly demontaminated ",null,null,"1 unit ","BOX","EA",19.999999999999996,6599.9999999999991]
[null,"3022300-STD",null,"Pano/OptiFit prescription eyewear frame ",null,null,"1 unit","EA","EA",81.199999999999989,26795.999999999996]
[null,"Maintenance "]
[null,1779065,null,"PPE cleaning product US - 5 liters",null,null,"1 unit","EA","EA",105.45454545454544,34799.999999999993]
[null,1779061,null,"ALTUSIL eyepiece burette",null,null,"1 unit","","EA",9.6999999999999993,3200.9999999999995]
[null,"N65700300",null,"7003 Respirator wipes ",null,null,"1 unit","BOX","BOX",19.009090909090908,6273]
[]
[null,"Respiratory Protection |  ESCAPE /  EVACUATION EQUIPMENT",null,null,null,null,""]
[]
[null,"EVAMASQUE - FILTERING HALF -MASK FOR 15 MINUTES OF EVACUATION FROM CHEMICAL ENVIRONMENTS "]
[null,1728570,null,"Evamasque - Full face mask with  ABEK filter ","DIN 58647-7",null,"1 unit","EA","EA",44.809090909090905,14786.999999999998]
[null,1728571,null,"MAINTENANCE KIT 4 anti-gas filter (includes seal label + elastic strap) ","DIN 58647-7",null,"1 unit","BOX","BOX",67.536363636363646,22287.000000000004]
[null,"EVAMASQUE SPARE PARTS "]
[null,1728575,null,"Exhalation valve dismounting tool ",null,null,"1 unit","EA","EA",24.954545454545453,8235]
[null,1779993,null,"EVAMASQUE BOX AND STRAP",null,null,"1 unit","EA","EA",24.45454545454545,8069.9999999999982]
[null,"SPD00007027",null,"ADHESIVE TAPE- 33 meters (enough for 60 device)",null,null,"1 ROL","ROL","EA",25.636363636363633,8459.9999999999982]
[null,1728502,null,"HALF MASK EVAMASQUE",null,null,"1 unit","EA","EA",26.3,8679]
[]
[null,"OPENGO - COMPACT AND EASY TO USE ESCAPE HOOD FOR USE IN  HIGH RISK CHEMICAL ENVIRONMENT "]
[null,1728806,null,"OPENGO with ABEK1 P3 filter intended for escape in the event of chemical pollution with particles - Comes with a carrying case with belt","EN 140, EN 14387",null,"1 unit","","EA",148.18181818181816,48899.999999999993]
[null,1728807,null,"OPENGO with IPR D91 filter for escape in the event of iodine or radioactive dust pollution - Comes with a carrying case with belt ","EN 140, EN 14387",null,"1 unit","","EA",184.5272727272727,60893.999999999993]
[null,"Respiratory Protection | POWERED AIR PURYFYING RESPIRATORS (PAPR)",null,null,null,null,""]
[null,"TURBOVISOR - COMPLETE KIT FOR OPTIMAL COMFORT AND PROTECTION AGAINST PARTICLES"]
[null,1001769,null,"Turbovisor MV complete kit with hood and polycarbonate visor, 2 disposable visor covers, 1 cotton head cover, 1 spare fabric, 1 power unit, 8 hour waist mounted battery pack, 1 battery charger unit and fabric carrying bag.",null,null,"1 unit","EA","EA",403.16363636363639,133044]
[null,1001771,null,"Turbovisor MV complete kit with hood and polycarbonate visor, 2 disposable visor covers, 1 cotton head cover, 1 spare fabric, 1 power unit, 6 hour browguard mounted battery pack, 1 battery charger unit and fabric carrying bag.",null,null,"1 unit","EA","EA",393.56363636363636,129876]
[null,1001734,null,"Charger for 8 hour battery Turbovisor MV",null,null,"1 unit","EA","EA",56.645454545454548,18693]
[null,1001805,null,"Charger for 6 hour battery DTVS-1511 for Turbovisor MV",null,null,"1 unit","EA","EA",62.399999999999991,20591.999999999996]
[null,"Respiratory Protection |  CompactAir",null,null,null,null,""]
[null,"COMPACT AIR  - SIMPLE, ROBUST AND RELIABLE BREATHING APPARATUS",null,null,null,null,""]
[null,"A150102-00",null,"Compact Air Bayonet",null,null,"1 unit","","EA",575.27272727272714,189839.99999999994]
[null,"A160006",null,"CA Battery",null,null,"1 unit","","EA",147.87272727272725,48797.999999999993]
[null,"A150103-00",null,"Compact Air  Din thread",null,null,"1 unit","","EA",575.27272727272714,189839.99999999994]
[null,"A150107",null,"CA Blower with belt and hose",null,null,"1 unit","","EA",314.26363636363635,103707]
[null,"A160723",null,"CA Comfort belt",null,null,"1 unit","","EA",31.890909090909087,10523.999999999998]
[null,"COMPACT AIR 200"]
[null,"A150401",null,"Compact Air 200 WITH BAYONET FOR HOOD",null,null,"1 unit","","EA",781.90909090909076,258029.99999999994]
[null,"A160696",null,"CA Waistbelt + backplate",null,null,"1 unit","","EA",25.036363636363632,8261.9999999999982]
[null,"A161356",null,"CA 200 Breathing tube for bayonet kit, 970 mm length",null,null,"1 unit","EA","EA",39.36363636363636,12989.999999999998]
[null,"CA222EU",null,"Lithium-ion battery pack and housing CA200",null,null,"1 unit","","EA",207.27272727272722,68399.999999999985]
[null,"A161301-10",null,"Hose cover Tyvek® -10 pcs",null,null,"10 units","BOX","BOX",233.73636363636362,77133]
[null,"CA221EU",null,"Blower CA200",null,null,"1 unit","EA","EA",894.63636363636363,295230]
[null,"CA231EU",null,"Universal battery charger CA200",null,null,"1 unit","","EA",105.59090909090908,34844.999999999993]
[null,"A160531",null,"Air flow meter for CA200",null,null,"1 unit","","EA",6.0909090909090899,2009.9999999999998]
[null,"  CompactAir Accessories ",null,null,null,null,""]
[null,"A160723",null,"Nylon Comfort pad (CAIR, CA200)",null,null,"1 unit","BOX","EA",31.890909090909087,10523.999999999998]
[null,"A001412",null,"CA 200 Breathing hose - sealing ring",null,null,"1 unit","BOX","EA",9.4999999999999982,3134.9999999999995]
[null,"A160591",null,"CA Universal charger",null,null,"1 unit","BOX","EA",101.5181818181818,33500.999999999993]
[null,"A160712",null,"Blower sealing rings -10 pcs (CAIR, CA200, Airbelt)",null,null,"10 units","BOX","BOX",10.209090909090909,3369]
[null,"A161370",null,"CA Hose bayonet",null,null,"1 unit","BOX","EA",58.163636363636357,19193.999999999996]
[null,"A161378",null,"CA Hose Din thread",null,null,"1 unit","EA","EA",58.163636363636357,19193.999999999996]
[null,"A160368",null,"Carrying case (CAIR, CA200, Airbelt)",null,null,"1 unit","EA","EA",14.363636363636363,4740]
[null,"A160684",null,"Decontamination PVC belt (CAIR, CA200)",null,null,"1 unit","EA","EA",17.563636363636363,5796]
[null,"A001783",null,"BELT PLATE for CA",null,null,"1 unit","EA","EA",9.5181818181818176,3141]
[null,"A160727",null,"PVC decontamination comfort pad (CAIR, CA200)",null,null,"1 unit","EA","EA",40.318181818181813,13304.999999999998]
[null,"A160693",null,"BELT COMPACT AIR /COMPACT AIR 200",null,null,"1 unit","EA","EA",8.1636363636363622,2693.9999999999995]
[null,"A160119",null,"Wire mesh screen",null,null,"50  units","BOX","BOX",160.9909090909091,53127]
[]
[null,"Respiratory Protection |  PAPR Hoods and welding masks",null,null,null,null,""]
[null,"PRIMAIR"]
[null,"A114110",null,"Primair VL. Class TH2","EN 12 941",null,"1 unit","","EA",152.24545454545455,50241]
[null,"A160252",null,"Tyvek hood Primair ",null,null,"5 units ","BOX","BOX",139.99999999999997,46199.999999999993]
[null,"A161472",null,"Sweatband ",null,null,"10 units","BOX","BOX",8.2727272727272716,2729.9999999999995]
[null,"PRIMAIR PLUS "]
[null,"PA111EU",null,"Primer Plus hood with bib and harness","EN 12 941",null,"1 unit","EA","EA",118.24545454545452,39020.999999999993]
[null,"PA121EU",null,"Primer Plus hood with bib and harness - coated","EN 12 941",null,"1 unit","EA","EA",126.75454545454545,41829]
[null,"PA112EU",null,"Disposable hoods Primair Plus",null,null,"3 units","BOX","BOX",59.518181818181809,19640.999999999996]
[null,"PA122EU",null,"Disposable coated hoods Primair Plus",null,null,"3 units","BOX","BOX",69.109090909090895,22805.999999999996]
[null,"PA104",null,"Sweatband Primair Plus",null,null,"10 units","BOX","BOX",18.709090909090907,6173.9999999999991]
[null,"PA105",null,"Peel away cover lens Primair Plus",null,null,"15 units","BOX","BOX",18.245454545454546,6021]
[null,"KOLIBRI - PROTECTION AGAINST IMPACTS. LIGHT AND COMFORTABLE "]
[null,"A114102",null,"KOLIBRI","EN 146",null,"1 unit","EA","EA",170.26363636363635,56186.999999999993]
[null,"A160730",null,"Disposable visor Kolibri, Junior B, Junior B Combi",null,null,"100 units","","BOX",30.509090909090908,10068]
[null,"A161472",null,"Sweatband",null,null,"10 units","BOX","BOX",8.2727272727272716,2729.9999999999995]
[null,"A160741",null,"Visor acetate Kolibri",null,null,"5 units","","BOX",80.345454545454544,26514]
[null,"A160747",null,"Visor PC Kolibri",null,null,"1 unit","","BOX",96.881818181818161,31970.999999999993]
[null,"A160138",null,"Comfa Seal Kolibri",null,null,"1 unit","","EA",26.427272727272726,8721]
[null,"A160214",null,"Headband airduct Kolibri",null,null,"1 unit","","EA",99.481818181818184,32829]
[null,"JUNIOR A  - OPTIMAL PROTECTION AND WIDE FIELD OF VIEW"]
[null,"A114106",null,"JUNIOR A","EN 12 941",null,"1 unit","","EA",191.40909090909091,63165]
[null,"A160734",null,"Disposable visors Junior A VL",null,null,100,"BOX","BOX",43.636363636363633,14399.999999999998]
[null,"A160733",null,"Visor acetate Junior A VL",null,null,"1 unit","","BOX",95.509090909090901,31517.999999999996]
[null,"A161014",null,"Chinguard Junior A VL",null,null,"1 unit","","EA",16.709090909090907,5513.9999999999991]
[null,"A161019",null,"Browguard Junior A VL",null,null,"1 unit","","EA",16.709090909090907,5513.9999999999991]
[null,"A160128",null,"Comfa Seal Junior A VL",null,null,"1 unit","","EA",25.036363636363632,8261.9999999999982]
[null,"A160213",null,"Headband airduct Junior A VL",null,null,"1 unit","","EA",99.481818181818184,32829]
[null,"A160219",null,"PU Cape- Junior A",null,null,"1 unit ",null,"EA",30.390909090909091,10029]
[null,"A160251",null,"Disposable Hoods  for Junior A",null,null,"1 box",null,"BOX",21.009090909090908,6933]
[null,"JUNIOR B, JUNIOR B COMBI "]
[null,"A114400",null,"Junior B VL PU","EN 12941",null,"1 unit","EA","EA",208.10909090909087,68675.999999999985]
[null,"A114200",null,"Junior B Combi VL PU","EN 12941",null,"1 unit","EA","EA",222.29999999999998,73359]
[null,"A114201",null,"Junior B Combi VL Neoprene","EN 12941",null,"1 unit","EA","EA",295.12727272727273,97392]
[null,"A160730",null,"Disposable visor Kolibri, Junior B, Junior B Combi",null,null,"100 units","","BOX",30.509090909090908,10068]
[null,"A160782",null,"Visor acetate Junior B and Junior B Combi",null,null,"1 unit","BOX","BOX",76.309090909090898,25181.999999999996]
[null,"A162876",null,"PU hood Junior B and Junior B Combi ",null,null,"1 unit","EA","EA",87.354545454545445,28826.999999999996]
[null,"A162879",null,"Neoprene hood Junior B and Junior B Combi ",null,null,"1 unit","EA","EA",238.05454545454546,78558]
[null,"A160216",null,"Headband airduct Junior B ",null,null,"1 unit","EA","EA",79.681818181818187,26295]
[null,"TIGERHOOD - HIGH PERFORMANCE SOLUTION FOR DEMANDING ENVIRONMENTS "]
[null,"A114725",null,"Tigerhood VL with visor 90x110 ","EN 12941",null,"1 unit","","EA",153.30909090909088,50591.999999999993]
[null,"A160741",null,"5 acetate visors",null,null,"5 units","BOX","BOX",80.345454545454544,26514]
[null,"A161472",null,"Sweatband",null,null,"10 units","BOX","BOX",8.2727272727272716,2729.9999999999995]
[null,"EUROMASKI - COMBINED WELDING AND GRINDING PROTECTION "]
[null,"A114703",null,"Euromaski VL","EN 12941",null,"1 unit","EA","EA",189.19090909090909,62433]
[null,"A161472",null,"Sweatband",null,null,"10 units","BOX","BOX",8.2727272727272716,2729.9999999999995]
[null,"A160143",null,"Comfa Seal  Euromaski",null,null,"1 unit","","EA",24.190909090909088,7982.9999999999991]
[null,"A160644",null,"Visor frame  Euromaski",null,null,"1 unit","","EA",12.581818181818182,4152]
[null,"Respiratory Protection |  SUPPLIED AIR RESPIRATORY",null,null,null,null,""]
[null,"AIRVISOR 2 - AIR-SUPPLIED RESPIRATOR KITS",null,null,null,null,""]
[null,"REPLACEMENT HEADPIECES",null,null,null,null,""]
[null,1013936,null,"DAVK-0051E Airvisor 2 headpiece only, with acetate chemical resistant visor; as supplied with DAVK-0001E and DAVK-0003E",null,null,"1 unit","EA","EA",110.39090909090909,36429]
[null,"SPARES AND ACCESSORIES",null,null,null,null,""]
[null,1001732,null,"DAF-9220/10 Disposable visor cover",null,null,"10 units","BOX","EA",2.7818181818181813,917.99999999999977]
[null,1001731,null,"DAF-9220/50 Disposable visor cover, Airvisor",null,null,"50 units","BOX","EA",1.0636363636363635,350.99999999999994]
[null,1028825,null,"Air supply tube, diffuser and connector for Airvisor 2 MV and Airvisor 2",null,null,"1 unit","EA","EA",16.327272727272724,5387.9999999999991]
[null,1028827,null,"Polycarbonate visor (impact resistant) for Airvisor 2",null,null,"1 unit","EA","EA",32.645454545454541,10772.999999999998]
[null,1028826,null,"Acetate visor with foam face skirt for AV2",null,null,"1 unit","EA","EA",26.872727272727268,8867.9999999999982]
[null,1001733,null,"DAF-9257/5 Disposable fabric balaclava for Airvisor 2 and Airvisor 2 MV",null,null,"5 units","BOX","EA",4.7272727272727275,1560]
[null,1001676,null,"DAVS-1408/5 Spare fabric head cover for Airvisor 2 and Airvisor MV",null,null,"5 units","BOX","EA",5.754545454545454,1898.9999999999998]
[null,1001716,null,"DAF-0705 Disposable chemical hood for Airvisor 2 and Airvisor 2 MV",null,null,"1 unit","EA","EA",13.445454545454544,4436.9999999999991]
[null,"AIRVISOR 2 MV - AIR-SUPPLIED RESPIRATOR KITS",null,null,null,null,""]
[null,1013938,null,"DMAK-0021E Airvisor 2 MV Spray Painting Kit complete with acetate chemical resistant visor, spraygun air hose with quick release connectors, fabric face seal cassette, two disposable visor covers, fabric balaclava, head / neck cover, storage bag, waistbelt complete (DAVW-1001E) includes integral low flow warning device, tested and certified to EN14594:2005 Class 4A",null,null,"1 unit","","EA",234.79999999999998,77484]
[null,1013939,null,"DMAK-0023E Airvisor 2 MV Chemical Kit complete with acetate chemical resistant visor, one fabric face seal cassette, two disposable visor covers, head / neck cover, storage bag, waistbelt complete (DAVW-1003E) includes integral low flow warning device, tested and certified to EN14594:2005 Class 4A",null,null,"1 unit","","EA",208.10909090909087,68675.999999999985]
[null,1013980,null,"DMAK-0024E Airvisor 2 MV Industrial Kit complete with polycarbonate impact resistant visor, fabric face seal cassette, two disposable visor covers, head / neck cover, storage bag, waistbelt complete (DAVW-1003E) includes integral low flow warning device, tested and certified to EN14594:2005 Class 4A",null,null,"1 unit","","EA",210.21818181818182,69372]
[null,1013987,null," DAWK-4011E Airvisor 2 W-Series Welding Kit complete high temperature welding shell (viewing window 90mm X 110mm), inner polycarbonate impact resistant visor, fabric face seal cassette, flame retardant head cover, two disposable visor covers, storage bag, waistbelt complete (DAVW-1003E) includes integral low flow warning device","EN14594:2005 Class 3A",null,"1 unit","","EA",312.16363636363633,103013.99999999999]
[null,1001778,null,"Disposable visor covers for Airvisor 2 MV and Turbovisor MV ",null,null,"10 units","BOX","EA",1.7909090909090908,591]
[null,1001779,null,"Disposable visor covers for Airvisor 2 MV and Turbovisor MV",null,null,"50 units","BOX","EA",1.5363636363636364,507]
[null,"Airvisor 2 MV Kits must be used with approved Blueline hoses to maintain CE certification",null,null,null,null,""]
[null,1013981,null,"DMAK-0071E Airvisor 2 MV headpiece only, with acetate chemical resistant visor; as supplied with DMAK-0021E and DMAK-0023E",null,null,"1 unit","EA","EA",115.18181818181817,38010]
[null,1013982,null,"DMAK-0072E Airvisor 2 MV headpiece only, with polycarbonate impact resistant visor, as supplied with DMAK-0024E",null,null,"1 unit","EA","EA",132.46363636363637,43713]
[null,"Respiratory Protection |  SUPPLIED AIR RESPIRATORY",null,null,null,null,""]
[null,"SPARES AND ACCESSORIES"]
[null,1028822,null,"Replacement browguard and frame for Airvisor 2 MV models",null,null,"1 unit","EA","EA",45.118181818181817,14889]
[null,1001774,null,"DTVS-1503/5 Replacement polycarbonate visor Turbovisor MV and Airvisor 2 MV",null,null,"5 units","BOX","EA",15.454545454545453,5100]
[null,1001775,null,"DTVS-1504/5 Replacement acetate visor for Turbovisor MV and Airvisor 2 MV",null,null,"1 db","BOX","EA",14.872727272727271,4907.9999999999991]
[null,1013994,null,"DTVS-1510/5 Spare fabric cassette  for Airvisor 2 MV",null,null,"5 units","BOX","EA",14.409090909090908,4755]
[null,1013987,null,"DAWK-4011E Airvisor 2 W-Series Welding Kit complete high temperature welding shell (viewing window 90mm X 110mm), inner polycarbonate impact resistant visor, fabric face seal cassette, flame retardant head cover, two disposable visor covers, storage bag, waistbelt complete (DAVW-1003E) includes integral low flow warning device, tested and certified to EN14594:2005 Class 3A",null,null,"1 unit","","EA",312.16363636363633,103013.99999999999]
[null,"SPARES AND ACCESSORIES",null,null,null,null,""]
[null,1001754,null,"DAWS-4204 Spare flame retardant head cover for do Airvisor 2 and Airvisor 2 MV",null,null,"5 units","BOX","EA",32.645454545454541,10772.999999999998]
[null,1001791,null,"DTVS-3074 Flame retardant balaclava for Airvisor 2",null,null,"1 unit","EA","EA",25.918181818181818,8553]
[null,"Airvisor 2 FV-Series Kits must be used with approved Blueline hoses to maintain CE certification",null,null,null,null,""]
[]
[null,"Respiratory Protection |  LIGHT DUTY SUPPLIED AIR BREATHING APPARATUS "]
[null,"AIRVISOR 2 WAISTBELT REGULATOR ASSEMBLIES",null,null,null,null,""]
[null,"Waistbelt complete with carbon cartridge, air flow regulator, quick release connectors and integral low flow warning device"]
[null,1013989,null,"DAVW-1001E for use with Airvisor 2 models \nDMAK-0021E and DAVK-0001E",null,null,"1 unit","EA","EA",134.38181818181818,44346]
[null,1013990,null,"DAVW-1003E for use with Airvisor 2 models \nDMAK-0023E/24E , DAVK-0003E/4E, \nDAWK-4001/11E",null,null,"1 unit","","EA",135.98181818181817,44873.999999999993]
[null,"AIRVISOR 2 WAISTBELT SPARES",null,null,null,null,""]
[null,1001725,null,"Miniature High Flow quick release socket",null,null,"1 unit","EA","EA",29.75454545454545,9818.9999999999982]
[null,1028829,null,"Regulator for Airvisor 2 and Airvisor 2 MV",null,null,"1 unit","EA","EA",45.118181818181817,14889]
[null,1001672,null,"DAVS-1404 Carbon cartridge for all waistbelts Airvisor, Airvisor 2, Airvisor MV and Airvisor 2 MV",null,null,"1 unit","EA","EA",38.4,12672]
[null,1001674,null,"DAVS-1406 Replacement waistbelt with lower half of plastic housing for Airvisor 2 and Airvisor 2 MV",null,null,"1 unit","EA","EA",30.709090909090907,10134]
[null,1028830,null,"Airvisor 2 Special High Flow quick release plug",null,null,"1 unit","EA","EA",16.327272727272724,5387.9999999999991]
[null,1028831,null,"Airvisor 2 High Flow quick release socket",null,null,"1 unit","EA","EA",22.563636363636363,7446]
[null,1001683,null,"DAVS-1418 1.2 metre spraygun air hose for Airvisor 2 and Airvisor 2 MV",null,null,"1 unit","EA","EA",48.954545454545453,16155]
[null,"Respiratory Protection |  MC 91 and  95",null,null,null,null,""]
[null,"MC95 -  FOR INTENSIVE WORK"]
[null,1762984,null,"MC 95 supplied air belt with Panoramasque full-face mask in EPDM, 10 m hose in a carrying box","EN 14594:2005",null,"1 unit","BOX","EA",528.18181818181813,174299.99999999997]
[null,1762983,null,"MC 95 supplied air belt without mask, 10 m hose in a carrying box","EN 14594:2005",null,"1 unit","BOX","EA",179.7,59300.999999999993]
[null,"MC91A - DOUBLE PROTECTION IN HIGHLY CONTAMINATED AREAS"]
[null,1762921,null,"MC91 with belt, AQR 06","EN14594:2005",null,"1 unit","EA","EA",211.18181818181816,69689.999999999985]
[null,1762920,null,"MC91 with belt, RBE 06 ","EN 14594:2005",null,"1 unit","BOX","EA",161.31818181818178,53234.999999999985]
[null,"DE4"]
[null,1763525,null,"DE 4 for 4 users RBE 06",null,null,"1 unit","EA","EA",959.90909090909099,316770]
[null,1763526,null,"DE 4 for 4 users AQR 06",null,null,"1 unit","BOX","EA",1732.7454545454543,571805.99999999988]
[null,1763504,null,"Set of maintenance filters DE 4 ( 4 users)",null,null,"1 unit","EA","EA",41.281818181818181,13623]
[null,1763538,null,"DE 4 for 4 users with CEJN outlets - Inlet RBE 11",null,null,"1 unit","BOX","EA",1176.2727272727273,388170]
[null,1763528,null,"DE4 (4 outputs) RBE11",null,null,"1 unit ","BOX","EA",637.27272727272714,210299.99999999994]
[null,"VORTEX "]
[null,"A001444",null,"Clip VORTEX",null,null,"1 unit","EA","EA",13.090909090909092,4320]
[null,"A160142",null,"Sound absorber Votrex",null,null,"1 unit","EA","EA",17.272727272727273,5700]
[null,"A150275",null,"VORTEX Air Conditioner",null,null,"1 unit","EA","EA",144.95454545454544,47834.999999999993]
[null,"BLUELINE AIR HOSE",null,null,null,null,""]
[null,1001726,null,"DAF-7319 BLUELINE air hose 3.5 meters for Airvisor 2",null,null,"1 unit","EA","EA",48.954545454545453,16155]
[null,1001727,null,"DAF-7351 BLUELINE air hose 7.5 meters for Airvisor 2",null,null,"1 unit","EA","EA",56.645454545454548,18693]
[null,1004716,null,"DAF-7350 BLUELINE air hose 10 meters for Airvisor 2",null,null,"1 unit","EA","EA",71.990909090909085,23756.999999999996]
[null,1001729,null,"30 M BLUELINE AIR HOSE for Clearflow 3",null,null,"1 unit","EA","EA",96.363636363636346,31799.999999999993]
[null,1001730,null,"20 m BLUELINE AIR HOSE for Clearflow 3",null,null,"1 unit","EA","EA",87.272727272727266,28799.999999999996]
[null,1001728,null,"15 M BLUELINE AIR HOSE for Clearflow 3",null,null,"1 unit","EA","EA",75.454545454545453,24900]
[]
[null,"Respiratory Protection |  LIGHT DUTY SUPPLIED AIR BREATHING APPARATUS "]
[null,"CLEARFLOW 3 FILTER SYSTEMS",null,null,null,null,""]
[null,"Clearflow 3 compressed air filter range has been developed to deliver  high quality breathable air to a range of supplied air respirator systems.",null,null,null,null,""]
[null," of supplied air respirator systems.Air is taken from the factory compressed air system",null,null,null,null,""]
[null,"The carbon adsorber  filter removes oil vapour and odour as necessary. ",null,null,null,null,""]
[null,"Standard Filter Systems",null,null,null,null,""]
[null,1763903,null,"Clearflow 3 wall-mounted Combination system, 2 CEJN outlets",null,null,"1 unit","EA","EA",520.26363636363624,171686.99999999997]
[null,1763904,null,"Clearflow 3 stand mounted Combination system, 2 CEJN outlets",null,null,"1 unit","","EA",766.19999999999993,252845.99999999997]
[null,1763905,null,"Clearflow 3, filtration unit, three elements, wall-mounted, two RBE 06 connections",null,null,"1 unit","","EA",605.39090909090896,199778.99999999997]
[null,1763906,null,"Clearflow 3, filtration unit, three elements, portable, two RBE 06 connections",null,null,"1 unit","","EA",841.88181818181818,277821]
[null,1763909,null,"Clearflow 3 filtration unit, three elements, wall mounted, two seamless outputs *Supplied without quick coupler",null,null,"1 unit","","EA",482.41818181818172,159197.99999999997]
[null,1763910,null,"Clearflow 3, filtration unit, three elements, portable, two connectionless outputs\n*Supplied without quick coupler",null,null,"1 unit","","EA",718.90909090909076,237239.99999999994]
[null,1763911,null,"Clearflow 3 wall-mounted with 2 double action outlets",null,null,"1 unit","","EA",668.77272727272725,220695]
[null,1763912,null,"Clearflow 3 on portable stand with 2 double action outlets",null,null,"1 unit","","EA",927.0181818181818,305916]
[null,"Spares and Accessories ",null,null,null,null,""]
[null,1763908,null,"Coalescing filter element for Clearflow 3",null,null,"1 unit","","EA",53.636363636363633,17700]
[null,1763907,null,"Adsorber filter element for Clearflow 3",null,null,"1 unit","","EA",56.363636363636353,18599.999999999996]
[null,"Spare filters for Clearflow 2 filter system",null,null,null,null,""]
[null,1016971,null,"DCFS-2163 Coalescing filter element Clearflow 2",null,null,"1 unit","EA","EA",33.609090909090902,11090.999999999998]
[null,"Accessories & Spare parts ",null,null,null,null,"1 unit"]
[null,1001707,null,"Pressure gauge for Clearflow 3",null,null,"1 unit","","EA",31.736363636363631,10472.999999999998]
[null,1001722,null,"Quick release outlet socket (CEJN for use with Airvisor) for Clearflow 3",null,null,"1 unit","EA","EA",30.709090909090907,10134]
[null,1763341,null,"Isolating valve for Clearflow 3",null,null,"1 unit","EA","EA",11.527272727272726,3803.9999999999995]
[null,1763921,null,"Differential Pressure Indicator (available as a service/repair kit) for Clearflow 3",null,null,"1 unit",null,"EA",34.090909090909086,11249.999999999998]
[null,1763420,null,"Quick release outlet socket (RBE6) for Clearflow 3",null,null,"1 unit","","EA",74.545454545454533,24599.999999999996]
[null,1763422,null,"Quick release outlet socket (AQR 06) for Clearflow 3",null,null,"1 unit","","EA",256.36363636363632,84599.999999999985]
[null,1763920,null,"Quick release outlet socket (double-action for use with Airvisor 2 DHC) for Clearflow 3",null,null,"1 unit","","EA",134.54545454545453,44399.999999999993]
[null,1763928,null,"Replacement coalescing filter stage (complete, supplied with inlet adaptor) for Clearflow 3",null,null,"1 unit","","EA",244.54545454545453,80700]
[null,1763916,null,"Replacement absorber filter stage for Clearflow 3",null,null,"1 unit","","EA",159.99999999999997,52799.999999999993]
[null,1763335,null,"Doubling kit RBE (‘Y’ piece + one RBE 06 connector) for Clearflow 3",null,null,"1 unit","","EA",103.63636363636361,34199.999999999993]
[null,1763333,null,"Doubling kit AQR (‘Y’ piece + one AQR 06 connector) for Clearflow 3",null,null,"1 unit","","EA",157.27272727272725,51899.999999999993]
[null,1763923,null,"Wall mounting bracket for regulator for Clearflow 3",null,null,"1 unit",null,"EA",42.727272727272727,14100]
[null,1763922,null,"Ring for regulator mounting bracket for Clearflow 3",null,null,"1 unit",null,"EA",30,9900]
[null,1763926,null,"Body connector (with 2 O-ring gaskets) for Clearflow 3",null,null,"1 unit",null,"EA",24.545454545454543,8099.9999999999991]
[null,1763925,null," Body connector with wall support (with 2 O-ring gaskets) for Clearflow 3",null,null,"1 unit",null,"EA",34.545454545454547,11400]
[null,1763924,null,"5 O-ring gaskets for Clearflow 3",null,null,"1 unit",null,"EA",11.818181818181817,3899.9999999999995]
[null,1763914,null,"Regulator (complete, but without gauge) for Clearflow 3",null,null,"1 unit",null,"EA",130.90909090909088,43199.999999999993]
[null,1763927,null,"Filter element cover (with manual drain) for Clearflow 3",null,null,"1 unit",null,"EA",49.090909090909086,16199.999999999998]
[null,"Respiratory Protection | Commander ",null,null,null,null,""]
[null,"COMMANDER"]
[null,"A133130-00",null,"Commander Leather cape",null,null,"1 unit","EA","EA",298.22727272727275,98415]
[null,"A133230-00",null,"Commander Bisonyl cape",null,null,"1 unit","EA","EA",223.67272727272726,73812]
[null,"A133730-00",null,"Comannder Cotton jack cape",null,null,"1 unit",null,"EA",275.94545454545454,91062]
[null,"A160123",null,"Mesh screen Commander",null,null,"50 units ","BOX ","BOX ",66.236363636363635,21858]
[null,"A160761-25",null,"Glass screen Commander",null,null,"25 units ","BOX","BOX",18.245454545454546,6021]
[null,"A160722",null,"Polyester screen Commander ",null,null,"50 units ","BOX ","BOX",63.354545454545452,20907]
[null,"A001979",null,"Window Commander",null,null,"1 unit","EA","EA",10.172727272727272,3356.9999999999995]
[null,"A160662",null,"Visor gasket Commander",null,null,"1 unit","EA","EA",8.836363636363636,2916]
[null,"A160472",null,"Regulator, silencer Commander",null,null,"1 unit","EA","EA",33.609090909090902,11090.999999999998]
[null,"A160210",null,"Airduct for Commander",null,null,"1 unit","EA","EA",12.49090909090909,4122]
[null,"A133135-00",null,"COMMANDER WITH LEATHER CAPE AND VORTEX",null,null,"1 unit","EA","EA",361.62727272727273,119337]
[null,"A133235-00",null,"COMMANDER WITH BISONYL CAPE AND VORTEX",null,null,"1 unit","EA","EA",261.81818181818176,86399.999999999985]
[null,"A133735-00",null,"COMMANDER WITH COTTON CAPE AND VORTEX",null,null,"1 unit","EA","EA",278.37272727272722,91862.999999999985]
[null,"A001976",null,"Hose adapter for Commander",null,null,"1 unit","EA","EA",9.745454545454546,3216]
[null,"A160695",null,"WAISTBELT for Commander",null,null,"1 unit","EA","EA",9.1181818181818173,3008.9999999999995]
[null,"A000233",null,"JACKET LEATHER WITHOUT NECK SEAL for Commander",null,null,"1 unit","EA","EA",336.32727272727266,110987.99999999997]
[null,"A160664",null,"VISOR REPAIR SET for Commander",null,null,"1 unit","EA","EA",21.099999999999998,6962.9999999999991]
[null,"A002550",null,"JACKET COTTON WITHOUT NECK SEAL for Commander",null,null,"1 unit","EA","EA",54.72727272727272,18059.999999999996]
[null,"A161292",null,"HOSE ASSEMBLY for Commander",null,null,"1 unit","EA","EA",26.927272727272722,8885.9999999999982]
[null,"A160146",null,"SILENCER for Commander",null,null,"1 unit","BOX","BOX",41.590909090909086,13724.999999999998]
[null,"A002505",null,"HOSE REGULATOR BAYONET CONNECTOR for Commander",null,null,"1 unit","EA","EA",65.172727272727258,21506.999999999996]
[null,"A160743",null,"VISOR ACETATE - 10 PCS for Commander",null,null,"10 units","BOX","BOX",113.81818181818181,37560]
[null,"A160482",null,"AIRFLOW INDICATOR for Commander",null,null,"1 unit","EA","EA",28.763636363636358,9491.9999999999982]
[null,"A002495",null,"CAPE LEATHER INCLUDING NECK SEAL for Commander",null,null,"1 unit","EA","EA",258.74545454545449,85385.999999999985]
[null,"A160621",null,"TOP PLATE PVC for Commander",null,null,"1 unit","EA","EA",18.863636363636363,6225]
[]
[null,"Respiratory Protection |  Spare parts for half & full face masks",null,null,null,null,""]
[null,"SPARE PARTS 5400 "]
[null,202820,null,"RX12 FFMTT Full face mask corrective lenses for 5400",null,null,"1 unit","EA","EA",18.454545454545453,6090]
[null,"N0655402",null,"Face Seal L 5400 Twin",null,null,"1 unit","EA","EA",18.109090909090909,5976]
[null,"N0655406",null,"Inner Mask 5400",null,null,"1 unit","EA","EA",3.1454545454545455,1038]
[null,"N06577017",null,"Inhalation Valve for 5400 Twin",null,null,"1 unit","BOX","BOX",3.1909090909090905,1052.9999999999998]
[null,"N06580776",null,"Face Seal 5400 Mono",null,null,"1 unit","EA","EA",25.454545454545453,8400]
[null,"N06589928",null,"INLET HOUSING NUT",null,null,"1 unit","EA","EA",30.45454545454545,10049.999999999998]
[null,"N06580814",null,"INHALATION VALVE SEAT 80814",null,null,"1 unit","BOX","BOX",1.3909090909090907,458.99999999999989]
[null,"N06580871",null,"INHALATION GROMMETS 80871",null,null,"1 unit","BOX","BOX",4.545454545454545,1499.9999999999998]
[null,"N0655403",null,"GASKET, 5 PACK 5400 SERIES",null,null,"1 unit","BOX","BOX",6.3181818181818175,2084.9999999999995]
[null,"N06580844",null,"LENS CLAMPS NUTS PK2 80844",null,null,"1 unit","BOX","BOX",1.718181818181818,567]
[null,"N0655406",null,"INNER MASK 5400",null,null,"1 unit","EA","EA",3.1454545454545455,1038]
[null,"N06577017",null,"INHALATION VALVE",null,null,"1 unit","BOX","BOX",3.1909090909090905,1052.9999999999998]
[null,"N0655407",null,"EXHALATION HOUSING 5400 SERIES",null,null,"1 unit","EA","EA",2.8454545454545452,938.99999999999989]
[null,"N06580843",null,"LENS CLAMPS SCREWS PK2 80843",null,null,"1 unit","BOX","BOX",4.7363636363636363,1563]
[null,"N06580757",null,"HEAD STRAP ASSY 54101",null,null,"1 unit","EA","EA",14.463636363636361,4772.9999999999991]
[null,"N80836A",null,"DISPOSABLE VISORS",null,null,"1 unit","BAG","BAG",15.363636363636362,5069.9999999999991]
[null,"N0655408",null,"EXHALATION HOUSING COVER(5400)",null,null,"1 unit","EA","EA",2.8181818181818179,929.99999999999989]
[null,"N0655402",null,"FACE SEAL 5400 SERIES -54101",null,null,"1 unit","EA","EA",18.109090909090909,5976]
[null,"N06577016",null,"EXHALATION ASSEMBLY",null,null,"1 unit","BOX","BOX",4.4818181818181815,1479]
[null,"N06580798",null,"LENS CLAMPS UPPER/LOWER 80798",null,null,"1 unit","EA","EA",15.909090909090908,5250]
[null,"N06577018",null,"EXHALATION VALVES, 4PK 77018",null,null,"1 unit","BOX","BOX",11.527272727272726,3803.9999999999995]
[null,"N06589957",null,"O'RING 89957 (PK OF 5 PIECES)",null,null,"1 unit","BOX","BOX",36.36363636363636,11999.999999999998]
[null,"N06580773",null,"40 MM CONNECTOR ASSY",null,null,"1 unit","EA","EA",6.2454545454545451,2061]
[null,"N06554015",null,"LENS 5400 SERIES, 54101 CLASS1",null,null,"1 unit","EA","EA",21.118181818181817,6969]
[null,"N06580759",null,"CONNECTOR SEAL 5400 SERIES",null,null,"1 unit","EA","EA",7.4454545454545444,2456.9999999999995]
[null,"N06580756",null,"HEAD STRAP ASSY 54301",null,null,"1 unit","EA","EA",25.990909090909089,8577]
[null,"N06580758",null,"LENS 54201/54301 CLASS 2 (5400)",null,null,"1 unit","EA","EA",30.990909090909092,10227]
[null,"N06580757",null,"HEAD STRAP ASSY 54201",null,null,"1 unit","EA","EA",14.463636363636361,4772.9999999999991]
[null,"N0655402",null,"FACE SEAL 5400 SERIES -54201",null,null,"1 unit","EA","EA",18.109090909090909,5976]
[]
[null,"SPARE PARTS 5500 "]
[null,"550011M",null,"Facepiece REPL 5500 SERIES medium ",null,null,null,null,"EA",6.209090909090909,2049]
[null,"N06577092",null,"Cradle suspension  for 7700 and 5500",null,null,"1 unit","EA","EA",6.3636363636363633,2100]
[null,"N06577020",null,"N5500 EXHAL VLV/GUARD PK1",null,null,"EA","EA","EA",0.78181818181818186,258]
[null,"N06577019",null,"N5500 EXHAL VLV SEATS PK2",null,null,"BOX","BOX","BOX",0.74545454545454537,245.99999999999997]
[null,"N06577092",null,"N7700-92U CRDL SUSPENS'N HARNESS",null,null,"EA","EA","EA",6.3636363636363633,2100]
[]
[null,"SPARE PARTS 7700"]
[null,"N06577011",null,"7700-11M BASIC FACEPIECE",null,null,"1 unit","EA","EA",9.4363636363636374,3114.0000000000005]
[null,"N06577017",null,"N7700-17U inhalation VLVS PK 6",null,null,"1 unit","BOX","BOX",3.1909090909090905,1052.9999999999998]
[null,"N06577016",null,"Filter connector PK2",null,null,"1 unit","BOX","BOX",4.4818181818181815,1479]
[null,"N06577019",null,"N7700-19U EXHAL VLV SEATS PK2",null,null,"1 unit","BOX","BOX",0.74545454545454537,245.99999999999997]
[null,"N06577020",null,"N7700-20U EXHAL VLV/GUARD PK1",null,null,"1 unit","EA","EA",0.78181818181818186,258]
[]
[null,"SPARE PARTS OPTI -FIT "]
[null,1715053,null,"Lower half-collar, black, Opti-fit Mono",null,null,"10 units","EA","EA",9.918181818181818,3273]
[null,1715060,null,"Open rectangle 10,2x20x2,3  Opti-fit Mono",null,null,"1 unit","EA","EA",0.48181818181818181,159]
[null,1715051,null,"O-ring for Opti-fit   ",null,null,"1 unit","EA","EA",5.2818181818181813,1742.9999999999998]
[null,1715052,null,"Upper half-collar, black, Optti-fit",null,null,"1 unit","EA","EA",9.463636363636363,3123]
[null,1715057,null,"Lower buckle support Opti-fit  ",null,null,"1 unit","EA","EA",1.4454545454545453,476.99999999999994]
[null,1715058,null,"Upper buckle support Opti-fit  ",null,null,"1 unit","EA","EA",0.96363636363636362,318]
[null,1715059,null,"Buckle Opti-fit  ",null,null,"1 unit","EA","EA",1.7818181818181817,588]
[null,1715061,null,"Base connection Opti-fit RD4x1,7\"",null,null,"1 unit","EA","EA",4.9363636363636356,1628.9999999999998]
[null,1715067,null,"Srew for ocular collar Opti-fit",null,null,"1 unit","EA","EA",0.38181818181818178,125.99999999999999]
[null,1715120,null,"Opti-fit Twin connector",null,null,"1 unit","EA","EA",7.6727272727272711,2531.9999999999995]
[null,1715123,null,"Flat seal for filter holder - T-SERIES only, Opti-fit Twin",null,null,"1 unit","EA","EA",3.6545454545454534,1205.9999999999995]
[null,1715124,null,"Filter holder T-SERIES, Opti-fit Twin",null,null,"1 unit","EA","EA",8.6363636363636367,2850]
[null,1705207,null,"Valve holder seal connector rd 4x 1/7\", Opti-fit",null,null,"1 unit","EA","EA",4.0727272727272732,1344.0000000000002]
[]
[null,"SPARE PARTS PREMIER & VALUAIR "]
[null,1001611,null,"Headband assembly Premier",null,null,"10 units","BOX","EA",11.327272727272726,3737.9999999999995]
[null,1001612,null,"Exhale valve Valuair, Premier",null,null,"10 units","BOX","EA",5.1818181818181817,1710]
[null,1001613,null,"Inhale valve Valuair, Premier",null,null,"10 units","BOX","EA",1.5363636363636364,507]
[null,1001622,null,"Filtr connector Valuair, Premier",null,null,"10 units","BOX","EA",1.3181818181818181,435]
[null,1001624,null,"Head assembly Valuair Plus",null,null,"10 units","BOX","EA",4.7454545454545451,1566]
[null,1727030,null,"Inhalation valve diam. 33 -d3x,4 Valuair, Premier",null,null,"1 unit","EA","EA",0.48181818181818181,159]
[]
[null,"SPARE PARTS PANORAMASQUE "]
[null,1705205,null,"Phonic device diameter 54 stainless steel, Pano",null,null,"1 unit","EA","EA",16.327272727272724,5387.9999999999991]
[null,1702248,null,"Tightening collar for Panoramasque",null,null,"10 units","EA","EA",1.9181818181818178,632.99999999999989]
[null,1701040,null,"Silicon exhalation valve < 94, Pano",null,null,"1 unit","EA","EA",4.045454545454545,1334.9999999999998]
[null,1701381,null,"Key nut of valve box 94 s.t.r.§ packaging screw l > 94, Pano",null,null,"1 unit","EA","EA",90.22727272727272,29774.999999999996]
[null,1701384,null,"Key for top of speech diaphragm 94, Pano",null,null,"1 unit","EA","EA",90.22727272727272,29774.999999999996]
[null,1701417,null,"Nut tr 36 x 1,5 for valve box and speech diaphragm 94 > 94, Pano",null,null,"1 unit","EA","EA",3.6545454545454534,1205.9999999999995]
[null,1702000,null,"Complete mask connector 0h RD40, Pano",null,null,"1 unit","EA","EA",6.2454545454545451,2061]
[null,1705211,null,"O'ring seal 5,52 x 1,78, Pano",null,null,"1 unit","EA","EA",3.6545454545454534,1205.9999999999995]
[null,1710050,null,"Rectangle with roll in stainless steel 25 x 11,3, Pano",null,null,"1 unit","EA","EA",0.67272727272727273,222]
[null,1710081,null,"Pano lenses chlorine c",null,null,"1 unit","EA","EA",36.909090909090907,12180]
[null,1710085,null,"Pano lenses triplex",null,null,"1 unit","","EA",77.936363636363637,25719]
[null,1710086,null,"Pano lenses pc cl2/p",null,null,"1 unit","EA","EA",25.918181818181818,8553]
[null,1710096,null,"Black lenses collar Pano with screw",null,null,"1 unit","EA","EA",21.118181818181817,6969]
[null,1710102,null,"Screw and nut 2,5 thickness for half collar, Pano",null,null,"1 unit","EA","EA",1.3363636363636364,441]
[null,1710115,null,"Inner mask na with 2 holes d27 EPDM > 94, Pano",null,null,"1 unit","EA","EA",25.918181818181818,8553]
[null,1710117,null,"Inner mask na with 2 holes d27 SI, Pano",null,null,"1 unit","EA","EA",19.2,6336]
[null,1710256,null,"Sctratchproof PC lens Pano (marked CL3) ",null,null,"1 unit","EA","EA",13.918181818181818,4593]
[null,1710317,null,"Neck cotton strap with open d-rings, Pano",null,null,"1 unit","EA","EA",3.7454545454545451,1236]
[null,1710323,null,"Full support mesh Pano",null,null,"1 unit","EA","EA",85.918181818181822,28353]
[null,1779502,null,"Pliers for mask connection collar Pano",null,null,"1 unit","","EA",116.08181818181816,38306.999999999993]
[null,1710022,null,"Complete harness for Panoramasque",null,null,"1 unit",null,"EA",21.763636363636365,7182.0000000000009]
[null,1710083,null,"Visor Pano PMMA marked cl2/m",null,null,"1 unit","EA","EA",20.627272727272729,6807.0000000000009]
[null,1710120,null,"Inhalation valve for inner mask Pano",null,null,"1 unit","EA","EA",1.6818181818181819,555]
[]
[null,"OTHER "]
[null,1001572,null,"Headband assembly for MX/PF",null,null,"5 units","BOX","EA",19.172727272727272,6327]
[null,1001571,null,"Exhalation valve for MX/PF 950",null,null,"5 units","BOX","EA",7.7818181818181813,2568]
[null,1001618,null,"Adaptor for MX/PF 950",null,null,"2 units","BOX","EA",3.5999999999999996,1187.9999999999998]
[null,1712030,null,"Stop rectangle stop pp stainless for FF mask",null,null,"1 unit","EA","EA",0.1818181818181818,59.999999999999993]
[null,1712470,null,"Varnished rectangle for fixed head strap for FF mask",null,null,"1 unit","EA","EA",0.6272727272727272,206.99999999999997]
[null,1772010,null,"Carrying bag with zip for FF mask",null,null,"1 unit","","EA",59.518181818181809,19640.999999999996]
[null,1772040,null,"Carrying bag with velcro for FF mask",null,null,"1 unit","","EA",43.199999999999996,14255.999999999998]
[null,1772200,null,"Waterproof cloth case for FF mask",null,null,"1 unit","","EA",36.481818181818177,12038.999999999998]
[null,1772500,null,"Plastic moulded container for masks",null,null,"1 unit","","EA",47.036363636363632,15521.999999999998]
[null,"N65007712",null,"Carry bag half face mask 77BAG ",null,null,null,null,"EA",18.145454545454545,5988]
[null,"N65007612",null,"Carry bag for full face mask 76BAG",null,null,null,"EA","EA",20.909090909090907,6899.9999999999991]
[null,"N65007910",null,"Carry bag for filters 79BAG ",null,null,null,null,"EA",17.563636363636363,5796]
[null,"N06577011",null,"7700-11M Basic face piece ",null,null,"1 unit","EA","EA",9.4363636363636374,3114.0000000000005]
[]
[null,"SPARES FOR OPTIFIT FULL FACE RESPIRATORS",null,null,null,null,""]
[null,1715050,"S01/T02","Face-seal Opti-fit - size S ",null,null,"1 unit","EA","EA",45.118181818181817,14889]
[null,1715065,"S01/T02","Face-seal Opti-fit - size M ",null,null,"1 unit","EA","EA",47.990909090909085,15836.999999999998]
[null,1715066,"S01/T02","Face-seal Opti-fit - size L",null,null,"1 unit","EA","EA",38.4,12672]
[null,1715070,"S06/T21","Valve for inner mask Opti-fit",null,null,"1 unit","EA","EA",1.9181818181818178,632.99999999999989]
[null,1715069,"S07/T14","Valve seat for inner mask Opti-fit",null,null,"1 unit","EA","EA",3.8363636363636355,1265.9999999999998]
[null,1715056,"S08/T01","5-points head-harness Opti-fit Twin",null,null,"1 unit","EA","EA",8.4454545454545435,2786.9999999999995]
[null,1715062,"S16/T10","Exhalation valve Opti-fit ",null,null,"1 unit","EA","EA",9.1181818181818173,3008.9999999999995]
[null,1715054,"S18/T15","Inner mask Opti-fit",null,null,"1 unit","EA","EA",19.2,6336]
[null,"OPTIFIT SINGLE SPARES",null,null,null,null,""]
[null,1710713,"S02","Visor for Opti-fit Mono",null,null,"1 unit","EA","EA",31.690909090909091,10458]
[null,1702150,"S15","Inhalation valve membrane for Opti-fit",null,null,"1 unit","EA","EA",0.67272727272727273,222]
[null,"OPTIFIT TWIN SPARES",null,null,null,null,"1 unit"]
[null,1715121,"T03","Visor Opti-fit Twin",null,null,"1 unit","EA","EA",31.690909090909091,10458]
[null,"AIRVISOR SPARES (PRE-AIRVISOR 2)",null,null,null,null,"1 unit"]
[null,"** NOT FOR USE WITH AIRVISOR 2 KITS **",null,null,null,null,"1 unit"]
[null,1001653,null,"DMAK-0071 Airvisor MV head-piece only with acetate chemical resistant visor; as supplied with DMAK-0021 and DMAK-0023",null,null,"1 unit","EA","EA",95.999999999999986,31679.999999999996]
[null,1001654,null,"Hood with polycarbonate visor for Airvisor MV",null,null,"1 unit","EA","EA",100.79999999999998,33263.999999999993]
[null,1001781,null,"DTVS-1510/5 Spare fabric cassette Turbovisor MV",null,null,"5 units","BOX","BOX",12.954545454545451,4274.9999999999991]
[]
[null,"TURBOVISOR MV",null,null,null,null,""]
[null,null,null,"Turbovisor MV kit with polycarbonate visor (EN166 39-B), main filter, two disposable visor covers, battery pack, battery "]
[null,null,null,"charger unit, cotton head cover, air flow test disc and fabric carrying bag. For use in general industrial operations, e.g"]
[null,null,null,"woodworking, handling of dusts, grinding and polishing of metals, plastics etc. Also for use in the pharmaceutical and similar industries."]
[null,null,null,null,null,null,""]
[null,"Spares and accessories",null,null,null,null,""]
[null,1001772,null,"DTVS-1501 Replacement browguard and moulded frame for 8 hour model Turbovisor MV",null,null,"1 unit","EA","EA",55.68181818181818,18375]
[null,1001773,null,"DTVS-1502 Replacement browguard and moulded frame for 6 hour model Turbovisor MV",null,null,"1 unit","EA","EA",55.68181818181818,18375]
[null,1001776,null,"DTVS-1505 Replacement 6 hour power unit without filter for Turbovisor MV",null,null,"1 unit","EA","EA",211.18181818181816,69689.999999999985]
[null,1001777,null,"DTVS-1506 Replacement 8 hour power unit without filter for Turbovisor MV",null,null,"1 unit","EA","EA",220.77272727272722,72854.999999999985]
[null,1001797,null,"DTVS-3170 Pre-filters Turbovisor MV",null,null,"10 units","BOX","EA",0.63636363636363635,210]
[null,1001793,null,"DTVR-TH2-2 Main particulate filter Turbovisor MV",null,null,"2 units","BOX","EA",13.727272727272725,4529.9999999999991]
[null,1001794,null,"DTVR-TH2-C Main particulate filter with odour removal Turbovisor MV",null,null,"10 units","BOX","EA",18.481818181818181,6099]
[null,1001782,null,"DTVS-1511 Replacement 6 hour head mounted battery pack Turbovisor MV",null,null,"1 unit","EA","EA",142.07272727272726,46884]
[null,1001792,null,"DTVR-BP2 Replacement 8 hour waist mounted battery pack",null,null,"1 unit","EA","EA",172.78181818181818,57018]
[null,1001790,null,"DTVS-3072/5 Spare cotton head cover Turbovisor MV",null,null,"5 units","BOX","EA",13.445454545454544,4436.9999999999991]
[null,1001787,null,"TURBOVISOR EURO 8HR ( WITH FOAM FACESEAL)",null,null,"1 unit","EA","EA",336.42727272727274,111021]
[null,1001788,null,"DTVR-V1 Polycarbonate visor (EN166 39-B) with foam face seal for all models Turbovisor MV",null,null,"1 unit","EA","EA",30.709090909090907,10134]

{"sheet":"Hand Protection","index":5,"n_rows":528,"n_cols":11,"rows_kept":528,"cut":false,"hidden":false,"merged":[[46,1,46,8]]}
[null,"Hand Protection |  NEW PRODUCT INTRODUCTION ",null,null,null,null,""]
[null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per","NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,"NEW!!! Black Dyneema® Diamond, a black diamond on your hands!"]
[null,"A high performed cut protective glove for handling sharp objects in oily environments"]
[null,"Highly protective cut resistance gloves level B and level D available in 2 types of Nitrile coating: palm coated sandy finished and 3/4 dipped nitrile foam, 2 gauges levels, suitable for work in wet or oily environment. Gauge 13 gloves provides"]
[null,"superb cut resistant protection, while gauge 18 brings outstanding comfort without giving away cut protection."]
[null,2332472,null,"NEW!!! Diamond Black Comfort 3/4 C&G D Black knitted lightweight Dyneema® Diamond\nwith 3/4 foam nitrile coating, gauge 13","EN388:2016 4X42D","7 to 11","10 PR","CAS","PR",10.872727272727271,3587.9999999999995]
[null,2332478,null,"NEW!!! Diamond Black Skin 3/4 C&G B Black knitted lightweight Dyneema® Diamond\nwith 3/4 foam nitrile coating, gauge 18","EN388:2016 4X42B","7 to 11","10 PR","CAS","PR",8.7854545454545452,2899.2]
[null,2332372,null,"NEW!!! Diamond Black Comfort C&G D Black knitted lightweight Dyneema® Diamond\nwith sandy finish nitrile coating, gauge 13","EN388:2016 4X42D","7 to 11","10 PR","CAS","PR",10.458181818181817,3451.2]
[null,2332378,null,"NEW!!! Diamond Black Skin C&G B Black knitted lightweight Dyneema® Diamond\nwith sandy finish nitrile coating, gauge 18","EN388:2016 4X42B","7 to 11","10 PR","CAS","PR",8.1963636363636354,2704.7999999999997]
[null,"VERTIGO - Knitted Spectra® gloves. Cut resistant (Level 3 & 5 to EN 388). PU or nitrile coating. High precision work."]
[null,"COMFORT"]
[null,"The Vertigo® line features seamless and lightweight polyamide (cut 1) Spectra® (cut B) and Spectra® + glass fiber (cut C) liners with PU or nitrile coating."]
[null,"RESISTANCE & SAFETY"]
[null,"The Spectra® and polyamide thread provides outstanding properties against cuts.The polyurethane/nitrile coating at the palm and fingertips provides outstanding abrasion resistance."]
[null,"The tight knit gives the gloves perfect support, limits the penetration of dirt and offers a good touch.The ventilated back optimise their breathability. The cool Spectra® touch gives an added sensation of comfort."]
[]
[null,2318778,null,"NEW!!! Vertigo Liner C&G C. Knitted glove in Spectra®/Polyamide for dry applications, Check&Go concept.\n","EN 420                         EN 388-2016 : 3X4XC","7 to 11","10 PR","CAS","PR",4.7781818181818183,1576.8]
[null,2318767,null,"NEW!!! Vertigo GREY PU C&G B. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Lycra. Grey PU coating on palm, Check&Go\n","EN 420                         EN 388-2016 : 4X42B","7 to 11","10 PR","CAS","PR",4.2618181818181817,1406.3999999999999]
[null,"2318767/VMP",null,"NEW!!! Vertigo GREY PU C&G B. Vending machine packaging. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Lycra. Grey PU coating on palm, Check&Go, Size 6,7,11 - 50 pairs per box, Size 8,9,10 - 100 pairs per box\n","EN 420                         EN 388-2016 : 4X42B","7 to 11",null,null,"PR",4.378181818181818,1444.8]
[null,2318768,null,"NEW!!! Vertigo GREY PU C&G C. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Polyamide. Grey PU coating on palm, Check&Go\n","EN 420                         EN 388-2016 : 4X42C","7 to 11","10 PR","CAS","PR",4.9454545454545453,1632]
[null,"2318768/VMP",null,"NEW!!! Vertigo GREY PU C&G C. Vending machine packaging. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Polyamide. Grey PU coating on palm, Check&Go, Size 6,7,11 - 50 pairs per box, Size 8,9,10 - 100 pairs per box\n","EN 420                         EN 388-2016 : 4X42C","7 to 11",null,null,"PR",5.0690909090909084,1672.7999999999997]
[null,2318769,null,"NEW!!! Vertigo White PU C&G B. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Lycra. White PU coating on palm, Check&Go\n","EN 420                         EN 388-2016 : 4X42B","7 to 11","10 PR","CAS","PR",4.2618181818181817,1406.3999999999999]
[null,2318770,null,"NEW!!! Vertigo GREY PU LONG C&G B. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Lycra. Grey PU coating on palm, Check&Go, Wrist 11cm\n","EN 420                         EN 388-2016 : 4X42B","7 to 11","10 PR","CAS","PR",4.6036363636363626,1519.1999999999996]
[null,2318771,null,"NEW!!! Vertigo GREY PU LONG C&G C. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Lycra/out side glass fibre. Grey PU coating on palm, Check&Go, Wrist 11cm\n","EN 420                         EN 388-2016 : 4X42C","7 to 11","10 PR","CAS","PR",5.0763636363636362,1675.2]
[null,2318765,null,"NEW!!! Vertigo GREY First PU C&G B. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Lycra. Grey PU coating on palm, Check&Go, composite wrist\n","EN 420                         EN 388-2016 : 4X42B","7 to 11","10 PR","CAS","PR",4.0872727272727269,1348.8]
[null,2318766,null,"NEW!!! Vertigo GREY First NIT C&G B. Heavy objects handling with high cut risks in dry or  slightly greasy environment.Knitted glove in Spectra®/Lycra. Grey nitrile coating on palm, Check&Go, composite wrist\n","EN 420                         EN 388-2016 : 4X42B","7 to 11","10 PR","CAS","PR",4.2618181818181817,1406.3999999999999]
[null,2132251,null,"NEW!!! Vertigo BLACK PU C&G A. Knitted extremely lightweight black polyamide, black polyurethane coating. Check&Go\n","EN 420                         EN 388 : 4131A","7 to 11","10 PR","CAS","PR",0.84363636363636352,278.39999999999998]
[null,2232270,null,"NEW!!! Vertigo BLACK NIT C&G 1. Knitted extremely lightweight black polyamide, black nitrile coating. Check&Go\n","EN 420                         EN 388 : 4121X","7 to 11","10 PR","CAS","PR",1.9563636363636361,645.59999999999991]
[null,2342242,null,"NEW!!! Vertigo BLACK PU C&G B. Knitted lightweight black polyamide/Spectra/Elastan, black polyurethane coating. Check&Go\n","EN 420                         EN 388-2016 : 4X42B","7 to 11","10 PR","CAS","PR",4.4290909090909087,1461.6]
[null,2342552,null,"NEW!!! Vertigo BLACK NIT C&G B. Knitted lightweight black polyamide/Spectra/Elastan, black nitrile coating. Check&Go\n","EN 420                         EN 388-2016 : 4X43B","7 to 11","10 PR","CAS","PR",4.7709090909090897,1574.3999999999996]
[null,2342545,null,"NEW!!! Vertigo BLACK PU C&G C. Knitted lightweight black polyamide/Spectra/Elastan/ outside glass fiber, black polyurethane coating. Check&Go\n","EN 420                         EN 388-2016 : 4X43C","7 to 11","10 PR","CAS","PR",4.9454545454545453,1632]
[null,2342555,null,"NEW!!! Vertigo BLACK NIT C&G C. Knitted lightweight black polyamide/Spectra/Elastan/ outside glass fibre, black nitrile coating. Check&Go\n","EN 420                         EN 388-2016 : 4X43C","7 to 11","10 PR","CAS","PR",5.1999999999999993,1715.9999999999998]
[null,4150072,null,"NEW!!! Vertigo grey sleeves  Knitted lightweight grey Spectra/Elastan/ outside glass fibre, Velcro on top. \n","EN 420                         EN 388-2016 : 3X4XC","One size","10 EA","BOX","EA",5.52,1821.6]
[]
[null,"SKELETON - cut resistant glove (1-5) designed for shocks absorption"]
[null,"COMFORT"]
[null,"The knitting technique gives the gloves perfect support, limits the penetration of dirt and offers a good touch.The ventilated back improves the glove's breathability. "]
[null,"RESISTANCE & SAFETY"]
[null,"The composition of the glove offer  a constant, reliable and safe protection to cut from level 1 to level C.Versions dipped in nitrile foam. The reinforcements on the top of the "]
[null,"hand helps to protect  the top of fingers and the metacarpian area against shocks."]
[]
[null,2332271,null,"NEW!!! SKELETON Nit A. Handling of heavy parts in oily or greasy environment. Shock absober pad on top of the hand to protect metacarpian and fingers. Knitted glove in black polyamide. Reinforcement on thumb and plam. Black nitrile foam coating on palm. Rubber pads on top of the hand and fingers.Knitted dipped glove with polyamide fiber, gauge 13. Coating:black nitrile foam. Lenght 25 cm. Dexternity: class 5.\n","EN 420 \nEN 388-2016 : 3122AP","7 to 11","10 PR","CAS","PR",10.698181818181819,3530.4]
[null,2332275,null,"NEW!!! SKELETON Nit B. Handling of heavy parts with cut risks in oily or greasy environment. Shock absober pad on top of the hand to protect metacarpian and fingers.Knitted glove in Spectra®.The knitting technique provides the glove with excellent fit and high dexterity.The Spectra® yarn offers very good resistance to cut.Nitrile coating provides good protection against oil and grease. The foam coating makes the glove more flexible than standard nitrile.Rubber pad on top of the hand and fingers helps to protect metacarpian and fingers from shocks. Length 25 cm. ","EN 420 \nEN 388-2016 : 4X43BP","7 to 11","10 PR","BOX","PR",12.647272727272728,4173.6000000000004]
[null,2332524,null,"SKELETON Nit C. Knitted glove in composite and para-aramid yarn. Plated polyamide. Black nitrile foam coating on palm. Rubber pads on top of the hand and fingers. Fiber: Para-aramid and composite. Length 25 cm. Perfect for handling of heavy parts with high cut risks in oily or greasy environment. Shock absober pad on top of the hand to protect metacarpian and fingers.","EN 420 \nEN 388-2016 : 4X42CP \n","7 to 11","10 units","BOX","PR",13.709090909090909,4524]
[null,"Check & Go Deep Tril range: 1, B, C, D  designed with easy visual recognition of the cut protection level. PU or nitrile coating. High precision work.",null,null,null,null,null,null,null,0,0]
[null,2299400,null,"NEW!!! C&G DeepTril A. Handling in oily or greasy conditions. Outdoor handling in wet environment. Assembly work in greasy/oily environment.Black polyamide knitted glove. Fully dipped black foam nitrile coating. PVC dots on palm. Elasticated knitted wrist. Gauge 13. Length : 25 cm","EN 420\nEN 388-2016 : 4121A","7 to 11","10 units ","BOX"," PR",4.5745454545454542,1509.6]
[null,2299403,null,"NEW!!! C&G DeepTril B. Assembly work with cut risks in greasy/oily environment. Outdoor handling in wet environment. Black HPPE knitted glove. Fully dipped black foam nitrile coating.Elasticated knitted wrist.Gauge 13. Length: 25 cm. The ergonomics seamless knit construction conforms better to the natural shape of the hand for greater strength and durability, superior confort.The filament yarn reduce linting for the most sensitive applications and easily laundered for extended use. The tight knit gives the glove perfect support, limits the penetration of dirt and offers a good touch.The foam coating optimise the glove's breathability,  PVC dots on palm improves the grip.The knitted and elasticated wrist gives the glove good support.The nitrile coating provides outstanding abrasion resistance and a good protection in light oily environement.","EN 420\nEN 388-2016 : 4X43B","7 to 11","10 PR","BOX","PR",8.48,2798.4]
[null,null,null,null,null,null,null,null,null,null,0]
[null,2299405,null,"NEW!!! C&G DeepTril C. Assembly work with high cut risks in greasy/oily environment. Outdoor handling in wet environment. Black HPPE/composite fiber knitted glove. Fully dipped black foam nitrile coating. Elasticated knitted wrist. Gauge 13.Length: 25 cm. The nitrile foam coating provides outstanding abrasion resistance and good protection in light oily environnement.HPPE mixed with composite fiber provides very high resistance to cut.The ergonomics seamless knit construction conforms better to the natural shape of the hand for greater strength and durability, superior confort. The filament yarn reduce linting for the most sensitive applications and easily laundered for extended use. The tight knit gives the glove perfect support, limits the penetration of dirt and offers a good touch.The foam coating optimise the glove's breathability and PVC dots on palm improves the grip.The knitted and elasticated wrist gives the glove good support.","EN 420\nEN 388-2016 : 4X42C","7 to 11","10 PR","BOX","PR",11.679999999999998,3854.3999999999992]
[]
[null,"NEW!!! "]
[null,"CHECK & GO - CUT RESISTANT RANGE OF GLOVES"]
[null,"COMFORT"]
[null,"Knitted gloves cut resistant level 1, B and C with color coding. Designed with easy visual recognition "]
[null,"of the cut protection level. PU or nitrile coating. High precision work."]
[null,"RESISTANCE"]
[null,"The Dyneema® and polyamide thread provides best properties against cuts.The polyurethane/nitrile coating at the palm and fingertips provides outstanding abrasion resistance."]
[null,"SAFETY"]
[null,"Color coding on top of the hand and coating color helps safety manager and workers to visually recognize the level of cut protection."]
[]
[null,"CHECK &GO "]
[null,2332255,null,"Check & Go Red PU 1.100% Nylon knitted glove\nRed PU coating on the palm and fingers","EN 420 \nEN 388-2016 : 4131X ","7 to 11","10 units","BOX","PR",0.98909090909090913,326.40000000000003]
[null,2332265,null,"Check & Go Red Nit 1.Red Nitrile. Coating on palm and fingers. Red color White polyamide knitted glove. Red oilproof nitrile coating on palm and fingertips .Elastic knitted wrist ","EN 420 \nEN 388-2016 : 4121X","7 to 11","10 units","BOX","PR",0.98909090909090913,326.40000000000003]
[null,2332242,null,"Check & Go Amber PU B. Orange Polyurethane (PU). Coating on palm and fingers. Orange color. ","EN 420 \nEN 388-2016 : 4X42B ","7 to 11","10 units","BOX","PR",6.5672727272727265,2167.1999999999998]
[null,2332552,null,"Check & Go Amber Nit B\nOrange Nitrile. Coating on palm and fingers. Orange color. ","EN 420 \nEN 388-2016 : 4X43B ","7 to 10","10 units","BOX","PR",5.5418181818181811,1828.7999999999997]
[null,2332545,null,"Check & Go Green PU C\nGreen Polyurethane (PU). Coating on palm and fingers. Green color.","EN 420 \nEN 388-2016 : 4X43C ","7 to 10","10 units","BOX","PR",7.3527272727272717,2426.3999999999996]
[null,2332555,null,"Check & Go Green Nit C\nGreen Nitrile. Coating on palm and fingers. Green color","EN 420 \nEN 388-2016 : 4X43C ","7 to 10","10 units","BOX","PR",7.2727272727272725,2400]
[]
[null,"NEW!! "]
[null,"TUFFSHIELD Deep blue - CUT LEVEL C"]
[null,"Protection against extreme cut risks: slaughtering, food, fish, paper industry. To be used in wet environment. "]
[null,"Can also be used in oily environement in various industries."]
[null,"RESISTANCE :The mix of HPPE and composite fiber to obtain excellent protection levels against cuts (level C). "]
[null,"HYGIENE The HPPE fibre resists cuts, abrasion and detergents."]
[null,"COMFORT:The composite fibres have been protected so that they do not come directly in contact with the skin. "]
[]
[null,2312928,null,"TUFFSHIELD Deep blue. Knitted glove, HPPE, composite fiber and polyamide \nFully dipped light blue nitrile foam coating. \n","EN 420 \nEN 388-2016 : 4X42C ","7 to 11","10 units","BOX","PR",11.57090909090909,3818.3999999999996]
[null,2312929,null,"TUFFSHIELD Deep blue Right HAND. Knitted glove, HPPE, composite fiber and polyamide \nFully dipped light blue nitrile foam coating. ","EN 420 \nEN 388-2016 : 4X42C ","7 to 11","1 unit","BOX","EA",7.5490909090909089,2491.1999999999998]
[null,"Hand Protection |  GENERAL HANDLING",null,null,null,null,""]
[null,"GENERAL HANDLING",null,null,null,null,""]
[null,"PERFECT POLY",null,null,null,null,""]
[null,2400251,null,"PERFECT POLY BLACK. Knitted extremely lightweight black polyamide. Grey polyurethane coating.","EN 388 : 4121","6 to 11","10 units","BOX","PR",0.99636363636363645,328.8]
[null,2400260,null,"PERFECT POLY SKIN; Lightweight blue polyamide glove with grey PU coating on the palm and fingertips for good dexterity in electronic and automobile industries","EN 388 : 3111","7 to 10","10 units","BOX","PR",1.3381818181818181,441.59999999999997]
[null,2232240,null,"PERFECT POLY FINGER; Lightweight white polyamide glove with white PU coating on the fingertips only","EN420\nminor\nrisks","6 to 10","10 units","BOX","PR",1.3018181818181818,429.59999999999997]
[null,2400250,null,"PERFECT POLY GREY; Lightweight grey polyamide glove with grey PU coating on the palm and fingertips for fine handling in a dry or soiled environment","EN 388 : 4121","6 to 11","10 units","BOX","PR",1.0545454545454545,347.99999999999994]
[null,2232255,null,"PERFECT POLY WHITE; Lightweight white polyamide glove with white PU coating at the palm and fingertips","EN 388 : 4131","6 to 11","10 units","BOX","PR",0.9309090909090908,307.2]
[null,2132251,null,"PU 1st BLACK; Gauge 13 black polyamide knit with grey PU coating on the palm","EN388 : 4131","6 to 11","10 units","BOX","PR",0.84363636363636352,278.39999999999998]
[null,2100250,null,"PU 1st GREY Knitted lightweight grey polyamide. Grey polyurethane coating. ","EN 388 : 4131","6 to 11","10 units","BOX","PR",0.97454545454545449,321.59999999999997]
[null,2100052,null,"PU 1st GREY LONG. Knitted leightweight grey polyamide. Grey polyuretane coating. Length: 30 cm. ","EN 388 : 4131","6 to 11","100 units","CAS","PR",1.1636363636363636,384]
[null,2132255,null,"PU 1st WHITE; Gauge 13 white polyamide knit with white PU coating on the palm","EN 388 : 4131","6 to 11","10 units","BOX","PR",0.97454545454545449,321.59999999999997]
[null,2100450,null,"PU nylon black; Polyamide with its polyurethane coating provide fine grip, good abrasion and tear resistance, gauge 13","EN 388: 3121","6 to 11","100 pairs","CAS","PR",0.68363636363636349,225.59999999999994]
[null,2100451,null,"PU nylon grey, Polyamide with its polyurethane coating provide fine grip, good abrasion and tear resistance, gauge 13","EN 388: 4131","6 to 11","100 pairs","CAS","PR",0.68363636363636349,225.59999999999994]
[null,2100455,null,"PU nylon white, Polyamide with its polyurethane coating provide fine grip, good abrasion and tear resistance, gauge 13","EN 388: 3121","6 to 11","100 pairs","CAS","PR",0.68363636363636349,225.59999999999994]
[null,"WORKEASY"]
[null,2100251,null,"WORKEASY BLACK PU. Knitted lightweight black polyester.Black polyurethane coating. ","EN 388 : 3121","6 to 11","10 units","BOX","PR",0.87272727272727257,287.99999999999994]
[null,2132200,null,"WORK EASY LINER WHITE. Knitted lightweight polyester. ","Minor risks","7 to 11","100 units","CAS","PR",0.52363636363636357,172.79999999999998]
[null,"Hand Protection |  GENERAL HANDLING",null,null,null,null,""]
[null,"POLYTRIL",null,null,null,null,""]
[]
[null,2332663,null,"NEW! POLYTRIL™ Flex Fine handling in dry, greasy, damp and dirty environment, silicone and DMF free product.","EN 420\nEN 388 : 4131","6 to 11","10 PR","CAS","PR",2.4872727272727269,820.79999999999984]
[null,2232230,null,"POLYTRIL; Lightweight polyamide glove with grey watertight Nitrile at the fingertips and palm for fine handling dry and greasy objects","EN388 : 4121","7 to 10","10 units","BOX","PR",1.5781818181818179,520.79999999999995]
[null,2232231,null,"POLYTRIL BLACK; Lightweight polyamide glove with black watertight Nitrile at the fingertips and palm for fine handling dry and greasy objects","EN388 : 4121","6 to 11","10 units","BOX","PR",1.5781818181818179,520.79999999999995]
[null,2232233,null,"POLYTRIL MIX; Black cotton polyamide glove with black watertight rough Nitrile coating at the palm and fingertips for heavy handling in greasy and damp conditions","EN388 : 4232","6 to 11","10 units","BOX","PR",1.7527272727272727,578.4]
[null,2232236,null,"POLYTRIL TOP; Knitted polyamide glove with black oil-proof Nitrile coating on palm and back, fully dipped for use in oily or greasy conditions","EN388 : 4121","6 to 10","10 units","BOX","PR",1.8690909090909087,616.79999999999984]
[null,2232270,null,"POLYTRIL AIR ; Black nylon glove with breathable black foam Nitrile coating on the palm and fingertips for dexterity in greasy and damp conditions with excellent grip and abrasion resistance","EN388 : 4121","7 to 11","10 units","BOX","PR",1.9563636363636361,645.59999999999991]
[null,2232272,null,"POLYTRIL AIR  ¾; Black nylon glove with breathable ¾ black foam Nitrile coating for dexterity in greasy and damp conditions, foam Nitrile provides excellent grip and abrasion resistance","EN388 : 4121","7 to 10","10 units","BOX","PR",2.0945454545454543,691.19999999999993]
[null,2232273,null,"POLOTRYL AIR COMFORT. Knitted lightweight polyamide/ cotton/ Lycra. Black nitrile foam coating. ","EN388 : 4121","6 to 11","10 units","BOX","PR",2.3127272727272725,763.19999999999993]
[null,2232278,null,"POLYTRIL AIR SKIN; Polyamide knitted glove with ultra thin breathable black foam Nitrile coating on the palm and fingers, gauge 15,  for precision work","EN388 : 3131","7 to 10","10 units","BOX","PR",2.1309090909090909,703.19999999999993]
[null,2332276,null,"NEW! POLYTRIL™ GRIP . Handling in oily or greasy conditions. Outdoor handling in wet environment. Assembly work in greasy/oily environment. Construction, automotive, metal industry.","EN 388 : 3131","7 to 11","10 PR","CAS","PR",4.3127272727272716,1423.1999999999996]
[null,"OIL GRIP"]
[null,"NF35F",null,"OIL GRIP FC (Fully Coated). Knitted green polyamide. Fully coated with double dipped nitrile.","EN388 : 4131","7 to 11","12 units","BOX","PR",3.876363636363636,1279.1999999999998]
[null,"NF35",null,"OIL GRIP. Knitted green polyamide. Micro finish black nitrile coating. ","EN388 : 3121","7 to 11","12 units","BOX","PR",3.898181818181818,1286.3999999999999]
[null,"DEXGRIP",null,null,null,null,""]
[null,2094140,null,"DEXGRIP. Knitted glove cotton/polyamide grey. Palm and fingertips coated in blue color crinkled latex. Knitted wrist. Lenght : 26 cm.","EN388 : 2142               EN 407 : X2XXXX","7 to 11","10 units","BOX","PR",1.6727272727272724,551.99999999999989]
[null,2094150,null,"DexGRIP LIGHT. Knitted lightweight polyamide/blue cotton. Thin blue crinkled Latex coating. ","EN388 : 2121","7 to 10 ","10 units","BOX","PR",1.6945454545454546,559.20000000000005]
[null,2094145,null,"GRIP LATEX; Cotton jersey glove with crinkled latex coating for handling heavy, abrasive, slippery or damp objects","EN388 : 4231","7 to 10","10 units","BOX","PR",4.2327272727272724,1396.8]
[null,"SOFLEX",null,null,null,null,""]
[null,2095225,null,"SOFLEX; Nitrile glove on a cotton liner for handling slightly greasy objects, yellow Nitrile coating on palm and fingers, ventilated back","EN388 : 4111","7 to 11","10 units","BOX","PR",1.8036363636363635,595.19999999999993]
[null,"T4700P",null,"Superlite plus. Cut and sewn with interlock cotton. Yellow nitrile palm coating. Knitted wrist. ","EN388 : 3111","6 to 10","12 units","BOX","PR",1.6145454545454547,532.80000000000007]
[null,"T4700",null,"Superlite plus. Cut and sewn with interlock cotton. Yellow nitrile palm coating. Knitted wrist. ","EN388 : 3111","6 to 10","12 units","BOX","PR",1.8763636363636362,619.19999999999993]
[null,"BLUESAFE"]
[null,"T101",null,"Bluesafe. Cut and sewn with interlock cotton. Blue nitrile 3/4 coating. Knitted wrist. ","EN388 : 3111","8 to 10","12 units","BOX","PR",1.8836363636363633,621.59999999999991]
[null,"T102",null,"Bluesafe. Cut and sewn with interlock cotton. Fully coated blue nitrile. Knitted wrist. ","EN388 : 3111","9L to 10XL","12 units","BOX","PR",1.9345454545454543,638.4]
[null,"T107",null,"Bluesafe. Cut and sewn with interlock cotton. Blue nitrile 3/4 coating. Safety cuff.  ","EN388 : 3111","9L to 10 XL ","12 units","BOX","PR",2.0436363636363635,674.4]
[null,"T157",null,"Bluesafe. Cut and sewn with interlock cotton. Fully coated blue nitrile. Safety cuff.  ","EN388 : 3111","9L to 10 XL ","12 units","BOX","PR",2.0945454545454543,691.19999999999993]
[null,"GRIP TASK"]
[null,"T63WG",null,"GRIP TASK. Glove 3/4 coated with yellow latex on cotton Jersey liner Knitted cuff. Lenght:25cm","EN388","8XL, 11XXL",12,"BOX","PR",2.3272727272727272,768]
[null,"T65WG",null,"GRIP TASK. Glove fully coated with yellow latex on cotton Jersey liner 10 cm cuff","EN388","8XL, 11XXL","48 units","BOX","PR ",3.8400000000000003,1267.2]
[null,"T66WG",null,"Grip Task. Glove 3/4 coated with yellow latex on cotton Jersey liner Safety cuff.",null,"11XXL","12 units","BOX","PR ",2.5309090909090908,835.19999999999993]
[]
[null,"WORKNIT HD"]
[null,"85/3721",null,"WORKNIT HD. Cut and sewn with jersey cotton. Palm coated in flexible nitrile. Black dots on reverse. ","EN388 : 3111","8 to 10","144 units","CAS","PR",6.2472727272727262,2061.5999999999995]
[null,"85/3729",null,"WORKNIT HD. Cut and sewn with jersey cotton. Palm coated in flexible nitrile. Cotton stripes on reverse. ","EN388 : 3111","8 to 10","144 units","CAS","PR",5.4763636363636357,1807.1999999999998]
[null,"SOFRACLEAN "]
[null,"RU530",null,"RU530; Semi-heavy 100% cotton interlock glove, bleached white for enhanced hygiene and cleanliness, length 21cm","minor risks","7 and 9","12 units","BOX","PR",0.76363636363636356,251.99999999999997]
[null,"RU711",null,"RU711. Cut and sewn interlock whitened cotton with elastine, ambidextrous. ","Minor risks","6 and 8 ","12 units","BOX","PR",2.1309090909090909,703.19999999999993]
[null,2078222,null,"SOFRACLEAN FIT; cotton interlock glove for handling fine parts in a clean environment, ambidextrous, length 27cm","minor risks","7 and 9","10 units","BOX","PR",0.68363636363636349,225.59999999999994]
[null,"POLYTEX"]
[null,"UA0100",null,"UA0100. Cut and sewn polyamide Lycra, industrial cutting, ambidextrous. ","Minor risks","6 to 10","200 units","CAS","PR",2.5236363636363635,832.8]
[null,"RF075",null,"POLYTEX 75; 100% white polyester glove","EN388 : 0121","7 and 9","12 units","BOX","PR",1.4545454545454544,479.99999999999994]
[null,"RF040",null,"POLYTEX 40; 100% white polyamide, town model","EN388 : 1121","7 to 11","300 pairs","box","PR",2.56,844.80000000000007]
[null,"Hand Protection |  GENERAL HANDLING",null,null,null,null,""]
[]
[null,"TRICOTON",null,null,null,null,""]
[null,"RGT350",null,"TRICOTON ULTRA LIGHT; 100% cotton ultra lightweight, gauge 13, knitted glove with elastic cuff for fine handling in clean environment, can be used as an under-glove","EN420 minor risks","6 to 10","10 units","BOX","PR",0.53090909090909089,175.2]
[null,"RGT550",null,"TRICOTON LIGHT; 100% cotton light-weight, gauge 13, knitted glove with elastic cuff for fine handling in clean environment, can be used as an under-glove","EN420 minor risks","6 to 10","10 units","BOX","PR",0.61090909090909085,201.59999999999997]
[null,"RGT10550",null,"TRICOTON LIGHT LONG. 100 % cotton knitted glove\n10 cm elastic wrist. Length: 280 mm.","EN420 minor risks","7 to 9","300 units","CAS","PR ",1.0836363636363635,357.59999999999997]
[null,"TRICONYL",null,null,null,null,""]
[null,"RGT020",null,"TRICONYL; White 100% polyamide knitted glove, ambidextrous, gauge 13, for light handling and assembly of fine parts","EN388 : 213X","6 to 10","300 units","CAS","PR ",0.81454545454545457,268.8]
[null,"RGT820M",null,"TRICONYL MITT; White 100% polyamide knitted fingerless mitt, gauge 13, with PVC dots on the palm ","EN388 : 213X","7 and 9","300 units","CAS","PR",1.8181818181818181,600]
[null,2232097,null,"TRICONYL LONG; Lightweight white 100% polyamide knitted glove, gauge 13, long cuff, length 27cm","EN388 : 213X",9,"400 units","CAS","PR",1.1563636363636363,381.59999999999997]
[null,2232420,null,"TRICONYL MICRODOTS; White 100% polyamide knitted glove, with small black PVC dots on the palm and fingers for abrasion resistance and grip","EN420 minor risks","6 to 10","10 units","BOX","PR",1.3381818181818181,441.59999999999997]
[null,2232098,null,"TRICONYL FIT; White 100% polyamide knitted glove, ambidextrous, non pilling, the polyamide fabric is suitable for the agrifood industry as well as for precision work","EN420 minor risks","7 to 10","10 units","BOX","PR",1.0472727272727271,345.59999999999997]
[null,"RESISTEX"]
[null,2232092,null,"RESISTEX LIGHT GRIP 2; Cotton-polyester blend glove with double side blue PVC tiger paw grip pattern, ambidextrous","EN388 : 113X","7 to 9","10 units","BOX","PR",0.80727272727272736,266.40000000000003]
[null,"RGT880DC",null,"RESISTEX LIGHT GRIP FL; Cotton-polyester blend glove with red PVC tiger paw grip pattern on palm and fingers, index and thumb cut","EN388 : 113X","7 and 9","300 units","CAS","PR",2.3563636363636364,777.6]
[null,"ABRATEX - POLYAMIDE AND COTTON, CUT RESISTANT 2",null,null,null,null,""]
[null,"RGT088",null,"ABRATEX LIGHT; lightweight poly / cotton knitted glove ","EN388 : 224X","6 to 10","10 units","BOX","PR ",1.3963636363636363,460.79999999999995]
[null,"RGT888",null,"ABRATEX LIGHT GRIP; lightweight poly / cotton knitted glove with PVC dots on the palm and fingers for abrasion resistance and grip","EN388 : 224X","6 to 11","10 pairs ","BOX ","PR",1.6072727272727272,530.4]
[null,"K711",null,"EAGLE GRIP 711. Grey polyamide lightweight knitted glove PVC dots on Palm Elastic cuff, 6cm. Lenght : 25 cm "," EN 388 : 214X","7S, 8M, 9L, 10XL","144 units","BOX ","BOX",9.0763636363636362,2995.2]
[]
[null,"VELVET "]
[null,2012860,null,"VELVET PALM LONG CUFF; Water-repellent velvet leather palm and water-repellent grain leather back, 10cm safety cuff","EN388 : 3122","7 to 11","10 units","BOX","PR",10.130909090909091,3343.2]
[null,2049131,null,"VELVET PALM LASTEX. Palm velvet/ reverse water repellent cowhide grain leather. Comprehensive vein protection. ","EN388 : 3122","8 to 11","10 units","BOX","PR",9.3454545454545439,3083.9999999999995]
[null,"HYDRO"]
[null,2049260,null,"HYDROGRAIN; Water-repellent cowhide grain leather glove for handling in damp conditions","EN388 : 2121","7 to 12","10 units","BOX","PR",10.618181818181817,3503.9999999999995]
[null,2049160,null,"HYDROGRAIN EW; Water-repellent cowhide grain leather glove for handling in damp conditions, elasticated at the back of the wrist","EN388 : 2122","7 to 12","10 units","BOX","PR",11.192727272727272,3693.5999999999995]
[null,"NATURAL LEATHER"]
[null,2030195,null,"GRAIN DRIVER; Natural cowhide grain leather combines resistance and dexterity","EN388 : 3121","8 to 11","10 units","BOX","PR",6.4,2112]
[null,"CT1615CH",null,"PRECISION TEX 2; Goatskin grain leather glove with green cotton interlock back","EN388 : 2121","6 to 11","10 units","BOX","PR ",5.6363636363636358,1859.9999999999998]
[null,2051652,null,"PRECISION TEX EW; Lambs leather glove with cotton jersey back and elasticated wrist","EN388 : 1X11","7 to 10","10 units","BOX","PR",4.7927272727272721,1581.5999999999997]
[null,2058685,null,"CRYOGENIC; Water-repellent grain leather glove with double layer insulation for handling liquid nitrogen offering protection against a small splattering, tested at -170C","EN388 : 3222         EN511 : 222","9 to 11","1 unit","BOX","PR",40.763636363636358,13451.999999999998]
[null,2281561,null,"FIREMAN; Water-repellent grain leather glove lined with Kevlar cotton, safety cuff","EN388 : 3222         EN407 : 4132XX","7 to 11","1 unit","","PR",26.02181818181818,8587.1999999999989]
[null,2049132,null,"VELVET SHOCK; Water-repellent grain leather glove with padded Poron® at the palm and back to absorb impacts, for use with pneumatic hammer tools","EN388 : 2121","9 to 11","10 units","BOX","PR",15.352727272727272,5066.3999999999996]
[null,"Hand Protection |  CUT RESISTANT",null,null,null,null,""]
[null,2397201,null,"NEW !!! PICGUARD Urban; High performance puncture needle stick resistant glove is tested to the highest ASTM protection level for puncture resistance.  Cut & sewn glove in Knitted coated fabric on palm (Pu / polyamide), polyester elasthan on back.\nLined with coated fabric (para aramid / pu) and polyester viscose\n","EN388 :4543           ASTM 2878","6 to 11","1 unit","BOX","PR",31.52,10401.6]
[null,2397200,null,"PICGUARD; High performance puncture needle stick resistant glove is tested to the highest ASTM protection level for puncture resistance, one-piece para-aramid coated PU ceramic protection layer is exceptionally thin allowing PicGuard to be used as an underglove together with a wide variety of over-gloves\n● BSIF Product Innovation Award Finalist 2011","EN388 :4444           ASTM 1342","S, M, L, XL","1 unit","","PR",80.09454545454544,26431.199999999993]
[null,"ARACUT - CUT RESISTANT 3 "]
[null,2094141,null,"ARACUT LAT; Medium-weight 100 % Kevlar knitted glove with coating at the palm and at the fingertips in blue crepe latex","EN388 : 3444          EN407 : X2XXXX","7 to 10","10 units","BOX","PR",6.9090909090909083,2279.9999999999995]
[null,"RGTK830",null,"ARACUT NIT; Medium-weight Aramide knitted glove with grey Nitrile coating at the palm","EN388 : 4342","7 to 11","10 units","BOX","PR ",11.91272727272727,3931.1999999999994]
[null,"CUT RESISTANT LEATHER"]
[null,2049296,null,"HYDROCUT KN; Water repellent cowhide grain leather glove with Kevlar lining for cut protection in a greasy or damp environment","EN388 : 3343","8 to 11","10 units","BOX","PR",21.170909090909088,6986.3999999999987]
[null,2049292,null,"VELVET CUT; Water-repellent grain leather with Kevlar lining in the palm, water-repellent velvet in the back, elastic wrist","EN388 : 3222","9 to 11","10 units","BOX","PR",17.949090909090906,5923.1999999999989]
[null,"PARA-ARAMID - CUT RESISTANT 3"]
[null,2232087,null,"ARACUT LIGHT; Lightweight, gauge 13, 100% Kevlar knitted glove, ambidextrous, can be used as a heat resistant underglove for handling objects up to 100C","EN388 : 024X ","7 to 10","10 units","BOX","PR",4.8218181818181813,1591.1999999999998]
[null,2032086,null,"ARACUT; Medium-weight, gauge 10, 100% Kevlar knitted glove, ambidextrous,  can be used for handling objects up to 100C","EN388 : 134X         EN407 : X1XXXX","6 to 10","10 units","BOX","PR",6.1018181818181825,2013.6000000000001]
[null,2032085,null,"ARACUT GRIP, Medium-weight, gauge 10, 100% Kevlar knitted glove with blue PVC dots at the palm","EN388 : 034X ","6 to 11","10 units","BOX","PR",6.7927272727272729,2241.6]
[null,2032101,null,"JUNKYARD DOG. For heavy handling of sharp or perforating parts in a dry or greasy atmosphere. 100% Kevlar® knitted glove\nCowhide split leather reinforcement on palm and fingers","EN388 : 4443 ","9 and 10","10 units","BOX","PR",14.727272727272725,4859.9999999999991]
[null,"GTK8500M",null,"ARACUT® FL DOTS. Handling of slipping and cutting parts. Various handlings. Para-aramid knitted Mitt (Kevlar® long fibres). Dots on the palm .End of the fingers cut on the level of the last phalange","EN388 : 134X ","7 to 9","10 units ","BOX"," PR",5.752727272727272,1898.3999999999999]
[null,4402835,null,"ARACUT SLEEVE ; Kevlar knitted sleeve, double thickness, thumbhole, length 45cm","EN388 :132X\nEN407 : X1XXXX","One size","5 pairs","BOX",null,8.9018181818181805,2937.5999999999995]
[null,4150064,null,"ARACUT SLEEVE 14; Kevlar knitted sleeve, double thickness, length 36cm","EN388 :132X\nEN407 : X1XXXX","One size","10 units","BOX","EA",3.6945454545454544,1219.2]
[null,4150055,null,"ARACUT SLEEVE II; Kevlar knitted sleeve, split leather reinforcement, length 36cm","EN388 : 132X\nEN407 : X1XXXX","One size","10 units","BOX","EA",7.0181818181818176,2316]
[null,4150058," ","ARACUT BLACK 14; Black Kevlar knitted sleeve, double thickness, length 36cm","EN388 :132X\nEN407 : X1XXXX","One size","10 units","BOX","EA",7.127272727272727,2352]
[null,4150057," ","ARMCUT 14 BT; Kevlar knitted sleeve, double thickness, mitten sytle at the fingers (3 Bar-Tac), length 36cm","EN388 :132X\nEN407 : X1XXXX","One size","10 units","BOX","EA",3.4836363636363634,1149.5999999999999]
[]
[null,"RESISTOP - CUT LEVEL 3"]
[null,"RGT099",null,"RESISTOP; Heavyweight glove with cotton interior and polyamide exterior, colour  white","EN388 :234X\nEN407 : X1XXXX","7 to 9","10 units","BOX","PR ",2.269090909090909,748.8]
[null,"RGT099V",null,"RESISTOP GREEN; Heavyweight glove with cotton interior and polyamide exterior, colour green","EN388 :234X\nEN407 : X1XXXX","7 to 10","10 units","BOX","PR ",2.3490909090909091,775.2]
[null,"RGT899V",null,"RESISTOP GRIP GREEN; Heavyweight glove with cotton interior, polyamide exterior and PVC raised dots at the palm for abrasion resistance and grip, colour green","EN388 :234X\nEN407 : X1XXXX","7 to 10","10 units","BOX","PR ",2.7854545454545452,919.19999999999993]
[null,"RGT15099G",null,"RESISTOP LONG. Knitted heavy 73% grey polyamide (outside) plaited 27% cotton (inside). 15 cm knitted wrist. ","EN388 :234X\nEN407 : X1XXXX","7 to 9","10 units","BOX","PR ",3.2290909090909095,1065.6000000000001]
[null,"CUT RESISTANCE 4 "]
[null,2332245,null,"Cut  LEVEL 4 NEW PERFECT CUTTING DIAMOND; White Dyneema® Diamond / Lycra glove with black polyurethane coating on the palm and fingers and red elasticated wrist, cut level 4","EN388 : 4442","6 to 11","10 units","BOX","PR",7.4254545454545458,2450.4]
[null,"NFG17X",null,"LIGHT TASK PLUS 4. Knitted polyamid/glass fibre. Bi-polyamer, 3/4 coating.","EN388 : 4432","7 to 11","12 units","BOX","PR",8.0654545454545445,2661.6]
[null,2332214,null,"NEW!!! PERFECT CUTTING® DIAMOND NIT. Handling sharp parts in a greasy or oily environment. Dyneema® Diamond/lycra®/ black polyamide knitted glove. Black nitrile foam coating on palm and fingers. Red Elastic wrist.The cool Dyneema® diamond touch gives an added sensation of comfort. The tight knit (gauge 13) gives the glove perfect support, limits the penetration of dirt and offers a good touch. The glove's ventilated back optimises its breathability. The Dyneema® diamond/lycra®/polyamide thread provides outstanding properties against cuts. \nThe nitrile foam coating at the palm and fingertips provides outstanding abrasion resistance.Caution! Do not expose this glove to the heat. ","EN 388 : 4543","7 to 11","10 PR","BOX","PR",8.1309090909090891,2683.1999999999994]
[null,"CUT RESISTANCE 4 /5"]
[null,"TUFF CUT",null,null,null,null,""]
[null,2232531,null,"TUFF CUTGRIP. Knitted lightweight para-aramid, polyeamide, steel fibre. Reinforced thumb and index in Kevlar. PVC dots on palm. ","EN388 : 354X             ISO 13997, 37.4N  EN407 : X1XXXX","7 to 11","10 units","BOX","PR",9.0763636363636362,2995.2]
[null,2232532,null,"TUFF CUT LATEX; Kevlar, high tenacity polyamide and steel fibre knitted glove with blue crinkled latex coating on palm and fingers","EN388 : 3543              ISO 13997, 24N     EN407 : X2XXXX","7 to 11","10 units","BOX","PR",9.5999999999999979,3167.9999999999991]
[null,2232533,null,"TUFF CUT NIT;  Kevlar, high tenacity polyamide and steel fibre knitted glove with black foam nitrile coating on palm and fingers","EN388 : 4543                   EN407 : X1XXXX","7 to 11","10 units","BOX","PR",9.5272727272727256,3143.9999999999995]
[null,2232535,null,"TUFF CUT PU; Kevlar, high tenacity polyamide and steel fibre knitted glove with PU coating on palm and fingers\n","EN388 : 4543              ISO 13997, 24N     EN407 : X1XXXX","7 to 11","10 units","BOX","PR",7.2218181818181817,2383.1999999999998]
[null,2232537,null,"TUFF CUT PALM; Kevlar, high tenacity polyamide and steel fibre knitted glove with split leather palm and fingers","EN388 4543\nEN407\nx1xxxx","7 to 10","1 unit","BOX","PR",13.876363636363633,4579.1999999999989]
[null,"CUT LEVEL 5 "]
[null,"DYNEEMA / COMPOSITE",null,null,null,null,""]
[null,"NFD35X",null,"OIL GRIP NFD35X. Knitted Dyneema/ white/green glass fibre.3/4 nitrile double coating. ","EN388 : 4543","7 to 11","12 units","BOX","PR",11.301818181818181,3729.6]
[null,2332243,null,"NEW!! PERFECT CUTTING DIAMOND BLACK Handling sharp parts in a dry or greasy environment.Dyneema® Diamond/lycra®/ polyamide knitted glove.Grey polyurethane coating on palm and fingertips. Elastic wrist. The knitting technique helps to obtain a glove that conforms snugly to the hand, with good dexterity. The glove offers maximum comfort and added sturdiness. The cool Dyneema® diamond touch gives an added sensation of comfort. The tight knit (gauge 13) gives the glove perfect support, limits the penetration of dirt and offers a good touch. The glove's ventilated back optimises its breathability. The Dyneema® diamond/lycra® thread provides outstanding properties against cuts. The polyurethane coating at the palm and fingertips provides outstanding abrasion resistance.Longer cuff for added protection of the wristCaution! Do not expose this glove to the heat","\nEN 388 : 4542 ","7 to 11","10 PR","BOX","PR",9.84,3247.2]
[null,2332247,null,"NEW!!! PERFECT CUTTING® DIAMOND PLUS.Handling sharp parts in a dry or greasy environment.Dyneema® Diamond/lycra®/ polyamide knitted glove.Grey polyurethane coating on palm and fingertips. Elastic wrist. The knitting technique helps to obtain a glove that conforms snugly to the hand, with good dexterity. The glove offers maximum comfort and added sturdiness. The cool Dyneema® diamond touch gives an added sensation of comfort. The tight knit (gauge 13) gives the glove perfect support, limits the penetration of dirt and offers a good touch. The glove's ventilated back optimises its breathability. The Dyneema® diamond/lycra® thread provides outstanding properties against cuts. The polyurethane coating at the palm and fingertips provides outstanding abrasion resistance.Longer cuff for added protection of the wristCaution! Do not expose this glove to the heat. Length: 30 cm. \n","\nEN 388 : 4542 ","7 to 11","10 PR ","BOX","PR",10.036363636363635,3311.9999999999995]
[]
[null,"LEATHER "]
[null,2049297,null,"SPLIT CUT . Anti-cut lined knitted plit leather cowhide. Lastex wrist. ","\nEN 388 : 4543 ","8 to 11",null,null,null,19.549090909090907,6451.1999999999989]
[null,"KEVLAR/ COMPOSSITE FIBER"]
[null,"SHARPFLEX",null,null,null,null,""]
[null,2232522,null,"SHARPFLEX; Composite knitted glove, cut level 5, gauge 13, length 25cm, ambidextrous","EN388 : 254X                   EN407 : X1XXXX","7 to 11","10 units","BOX","PR",3.1781818181818178,1048.8]
[null,2232523,null,"SHARPFLEX PU; Composite knitted glove, cut level 5, gauge 13, length 25cm with black PU coating on palm and fingers","\nEN 388 : 4541 ","7 to 11","10 units","BOX","PR",3.4690909090909083,1144.7999999999997]
[null,2232521,null,"SHARPFLEX DOTS. Knitted leightweight para-aramid, polyamide, composite fibre. Black PVC dots on palm.","EN388 : 454X                   EN407 : X1XXXX","7 to 11","10 pairs","BOX","PR",3.7381818181818174,1233.5999999999997]
[null,2232524,null,"SHARPFLEX Nit. . Knitted leightweight para-aramid, polyamide, composite fibre.Blue crinkled Latex coating.","EN388 : 4542                   EN407 : X1XXXX","7 to 11","10 units","BOX","PR",4.9454545454545453,1632]
[null,2232525,null,"SHARPFLEX LATEX; Composite knitted glove, cut level 5, gauge 13, length 25cm with blue crinkled latex coating on palm and fingers","EN388 : 3542                   EN407 : X2XXXX","7 to 10","10 units","BOX","PR",4.8872727272727268,1612.7999999999997]
[null,"Hand Protection |  CUT PROTECTION FOR FOOD CONTACT",null,null,null,null,""]
[null,"TUFFSHIELD  WITH DYNEEMA"]
[null,2312928,null,"NEW TUFFSHIELD Deep Blue. Knitted HPPE/polyamide/ composite fibre. Fully coated blue nitrile foam, blue colour in accordance with the food industry.","\nEN 388 : 4X42C          Food contact","7 to 11","10 units","BOX","PR",11.57090909090909,3818.3999999999996]
[null,2012953,null,"TUFFSHIELD EVOLUTION LIGHT; Lightweight glove, gauge 13, provides a high level of cut and slash protection, blue colour in accordance with the food industry, cut level 5","\nEN 388 : 254X          Food contact","6 to 10","10 units","BOX","PR",18.52363636363636,6112.7999999999984]
[null,2012950,null,"TUFFSHIELD EVOLUTION MEDIUM; Medium-weight glove, gauge 10, provides a high level of cut and slash protection, blue colour in accordance with the food industry, cut level 5","\nEN 388 : 254X          Food contact          Touch screen","6 to 11","10 units","BOX","PR",13.963636363636361,4607.9999999999991]
[null,2012957,null,"TUFFSHIELD EVOLUTION HEAVY; Heavyweight glove, gauge 7, provides a high level of cut and slash protection, white colour for heavier applications, cut level 5","\nEN 388 : 354X          Food contact","6 to 10","10 units","BOX","PR",21.716363636363635,7166.4]
[]
[null,"Hand Protection |  THERMAL PROTECTION",null,null,null,null,""]
[null,"WELDER",null,null,null,null,""]
[null,2000040,null,"PROOF WELDING; Water-repellent, heat treated split leather glove, fully lined with non flammable material, length 35cm","EN388 : 4144         EN407 : 413x4x EN12477 : Type A","8 to 10","10 units","BOX","PR",16.087272727272726,5308.7999999999993]
[null,2000041,null,"GREEN WELDING; Split leather glove with reinforced palm and heat resistant Kevlar stitching","EN388 : 4133         EN407 : 413x4x EN12477 : Type A","8 to 10","10 units","BOX","PR",14.247272727272726,4701.5999999999995]
[null,2000042,null,"GREEN WELDING PLUS; Split leather glove with reinforced palm, cloth lined with heat resistant Kevlar stitching","EN388 : 4133         EN407 : 413x4x EN12477 : Type A","8 to 10","10 units","BOX","PR",16.247272727272726,5361.5999999999995]
[null,2000044,null,"BLUE WELDING; Split leather glove lined with cotton padding, 140mm canvas lined cuff, length 35cm","EN388 : 3132         EN407 : 413x4x EN12477 : Type A","9 to 10","10 units","BOX","PR",12.065454545454545,3981.6]
[null,2012804,null,"ARGON; Flexible goats grain leather glove with 150mm split leather cuff","EN388 : 3121","9 to 11","10 units","BOX","PR",11.672727272727272,3851.9999999999995]
[null,2058640,null,"THERMA WELDER.  Black cowhide grain leather, resitant to high temperatures. 20cm ssplit cuff. Lenght:39cm","EN388 : 2121         EN407 : 413x4x EN12477 : Type B","8 to 11","10 units","BOX","PR",17.75272727272727,5858.4]
[null,2058691,null,"MIG FIT; Split leather glove with aluminised Kevlar heat reflective back, fully lined with cotton fleece for improved thermal insulation\n","EN388 : 3143         EN407 : 41344X EN12477 : Type A","10 to 11","5 units","BOX","PR",23.010909090909088,7593.5999999999995]
[null,2049294,null,"WELDING CUT; Water-repellent leather glove with Kevlar lining , velvet leather palm and grain leather back, heat resistant 150mm split leather cuff","EN388 : 3222         EN407 : 413X4X EN12477 : Type A","8 to 12","10 units","BOX","PR",20.450909090909089,6748.7999999999993]
[null,2058590,null,"MAXI WELDER CUT; Cowhide leather / Kevlar glove with Kevlar fleece palm, cotton-lining, silicone coating, back in water repellent grain leather, split leather 150mm cuff, Kevlar thread seams","EN388 : 3421         EN407 : 433x4x EN12477 : Type B","8 to 10","10 units","BOX","PR",22.734545454545454,7502.4]
[]
[null,"FOUNDRY",null,null,null,null,""]
[null,2012843,null,"FOUNDRY M10. Anti heat split leather. Split cuff lined cotton. Lenght: 30cm. ","EN388 : 3143         EN407 : 41324X","9 to 12","10 pairs","BOX","PR",13.687272727272726,4516.7999999999993]
[null,"Hand Protection |  THERMAL PROTECTION",null,null,null,null,""]
[]
[null,"HOTMILL",null,null,null,null,""]
[null,"RPB1433S",null,"JERSEY LIGHT; 100% cotton fleece lined jersey, brown colour, knitted wrist 14cm, length 26cm","EN388 : 0121         EN407 : X1XXXX","One size","200 units","CAS","PR",1.1781818181818182,388.8]
[null,"RGE6811",null,"CRYSTAL S REINFORCED; 100% cotton glove, brushed cotton drill, brushed exterior / interior, canvas cuff 6cm, length 27cm","EN388 : 1222         EN407 : X1XXXX","One size","120 units","CAS","PR",3.2436363636363637,1070.4000000000001]
[null,"TERRY HEAT RESISTANT GLOVES - HEAT CONTACT UP TO 250"]
[null,"RGT1685",null,"TERRY; 100% cotton terry knitted glove, ribbed cotton wrist, length 27cm","EN388 : 1232         EN407 : X2XXXX",10,"100 units","CAS","PR",1.4545454545454544,479.99999999999994]
[null,"RQE9607A",null,"TERRY HEAVY; 100% cotton terry glove, cuff 15cm, length 36cm","EN388 : 2331         EN407 : X2XXXX","One size","60 units","CAS","PR",3.9199999999999995,1293.5999999999999]
[null,2032625," ","TERRY MIX; Cotton / polyester terry knitted glove with elasticated wrist, 6cm, grey colour, length 25cm","EN388 : 232X         EN407 : X2XXXX",9,"10 units","BOX","PR",2.0509090909090908,676.8]
[null,2232039,null,"TERRYTOP CANVAS; 100 % cotton terry glove, 16cm canvas cuff","EN388 : 1231         EN407 : X2XXXX","One size","6 units","BOX","PR",3.7309090909090901,1231.1999999999998]
[null,"RAE8815",null,"RAE8815. 100% brushed jersey pique cotton. Palm and back (brushed inside). 15 cm canvas cuff. Length: 34 cm. ","EN388 : 1221         EN407 : X1XXXX",9,"120 units","CAS","PR",2.1963636363636363,724.8]
[null,"ARATHEMA "]
[null,"RGT425",null,"ARATHERMA Fit S. Knitted heave para-aramid. Lined knitted cotton glove.7cm knitted elastised wrist.","EN388 : 254X         EN407 : 42XXXX","8 to 10","5 units","BOX","PR ",14.007272727272726,4622.3999999999996]
[null,2232086,null,"ARATHERMA FIT; Kevlar knitted glove with cotton liner and long elasticated wrist, 10cm, for handling hot and cutting objects, withstands 14.5 seconds at 350C and 20.2 seconds at 250C, ambidextrous","EN388 : 254X         EN407 : 43XXXX","7 and 9","10 units","BOX","PR",13.694545454545453,4519.2]
[null,2032681,null,"ARATHERMA COMFORT. For handling of sharp and hot objects in a dry atmosphere. Glass industry and paper. Automobiles, car equipment manufacturers100 % Kevlar® knitted glove. Lined with 100% cotton knitted glove . 150 mm green fireproffed canvas cuff . Ambidextrous .","EN388 : 143X         EN407 : 43XXXX",9,"10 units ","BOX"," PR",15.854545454545454,5232]
[null,"RGT8971",null,"ARATHERMA FIT SHORT GRIP; Heavyweight 100% cotton knitted glove with Nitrile dots on both sides","EN388 : 133X         EN407 : X2XXXX","8 and 10","6 units","BOX","PR",3.7963636363636359,1252.8]
[null,2232070,null,"Aratherma Nomex Heavy- Knitted heavy NOMEX®. Lined cotton knitted glove. Ambidextrous. Length: 26.5cm","EN388 : 144X         EN407 : 43XXXX","7 and 9","10 units","BOX","PR",17.141818181818181,5656.7999999999993]
[null,"STR50",null,"Strongotherm Brown - Handlings of warm parts in glass industries... and removal from muld of warm parts for contact temperatures unitl 100°C.","EN 388 : 334X             EN 407 : X1XXXX","7 to 11","12 units","BOX","PR",2.0436363636363635,674.4]
[null,"51/7147",null,"North Grip N Hot Mill, 100% knitted cotton glove lined with cotton glove Double face coating of nitrile dots Ambidextrous, length 30cm","EN 388 : 134X              EN 407 : X2XXXX","one size","12 units","Box","PR",4.1527272727272724,1370.3999999999999]
[]
[null,"TOPFIRE",null,null,null,null,""]
[null,"SA40620",null,"TOPFIRE 40; Non-flammable para-aramid terry mitt, first lining in Kermel needled fabric, second lining in wool, third lining in cotton fleece, length 40cm","EN388 : 2543         EN407 : 44444X","One size","3 units","BOX","PR",47.50545454545454,15676.8]
[null,2280673,null,"TOPFIRE SUPERTHERMA; 100 % Kevlar glove with triple thickness in palm, thumb and fingers, cuff 13cm","EN388 : 2524         EN407 : 44413X","One size","1 unit","PR","PR",46.559999999999995,15364.8]
[null,2201336,null,"TOPFIRE KERMEL; Heat resistant Kermel mitt with Kevlar fleece reinforcement withstands contact temperatures up to 500C ","EN388 : 3544         EN407 : 4443XX","9 to 10","5 units","BOX","PR",63.592727272727267,20985.599999999999]
[null,"ZL910K3RK",null,"TOPFIRE KERMEL 3F; Three-finger heat resistant Kermel glove lined in cotton terry and cotton gauze, 15cm split leather cuff, brushed Kevlar fleece reinforcement between thumb and index finger, length 34cm","EN388 : 4543         EN407 : 44433X","One size","5 units","BOX","PR",59.207272727272724,19538.399999999998]
[null,"MFL40607DJ",null,"MFL40607 DJ; 100% cotton terry knitted mitt with sewn on cuff and thumb, PVC film between jersey and terry","EN 388: 2332\nEN 407: x2xxxx","One size","6 units","BOX","PR",7.8254545454545443,2582.3999999999996]
[null,"ZETEX - HEAT PROTECTION UP TO 500 "]
[null,2275112,null,"SUPERZETEX MITT; Heat resistant Zetex mitt with high performance Nomex® felt lined palm and Kevlar thumb reinforcement, length 15.8\"","EN 388: 4543\nEN 407: 44444X","One size","1 unit","","PR",94.494545454545445,31183.199999999997]
[null,"GLASS FIBRE "]
[null,"IHR540",null,"IHR540; Fibreglass glove with rubber and silicone coating, Kevlar felt lining and 20cm cuff in aluminised glass fabric, length 40cm, ambidextrous","EN 388: 2040\nEN 407: 44XX34","One size","1 unit","BOX","PR",96.4,31812.000000000004]
[null,"GBTK7065",null,"GBTK 7065 Five finger glove, knitted paraaramid terry cloth doubled from a PVC glove. 15 cm cuff, length 35cm","EN 388: 4543\nEN 407: 44XXXX","One size","5 units","BOX","PR",42.814545454545446,14128.799999999997]
[null,"STR2235L",null,"Strongotherm. Handling closed to a work position with heat emanation in glass industries, metal industries.Cotton terry sleeve (680g/m2) Knitted base Tightening elastic on the top","EN 388: 112X\nEN 407: X1XXXX","L","6 units","BOX","PR",2.6981818181818178,890.39999999999986]
[]
[null,"Hand Protection |  COLD PROTECTION",null,null,null,null,""]
[null,"COLD PROTECTION",null,null,null,null,""]
[null,2299500,null,"NEW!!! DEEPBLUE WINTER. Handling of oily or greasy parts in cold environment. Outdoor handling in wet environment. Assembly work in greasy/oily environment. Polyamide knitted glove. Fully dipped blue foam nitrile coating.. Fully Lined with a polar fleece. Self fastening system on the wrist. Gauge 13. Length : 25 cm","EN388 : 4121\nEN511 : X1X\n","7 to 11","10 units ","BOX"," PR",7.621818181818182,2515.2000000000003]
[null,2232023,null,"UP AND DOWN I-VIZ; Knitted glove in acrylic with 3/4 crinkled latex offers protection, dexterity and grip in cold, damp conditions","EN388 : 2231\nEN407 : X2XXXX\nEN511 : 020\n","7 to 11","10 units","BOX","PR",4.2472727272727271,1401.6]
[null,2232101,null,"SOFRACOLD; Blue Thermastat® knit glove for optimum warmth when handling cold and frozen products in a dry environment","minor risk","One size","10 units","BOX","PR",1.2145454545454544,400.79999999999995]
[null,2232037,null,"SOFRACOLD .Handling of frozen food or packaging in dry conditions. Thermastat® knitted glove with Lycra®. Blue PVC dots on one side. The knitting technique and Lycra® elasticity help to obtain a glove that conforms snugly to the hand.\n","EN388 : 213X\n\n",9,"10 units","BOX"," PR",1.2509090909090907,412.79999999999995]
[null,"NF11HD",null,"COLD GRIP. Knitted blue polyamide. Brushed winter liner. Black foam 3/4 PVC coatin","EN388 : 2232\nEN511 : X2X\n","9 to 11","12 units","BOX","PR",5.3090909090909086,1751.9999999999998]
[null,2006433,null,"WINTER PRO; PVC glove on 100 %  seamless woven cotton knitted liner for handling of frozen products","EN388 : 4221\nEN511 : 121          EN374-2\n","8 and 10","5 units","BOX","PR",7.1418181818181807,2356.7999999999997]
[null,"NFD11HD",null,"NEW!!! Cold Grip Plus 5 Knitted lightweight highly cut resistant fibre blend outer shell. Brushed acrylic thermal liner. 3/4 PVC coating, length 26cm","EN388 : 3532\nEN511 : 020\n","7 to 11","12 units","BOX","PR",7.8618181818181805,2594.3999999999996]
[null,"NF14HD",null,"Duro Task Sub Zero; Knitted acrylic brushed inside Crinkled latex coating on palm, gauge 7, length 25cm","EN388 : 1241\nEN511 : x1x\n","8 to 11","12 units","box","PR",3.7963636363636359,1252.8]
[null,2001610,null,"DEERFIT ; Water-repellent suede leather glove with Thinsulate® liner for protection against cold temperatures","EN388 : 2X2X\nEN511 : 120\n","7 to 11","10 units","BOX","PR",16.567272727272726,5467.2]
[null,2001615,null,"DEERFIT LUX ; Buffed suede leather glove with Thinsulate® lining for protection against cold temperatures ","minor risk","7 to 11","10 units","BOX","PR",11.127272727272727,3672]
[null,2001617,null,"WINTER PROOF DRIVER; Water-repellent black leather glove offers protection in cold and damp conditions","EN388 : 3122\n","7 to 11","10 units","BOX","PR",24.02181818181818,7927.1999999999989]
[null,"1640YC",null,"ARCTIC; Goats grain leather with water-repellent \"Scotchgard®\" treatment, 10cm cuff, with winter liner","EN388 : 3221\nEN511 : 120\n","8 to 11","5 units","BOX","PR",30.450909090909082,10048.799999999997]
[]
[null,"Hand Protection |  CHEMICAL PROTECTION",null,null,null,null,""]
[null,"DEXPURE - Light Chemical Protection EN374-2 Disposable",null,null,null,null,""]
[null,4580381,null,"NEW!!! DEXPURE ® 803-81, Non powdered violet blue nitrile thin mill glov, AQL 1.5, Length 24cm, food contact, 200 pcs/box","EN 374 -2, direct food contact","XS,S,M,L,XL","2000 units","CAS","CAS",10.153030303030302,3350.5]
[null,4580021,null,"DEXPURE® 800-21; Powdered natural latex glove, transparent, length 25cm","EN374-2      EN455-1","S,M,L,XL","1000 units","CAS","CAS",6.2833333333333332,2073.5]
[null,4580081,null,"DEXPURE® 800-81; Non powdered Nitrile glove, blue colour, grade A - AQL 1.5, length 24cm","EN374-2      EN455-1","S,M,L,XL","1000 units","CAS","CAS",8.4424242424242415,2785.9999999999995]
[null,4580091,null,"DEXPURE® 800-91; Lightly powdered Nitrile glove, blue colour, grade A - AQL 1.5,  length 24cm","EN374-2      EN455-1","S,M,L,XL","1000 units","CAS","CAS",8.4424242424242415,2785.9999999999995]
[null,4580121,null,"DEXPURE® 801-21; Non powdered natural latex glove, transparent, food contact-AQL1.5, length 24cm","EN374-2      EN455-1","S,M,L,XL","1000 units","CAS","CAS",7.215151515151514,2380.9999999999995]
[null,4580130,null,"DEXPURE® 801-30; 100% heavy latex glove, non powdered, patterned finish, blue colour, thickness 0.3mm, length 33cm","EN374-2      EN455-1","7, 8,9,10","50 units","BOX","BOX",13.687272727272726,4516.7999999999993]
[null,4580195,null,"DEXPURE® 801-95; 100% heavy Nitrile glove, non-powdered, patterned finish, light blue colour, thickness 0.2mm, length 27cm","EN374-2      EN455-1","7, 8,9,10","50 units","BOX","BOX",11.2,3695.9999999999995]
[null,"CS046W",null,"CHEM SOFT. Fine assembly of oily parts. Handling of chemicals. Electronics.Unpowdered nitrile glove. Translucent. Length : 40 cm. AQL : 1,6","EN 420 , EN 374-3","S, M, L, XL","50 units","BAG","PR",60.254545454545443,19883.999999999996]
[null,"FINGERCOTS "]
[null,"125LNR",null,"Nitrile 144 db / bag",null,"M",720,"BAG","BAG",9.9490909090909074,3283.1999999999994]
[null,"135LNR",null,"Nitrile 144 db / bag",null,"L",720,"BAG","BAG",10.087272727272726,3328.7999999999997]
[null,"PVC / NITRILE",null,null,null,null,""]
[null,507620,null,"FINEDEX® 507-620 PVC; PVC unsupported, chlorinated glove, black colour, length 32cm, thickness 0.65mm, plus PVC cuff 45cm","EN388 : 2100        EN374-2","8.5, 9.5, 10.5","25 units","BOX","PR",9.9272727272727259,3275.9999999999995]
[null,2095320,null,"PERFECT FIT FINEDEX 953-20 NITRASOFT. Blue nitrile, chlorinated interior, diamond pattern. 0.3mm length: 33cm","EN388 : 2001        EN374-3 : JKL           food contact","7 to 10 ","10 units","BOX","PR",1.7381818181818181,573.59999999999991]
[null,2009810,null,"FINEDEX ® 098-10 PVC SOFT.General maintenance, cleaning. Collective catering. Standard work in contact with chemicals. Maintenance.","EN388 : 3XXX        EN374-2","7 to 9","10 units ","BOX","PR",2.8509090909090906,940.8]
[null,"LATEX",null,null,null,null,""]
[null,2094432,null,"FINEDEX 944-32 FISHERMAN. Natural orange Latex, polyamide knitted liner, crinckled pattern. Thicknes: 1.3mm.  Lenght: 30cm.","EN388 : 4231         EN407 : X2XXXX      EN374-2                    food contact","7 to 11","10 units","BOX","PR",4.5381818181818181,1497.6]
[null,2094401,null,"CLEAN YELLOW. Yellow Latex glove, cotton flocked, diamond pattern. Thickness:0,4mm. Length:30cm. ","EN388 : X010       EN374-2                    ","6 to 10","10 units","BOX","PR",0.85818181818181805,283.19999999999993]
[null,2094431,null,"FINEDEX 944-31. Natural blue Latex, knitted polyamide support, pattered finish. Thickness:1.1mm. Lenght: 30cm","EN388 : 3131        EN374-2                    ","7 to 11","10 units","BOX","PR",4.6399999999999997,1531.1999999999998]
[null,2094421,null,"BLUE JERSEY GRIP . Natural blue Latex, interlock cotton support, patterned finish. Thickness:1.5mm. Length:30 cm. ","EN388 : 2121        EN374-2","6 to 11","10 units","BOX","PR",5.3818181818181818,1776]
[null,"T950FL",null,"LATEX HEAVY WEIGHT - T950FL. Heavy handling. Farming. Industrial cleaning. Chemicals, petrochemicals. Building.","EN 388 : 2111              EN 374-3 : AKL","7S, 8M, 9L, 10XL","12 units ","BOX"," PR",1.5854545454545454,523.20000000000005]
[null,"T356",null,"Latex Chlorinated, Unlined blue latex glove Chlorinated powder free treatment Curved fingers and diamond pattern for extra grip, length 30cm","EN388 : 1010        EN374-2                    ","7S, 8M, 9L, 10XL","12 units ","BOX","PR",0.96000000000000008,316.8]
[]
[null,"NITRILE - HEAVY DUTY CHEMICAL PROTECTION EN 374-3"]
[null,2095767,null,"NEW!!! MaxCoat TM, nylon liner with green nitrile coating, black grip coating on the palm, length 35cm, AQL < 0.65","EN ISO 374-1, Type B, JKL                             EN388 : 4121","7 to 11","10 units","BOX","PR",5.52,1821.6]
[null,2094831,null,"POWERCOAT® 948-31 NITRAF; Nitrile glove with cotton flock interior, pebble finish, green colour, length 33cm,  thickness 0.51mm","EN388 : 3101        EN374-3 JKL                    ","7 to 10","10 units","BOX","PR",1.9781818181818183,652.80000000000007]
[null,2095301,null,"POWERCOAT® 953-01 NITRAF; Nitrile glove with cotton flock interior, diamond-pattern finish, green colour, length 33cm,  thickness 0.4mm","EN388 : 4101        EN374-3 JKL                    ","7 to 11","10 units","BOX","PR",1.8618181818181816,614.4]
[null,2095304,null,"POWERCOAT® 953-04 NITRAF; Heavy unsupported Nitrile glove with smooth interior, diamond-pattern finish, green colour, length 45cm,  thickness 0.6mm","EN388 : 4101        EN374-3 JKL                    ","8 to 11","10 units","BOX","PR",6.2036363636363623,2047.1999999999996]
[null,"NK803",null,"NITRI KNIT . Blue nitrile. Interlock cotton lining. Length 30cm. ","EN388 : 3121        EN374-3 JKL                    ","7 to 10","12 units","BOX","PR",5.8109090909090906,1917.6]
[null,"NK804",null,"NITRI KNIT . Blue nitrile. Interlock cotton lining. Length 35cm. ","EN388 : 3111        EN374-3 JKL                    ","7 to 10","144 units","CAS","PR",6.756363636363635,2229.5999999999995]
[null,"LA132G",null,"NITRI GUARD PLUS - LA132G. Mechanical and chemical resistance to a large range of products (oils, detergents and many solvents). Preparation of greasy products, production of paints, varnishes.","EN 388 : 3101              EN 374-3  JKL","7S to 11XXL","144 units","CAS","PR",1.3818181818181816,455.99999999999994]
[]
[null,"NEOPRENE "]
[null,2095020,null,"POWERCOAT® 950-20 NEOFIT; Neoprene glove with cotton flock interior, patterned finish, black colour, length 33cm, thickness 0.60mm","EN388 : 3110        EN374-3 AKL                    ","7 to 11","10 units","BOX","PR",3.1127272727272728,1027.2]
[null,2095030,null,"POWERCOAT® 950-30 NEOFIT; Double dipped  Neoprene glove with cotton interlock base, rough finish, black with blue cuff, length 30cm, thickness 1.1mm ","EN388 : 3121        EN374-3 AKL                    ","7 to 10","10 units","BOX","PR",8.0945454545454556,2671.2000000000003]
[null,2095010,null,"POWERCOAT® 950-10 MIX-COLOR; Double-dipped Neoprene / latex glove with cotton flock interior, diamond-pattern finish, blue with yellow cuff, length 32cm, thickness 0.72mm","EN388 : 4111        EN374-3 AKL                    ","7 to 10","10 units","BOX","PR",2.2618181818181817,746.4]
[null,"BUTYL",null,null,null,null,""]
[null,2008010,null,"POWERCOAT® 080-10 BUTYL; Unsupported black Butyl® glove with rolled edge, smooth inside, length 35cm, thickness 0.5mm","EN388 : 2111        EN374-3 BKL                    ","8 to 11","10 units","BOX","PR",21.22909090909091,7005.6]
[null,"B131",null,"Butyl - Protection against aggressive chemicals like ketones (MEK, MIBK, Acetone) and Esters (Tricresyl Phosphate, Amyl Acetate, Ethyl Acetate). Gaz tight.","EN 388 : 2000                  EN 374-3  BCI","7S, 8M, 9L, 10XL","24 units","BOX","PR",32.552727272727275,10742.400000000001]
[null,"B174",null,"BUTYL B174. Protection against aggressive chemicals like ketones (MEK, MIBK, Acetone) and Esters (Tricresyl Phosphate, Amyl Acetate, Ethyl Acetate). Gaz tight.","EN388 : 2010                     ","8 to 10","1 unit","BAG ","PR",38.596363636363634,12736.8]
[null,"B131R",null,"BUTYL B131R. Protection against aggressive chemicals like ketones (MEK, MIBK, Acetone) and Esters (Tricresyl Phosphate, Amyl Acetate, Ethyl Acetate). Gaz tight.","EN388 : 2010                     ","7 to 10","1 unit","BAG ","PR",33.883636363636363,11181.6]
[null,"PVC",null,null,null,null,""]
[null,"Reusable gloves for the petrochemical industry",null,null,null,null,""]
[null,"830FWG",null,"Trawler King 830FWG ; Green PVC glove dipped on cotton liner Rough finish, thickness 1.6mm, length 27cm","EN388 : 4121        EN374-3 AKL                    ","8 to 10","12 units ","BOX"," PR",3.1781818181818178,1048.8]
[null,"850FWG",null,"Trawler King 850FWG ; Green PVC glove dipped on cotton liner Rough finish, thickness 1.6mm, length 35cm","EN388 : 4121        EN374-3 AKL                    ","8 to 10","12 units ","BOX"," PR",3.6799999999999997,1214.3999999999999]
[null,"860FWG",null,"Trawler King 850FWG ; Green PVC glove dipped on cotton liner Rough finish, thickness 1.6mm, length 40cm","EN388 : 4121        EN374-3 AKL                    ","8 to 10","12 units ","BOX"," PR",3.9854545454545458,1315.2]
[null,"T1412WG",null,"Deckhand T1412WG; Red PVC glove dipped on cotton liner Rough finish, thickness 1.4mm, length 30cm","EN388 : 4121        EN374-3 AKL                    ","8 to 11","12 units ","BOX"," PR",3.8036363636363637,1255.2]
[null,"T1612WG",null,"Pro Chem T1612WG; Red PVC glove dipped on cotton liner Rough finish, thickness 1.4mm, length 30cm","EN388 : 4121        EN374-3 AKL                    ","8 to 11","12 units ","BOX"," PR",3.9854545454545458,1315.2]
[null,"PVC MECHANICAL MAINBIS",null,null,null,null,""]
[null,"R30X",null,"REDCOTE PLUS R30X. Handling in an aggressive environment: oils, greases, chemicals, hydrocarbons. Chemical and petrochemical industry.Red PVC glove Dipped on cotton liner Smooth finish","EN388 : 4121        EN374-3 AKL                    ","9L, 10XL","12 units ","BOX"," PR",3.5345454545454547,1166.4000000000001]
[null,"R50X",null,"REDCOTE PLUS - R50X. Handling in an aggressive environment: oils, greases, chemicals, hydrocarbons. Chemical and petrochemical industry.","EN388 : 4121        EN374-3 AKL                    ","9L, 10XL","12 units ","BOX"," PR",4.1018181818181816,1353.6]
[null,"R60X",null,"REDCOTE PLUS – R60X. Handling in an aggressive environment: oils, greases, chemicals, hydrocarbons. Chemical and petrochemical industry.","EN388 : 4121        EN374-3 AKL                    ","9L, 10XL","12 units ","BOX"," PR",4.1018181818181816,1353.6]
[]
[null,"PVC MECHANICAL MAINGRIP",null,null,null,null,""]
[null,2006330,null,"REDGRIP KN 27G; Red PVC gauntlet with rough finish, length 27cm, thickness 1.3mm","EN388 : 3121        EN374-3                    ","7 to 11","100 units","CAS","PR",2.8509090909090906,940.8]
[null,"LATEX/ NITRILE FOR CONTROLLED ENVIRONMENT"]
[null,"CE412W",null,"Chemsoft CE. Nitrile white, non powered. Thicness 0,12mm. Lenght 30cm.","EN374-2","XS to XL","100 units","BAG","BAG",23.556363636363635,7773.5999999999995]
[null,"Ak1815O",null,"AK. Natural Latex, non powdered, patterned finish. Thickness:0,50mm. Lenght 38cm.","EN388 : 2110        EN374-3 AKL                   ","8 to 11","100 units","CAS","PR ",2.916363636363636,962.39999999999986]
[null,"Hand Protection |  ELECTRICAL PROTECTION",null,null,null,null,""]
[null,"ELECTRICAL PROTECTION -  ELECTROSOFT RED LATEX"]
[null,"Dielectric latex gloves to protect against electrical risks from 500 to 36000 volts. Version in cut edge or rolled edge. Need over glove for mechanical protection."]
[]
[null,2091083,null,"NEW!!! ELECTROSOFT RED CLASS 00. For electrical work with a maximum voltage of 500 volts. Must be used with a leather overglove.","\nEN 60903-2003\nCEI 903-2002","7 to 11","1 pair ","PR","PR",17.65818181818182,5827.2000000000007]
[null,2091084,null,"NEW!!! ELECTROSOFT RED CLASS 0.For electrical work with a maximum voltage of 1000 volts. Must be used with a leather overglove.","EN 60903-2003\nCEI 903-2002","8 to 11","1 pair ","PR","PR",24.247272727272726,8001.5999999999995]
[null,2091085,null,"NEW!!! ELECTROSOFT RED CLASS 1. For electrical work with a maximum voltage of 7500 volts. Must be used with a leather overglove","EN 60903-2003\nCEI 903-2002","8 to 11","1 pair ","PR","PR",33.607272727272722,11090.399999999998]
[null,2091086,null,"NEW!!! ELECTROSOFT RED CLASS 2.For electrical work with a maximum voltage of 17000 volts. Must be used with a leather overglove.","EN 60903-2003\nCEI 903-2002\n","8 to 11","1 pair ","PR","PR",38.007272727272721,12542.399999999998]
[null,2091087,null,"NEW!!! ELECTROSOFT RED CLASS 3. For electrical work with a maximum voltage of 26500 volts. Must be used with a leather overglove.","EN 60903-2003\nCEI 903-2002","9 to 11","1 pair ","PR","PR",50.370909090909088,16622.399999999998]
[null,"ELECTROSOFT - ELECTRICAL PROTECTION",null,null,null,null,""]
[null,"NEW!!! ELECTROSOFT BICOLOR - Dielectric latex gloves to protect against electrical risks from 500 to 36000 volts. Version in cut edge. Bicolor (red outside, beige inside) for easier and "]
[null,"faster dectection of defects during visual inspection. Need over glove for mechanical protection."]
[]
[null,2091073,null,"ELECTROSOFT BICOLOR CLASS 00\nFor electrical work with a maximum voltage of 500 volts. Recommended to be used in conjunction with leather protector for mechanical protection. Bicolor for easier detection of defects before use (i.e. accidental cuts, perforations, abrasions..)","EN 60903-2003\nCEI 903-2002","7 to 12 ","1 pr","PR","PR ",19.04,6283.2]
[null,2091074,null,"ELECTROSOFT RED CLASS 0\nFor electrical work with a maximum voltage of 1000 volts. Must be used with a leather overglove.Bicolor for easier detection of defects before use (i.e. accidental cuts, perforations, abrasions..)","EN 60903-2003","8 to 12 ","1 pr","PR","PR ",26.152727272727272,8630.4]
[null,2091075,null,"ELECTROSOFT BICOLOR CLASS 1\nFor electrical work with a maximum voltage of 7500 volts. Must be used with a leather overglove. 41 cm lenght, Thickness: 1,5 mm","EN 60903-2003\nCEI 903-2002","8 to 12 ","1 pr","PR","PR ",35.665454545454537,11769.599999999997]
[null,2091076,null,"ELECTROSOFT BICOLOR CLASS 2\nFor electrical work with a maximum voltage of 17000 volts. Must be used with a leather overglove. Lenght: 41cm, Thickness:2,3 mm","EN 60903-2003\nCEI 903-2002","8 to 12 ","1 pr","PR","PR ",40.981818181818177,13523.999999999998]
[null,2091077,null,"ELECTROSOFT BICOLOR CLASS 3\nFor electrical work with a maximum voltage of 26500 volts. Must be used with a leather overglove. Thickness 2,9mm, Length: 41 cm ","EN 60903-2003\nCEI 903-2002","8 to 12 ","1 pr","PR","PR ",54.319999999999993,17925.599999999999]
[null,2091078,null,"ELECTROSOFT BICOLOR CLASS 4\nHandling of high voltage to 36 000 volts. Must be used with a leather overglove. Thickness 3,4 mm, Lenght 41 cm. ","EN 60903-2003\nCEI 903-2002","8 and 12 ","1 pr","PR","PR ",104.43636363636362,34463.999999999993]
[]
[]
[null,"ISOARC - electrical and arc flash protection in one glove",null,null,null,null,""]
[null,2092002,null,"ISOARC, Class 0, Operating voltage 1000 V AC,Lenght 360mm, category RC, chlorine patterned palm. ","EN60903\nCEI903","7 to 11","1 unit","","PR",43.236363636363635,14268]
[null,2092015,null,"ELECTROSOFT COMPOSITE FLOCKED Class 0. nterior flocked cotton. Patterned finishes: good grip in damp conditions. Protection from electric arc in the event of a short circuit. Flocked patterned palm.Operating voltage: 1000 V AC. Length: 360mm.","Category RC","7 to 11","1 unit","","PR",49.956363636363626,16485.599999999995]
[null,"COMPOSITE - Can be used without an overglove",null,null,null,null,""]
[]
[null,2092012,null,"ELECTROSOFT COMPOSITE FLOCKED.  Interior flocked cotton. Patterned finishes: good grip in damp conditions. Protection from electric arc in the event of a short circuit. Flocked patterned palm. Class 00. Operating voltage: 500 V AC.  Length: 360mm.","Category RC","7 to 11","1 unit","","PR",43.010909090909088,14193.599999999999]
[null,2092011,null,"ELECTROSOFT COMPOSITE FLOCKED. Class 00 Interior flocked cotton. Patterned finishes: good grip in damp conditions. Protection from electric arc in the event of a short circuit. Flocked patterned palm. Class 00. Operating voltage: 500 V AC.  Length: 360mm.","Category RC","7 to 11","1 unit",null,"PR ",36.516363636363636,12050.4]
[null,"LATEX - Cut edge beige latex glove",null,null,null,null,""]
[null,2091906,null,"Class 0 glove for electrical work with a maximum of 1000V, use with protective overglove: 2012897, 410mm","EN60903\nCEI903","8 to 11","1 unit","","PR",24.210909090909087,7989.5999999999985]
[null,2091903,null,"ELECTROSOFT. Electrosoft Latex isolating gloves.Natural Latex base offers excellent dialectric characteristics. An ergonomic design increases comfort by providing additional softness and allows the glove to be put on and taken off very easily. Class 00, Operating voltage: 500V AC, Length: 360 mm. Colour: beige.","EN60903\nCEI904","7 to 11","1 unit","","PR",17.621818181818181,5815.2]
[null,2091907,null,"Class 0 glove for electrical work with a maximum of 1000V, use with protective overglove: 2012897","EN60903\nCEI905","8 to 11","1 unit","","PR",23.789090909090906,7850.3999999999987]
[null,2091911,null,"Class 1 glove for electrical work with a maximum of 7.5KV,  use with protective overglove: 2012898, 410mm","EN60903\nCEI906","8 to 11","1 unit","","PR",34.741818181818182,11464.8]
[null,2091912,null,"Class 1 glove for electrical work with a maximum of 7.5KV,  use with protective overglove: 2012898","EN60903\nCEI903","8 to 11","1 unit","","PR",32.530909090909084,10735.199999999997]
[null,2090221,null,"Class 2 glove for electrical work with a maximum of 17KV, use with protective overglove: 2012899, 410mm","EN60903\nCEI903","8 to 11","1 unit","","PR",39.127272727272725,12912]
[null,2091921,null,"Class 2 glove for electrical work with a maximum of 17KV, use with protective overglove: 2012899","EN60903\nCEI903","8 to 11","1 unit","","PR",36.632727272727266,12088.799999999997]
[null,2090231,null,"Class 3 glove for electrical work with a maximum of 26.5KV, use with protective overglove: 2012899","EN60903\nCEI903","9 to 11","1 unit","","PR",51.490909090909078,16991.999999999996]
[null,2091931,null,"Class 3 glove for electrical work with a maximum of 26.5KV, use with protective overglove: 2012899","EN60903\nCEI903","8 to 11","1 unit","","PR",47.447272727272718,15657.599999999997]
[null,2091941,null,"Class 4 glove for electrical work with a maximum of 36KV, use with protective overglove: 2012899","EN60903\nCEI903","8 to 11","1 unit","","PR",96.84363636363635,31958.399999999994]
[null,"LATEX - Rolled edge two-tone gloves comprise beige exterior and black interior to allow damage to be identified immediately"]
[null,2091908,null,"Class 0 glove for electrical work with a maximum of 1000V, use with protective overglove: 2012897","EN60903\nCEI903","9 to 11","1 unit","","PR",47.876363636363628,15799.199999999997]
[null,2091913,null,"Class 1 glove for electrical work with a maximum of 7.5KV,  use with protective overglove: 2012898","EN60903\nCEI903","9 to 11","1 unit","","PR",55.025454545454537,18158.399999999998]
[null,2091922,null,"Class 2 glove for electrical work with a maximum of 17KV, use with protective overglove: 2012899","EN60903\nCEI903","9 to 11","1 unit","","PR",66.909090909090907,22080]
[null,2091932,null,"Class 3 glove for electrical work with a maximum of 26.5KV, use with protective overglove: 2012899","EN60903\nCEI903","9 to 11","1 unit","","PR",77.679999999999993,25634.399999999998]
[null,2091942,null,"Class 4 glove for electrical work with a maximum of 36KV, use with protective overglove: 2012899","EN60903\nCEI903","10, 11","1 unit","","PR",113.6509090909091,37504.800000000003]
[null,"COMPOSITE GLOVES"]
[null,2092013,null,"ELECTROSOFT COMPOSITE Class 00. For electrical work with a maximum voltage of 500 volts. Can be used without overglove.","Category RC","7 to 11","1 unit","","PR",46.29818181818181,15278.399999999998]
[null,2092014,null,"ELECTROSOFT COMPOSITE FLOCKE. Operating voltage: 1000 V AC. Length: 360mm.","Category RC","7 to 11","1 unit","","PR",43.236363636363635,14268]
[null,2092016,null,"ELECTROSOFT COMPOSITE FLOCKE. Operating voltage: 1000 V AC. Length: 410mm.","Category RC","7 to 11","1 unit","","PR",53.425454545454535,17630.399999999998]
[null,2092017,null,"ELECTROSOFT COMPOSITE FLOCKED. Operating voltage: 7500 V AC, Length: 410mm.","Category RC","9 to  11","1 unit","","PR",54.559999999999995,18004.8]
[null,2092027,null,"ELECTROSOFT COMPOSITE FLOCKED. Operating voltage: 17000 V AC, Length: 410mm.","Category RC","9 to  11","1 unit","","PR",66.087272727272733,21808.800000000003]
[null,2092028,null,"ELECTROSOFT COMPOSITE Class 2",null,"9 to  11","1 unit","","PR",62.938181818181818,20769.599999999999]
[null,2090220,null,"Electrosoft Long composite gloves, 800mm, Class 2, 17000 V AC, category RC","Category RC","9, 10","1 unit","","PR",454.63272727272721,150028.79999999999]
[null,"COMPLEMENTARY PRODUCTS"]
[null,"OVERGLOVE"]
[null,2012897,null,"Overglove provides mechanical resistance for use with Electrosoft Electricians gloves, LT 2.5kV/5kV","EN388 2121","8 to 11","1 unit","","PR",15.207272727272725,5018.3999999999996]
[null,2012898,null,"Overglove provides mechanical resistance for use with Electrosoft Electricians gloves, MT 10kV","EN388 2121","8 to 11","1 unit","","PR",15.207272727272725,5018.3999999999996]
[null,2012899,null,"Overglove provides mechanical resistance for use with Electrosoft Electricians gloves, HT 20kV/30kV","EN388 2121","8 to 11","1 unit","","PR",15.207272727272725,5018.3999999999996]
[null,"G100",null,"Gloves inflator",null,null,"1 unit","","EA",303.06181818181813,100010.39999999998]
[null,"2092999.00",null,"Plastic box for electro gloves",null,null,"1 ea","EA","EA",8.82909090909091,2913.6000000000004]
[]
[null,"Hand Protection |  GLOVEBOX"]
[null,"DRYBOX NEOPRENE "]
[null,"5N1532/9Q",null,null,null,null,"1 pair","PR","PR",170.19636363636363,56164.799999999996]
[null,"6N1532/9Q",null,null,null,null,"1 pair","PR","PR",221.23636363636362,73008]
[null,"N6N1532A/9Q",null,null,null,null,"1 pair","PR","PR",223.87636363636361,73879.199999999997]
[null,"7N1532A/8H",null,null,null,null,"2 pairs ","BOX","PR",189.83272727272725,62644.799999999996]
[null,"N7N1532A/9Q",null,null,null,null,"2 pairs ","CAS ","PR",189.83272727272725,62644.799999999996]
[null,"N8N1532/8H",null,null,null,null,"2 pairs ","BOX","PR",216.01454545454541,71284.799999999988]
[null,"N8N1532/9Q",null,null,null,null,"2 pairs ","BOX","PR",216.01454545454541,71284.799999999988]
[null,"N8N1532/10H",null,null,null,null,"2 pairs ","BOX","PR",222.37090909090904,73382.39999999998]
[null,"N8N1532A/9Q",null,null,null,null,"2 pairs ","BOX","PR",222.37090909090904,73382.39999999998]
[null,"N8N1532A/10H",null,null,null,null,"1 pair","PR","PR",222.37090909090904,73382.39999999998]
[null,"N10N1532A/9Q",null,null,null,null,"1 pair","PR","PR",274.93090909090904,90727.199999999983]
[null,"6N3032/9Q",null,null,null,null,"1 pair","PR","PR",238.17454545454544,78597.599999999991]
[null,"6N3032A/9Q",null,null,null,null,"1 pair","PR","PR",242.20363636363632,79927.199999999983]
[null,"N8N3032/8H",null,null,null,null,"1 pair","PR","PR",273.58545454545452,90283.199999999997]
[null,"N8N3032/9Q",null,null,null,null,"1 pair","PR","PR",273.58545454545452,90283.199999999997]
[null,"N8N3032/10H",null,null,null,null,"2 pairs ","BOX","PR",273.58545454545452,90283.199999999997]
[null,"N8N3032/9QEU",null,null,null,null,"1 pair","PR","PR",273.58545454545452,90283.199999999997]
[null,"N8N3032A/9Q",null,null,null,null,"2 pairs ","BOX","PR",265.76727272727271,87703.2]
[null,"10N3032A/9Q",null,null,null,null,"1 pair","PR","PR",391.76727272727271,129283.2]
[]
[null,"DRYBOX CSM"]
[null,"N5Y1532A/9Q",null,null,null,null,"1 pair","PR","PR",212.69818181818181,70190.399999999994]
[null,"6Y1532/9Q",null,null,null,null,"1 pair","PR","PR",218.88727272727272,72232.800000000003]
[null,"N6Y1532A/9Q",null,null,null,null,"2 pairs ","BOX","PR",218.88727272727272,72232.800000000003]
[null,"N7Y1532/9Q",null,null,null,null,"2 pairs ","BOX","PR",226.25454545454545,74664]
[null,"7Y1532A/8H",null,null,null,null,"2 pairs ","BOX","PR",226.25454545454545,74664]
[null,"N7Y1532A/9Q",null,null,null,null,"2 pairs ","BOX","PR",226.25454545454545,74664]
[null,"N8Y1532/8H",null,null,null,null,"1 pair","PR","PR",239.51272727272723,79039.199999999983]
[null,"N8Y1532/9Q",null,null,null,null,"2 pairs ","BOX","PR",239.51272727272723,79039.199999999983]
[null,"N8Y1532/10H",null,null,null,null,"1 pair","PR","PR",239.51272727272723,79039.199999999983]
[null,"N8Y1532A/9Q",null,null,null,null,"2 pairs ","BOX","PR",239.51272727272723,79039.199999999983]
[null,"N8Y1532A/10H",null,null,null,null,"2 pairs ","BOX","PR",239.51272727272723,79039.199999999983]
[null,"N8Y1532AAWE",null,null,null,null,"2 pairs ","BOX","PR",239.51272727272723,79039.199999999983]
[null,"10Y1532ALC/9Q",null,null,null,null,"1 pair","PR","PR",337.09090909090907,111239.99999999999]
[null,"6Y3032A/9Q",null,null,null,null,"1 pair","PR","PR",175.95636363636362,58065.599999999991]
[null,"7Y3032/9Q",null,null,null,null,"2 pairs ","BOX","PR",353.48363636363638,116649.60000000001]
[null,"N8Y3032/8H",null,null,null,null,"1 pair","PR","PR",375.5272727272727,123923.99999999999]
[null,"N8Y3032/9Q",null,null,null,null,"2 pairs ","CAS ","PR",375.5272727272727,123923.99999999999]
[null,"N8Y3032/10H",null,null,null,null,"1 pair","PR","PR",375.5272727272727,123923.99999999999]
[null,"N8Y3032A/9Q",null,null,null,null,"1 pair","PR","PR",375.5272727272727,123923.99999999999]
[null,"N8Y3032A/10H",null,null,null,null,"1 pair","PR","PR",375.5272727272727,123923.99999999999]
[null,"10Y3032A/9Q",null,null,null,null,"1 pair","PR","PR",541.38909090909078,178658.39999999997]
[]
[null,"DRYBOX BUTYL"]
[null,"5B1532/9Q",null,null,null,null,"1 pair ","PR","PR",148.78545454545454,49099.199999999997]
[null,"N5B1532A/9Q",null,null,null,null,"1 pair ","PR","PR",150.56,49684.800000000003]
[null,"N6B1532/9Q",null,null,null,null,"2 pairs ","BOX","PR",150.56,49684.800000000003]
[null,"N6B1532A/9Q",null,null,null,null,"2 pairs ","CAS ","PR",150.56,49684.800000000003]
[null,"N7B1532/9Q",null,null,null,null,"2 pairs ","BOX","PR",159.03272727272724,52480.799999999988]
[null,"7B1532A/8H",null,null,null,null,"1 pair ","PR","PR",154.48727272727271,50980.799999999996]
[null,"N7B1532A/9Q",null,null,null,null,"2 pairs ","BOX","PR",154.48727272727271,50980.799999999996]
[null,"N8B1532/8H",null,null,null,null,"2 pairs ","BOX","PR",163.64363636363635,54002.399999999994]
[null,"N8B1532/9Q",null,null,null,null,"2 pairs ","BOX","PR",168.4581818181818,55591.199999999997]
[null,"N8B1532/10H",null,null,null,null,"2 pairs ","BOX","PR",163.64363636363635,54002.399999999994]
[null,"N8B1532A/9Q",null,null,null,null,"2 pairs ","BOX","PR",163.64363636363635,54002.399999999994]
[null,"N8B1532A/10H",null,null,null,null,"2 pairs ","BOX","PR",163.64363636363635,54002.399999999994]
[null,"N10B1532A/9Q",null,null,null,null,"2 pairs ","BOX","PR",216.01454545454541,71284.799999999988]
[null,"10B2032A/9Q",null,null,null,null,"1 pair ","PR","PR",235.59999999999997,77747.999999999985]
[null,"N5B3032/9Q",null,null,null,null,"2 pairs ","BOX","PR",173.84727272727272,57369.599999999999]
[null,"N7B3032/9Q",null,null,null,null,"1 pair ","PR","PR",175.43272727272725,57892.799999999996]
[null,"N7B3032A/9Q",null,null,null,null,"2 pairs ","BOX","PR",175.43272727272725,57892.799999999996]
[null,"N8B3032/8H",null,null,null,null,"2 pairs ","BOX","PR",202.92363636363635,66964.799999999988]
[null,"N8B3032/9Q",null,null,null,null,"2 pairs ","BOX","PR",202.92363636363635,66964.799999999988]
[null,"N8B3032/10H",null,null,null,null,"2 pairs ","BOX","PR",202.92363636363635,66964.799999999988]
[null,"N8B3032A/9Q",null,null,null,null,"2 pairs ","BOX","PR",202.92363636363635,66964.799999999988]
[null,"8B3032A/10H",null,null,null,null,"1 pair ","PR","PR",202.92363636363635,66964.799999999988]
[null,"10B3032A/9Q",null,null,null,null,"1 pair ","PR","PR",260.5236363636364,85972.800000000017]
[]
[null,"DRYBOX LED LOADED "]
[null,"8NLL3032/8H",null,null,null,null,"1 pair ","PR","PR",582.20363636363629,192127.19999999998]
[null,"8NLL3032/9Q",null,null,null,null,"1 pair ","PR","PR",589.13454545454533,194414.39999999997]
[null,"8NLL3032/10H",null,null,null,null,"1 pair ","PR","PR",582.20363636363629,192127.19999999998]
[]
[null,"DRYBOX CSM/NEOPRENE LED LOADED"]
[null,"N7NLY3032A/9Q",null,null,null,null,"1 pair ","PR","PR",467.34545454545452,154224]
[null,"8NLY3032/8M",null,null,null,null,"2 pairs ","BOX","PR",476.11636363636353,157118.39999999997]
[null,"8NLY3032/9Q",null,null,null,null,"2 pairs ","BOX","PR",481.78181818181815,158988]
[null,"8NLY3032/10H",null,null,null,null,"2 pairs ","BOX","PR",476.11636363636353,157118.39999999997]
[null,"8NLY3032A",null,null,null,null,"1 pair ","PR","PR",473.78181818181821,156348]
[]
[null,"DRYBOX CSM LED LOADED"]
[null,"N6YLY3032A/9Q",null,null,null,null,"1 pair ","PR","PR",445.12727272727267,146891.99999999997]
[null,"N7YLY3032/9Q",null,null,null,null,"1 pair ","PR","PR",500.10909090909087,165036]
[null,"7YLY3032A",null,null,null,null,"1 pair ","PR","PR",491.28727272727269,162124.79999999999]
[null,"8YLY3032A",null,null,null,null,"2 pairs ","BOX","PR",508.4581818181818,167791.19999999998]
[]
[null,"DRYBOX NEOPRENE SHORT"]
[null,"N103A/7",null,null,null,null,"1 pair ","PR","PR",65.454545454545439,21599.999999999996]
[null,"N103A/9",null,null,null,null,"2 pairs ","BOX","PR",65.454545454545439,21599.999999999996]
[null,"N103A/10",null,null,null,null,"2 pairs ","BOX","PR",65.454545454545439,21599.999999999996]
[]
[null,"DRYBOX CSM SHORT"]
[null,"Y103/8",null,null,null,null,"1 pair ","PR","PR",60.218181818181812,19871.999999999996]
[null,"Y154A/7",null,null,null,null,"1 pair ","PR","PR",65.454545454545439,21599.999999999996]
[null,"Y154A/8",null,null,null,null,"2 pairs ","BOX","PR",65.454545454545439,21599.999999999996]
[null,"Y154A/9",null,null,null,null,"2 pairs ","BOX","PR",65.454545454545439,21599.999999999996]
[null,"Y154A/10",null,null,null,null,"1 pair ","PR","PR",65.454545454545439,21599.999999999996]
[null,"Y254A/7",null,null,null,null,"1 pair ","PR","PR",65.679999999999993,21674.399999999998]
[null,"Y254A/8M",null,null,null,null,"2 pairs ","BOX","PR",65.679999999999993,21674.399999999998]
[null,"Y254A/9L",null,null,null,null,"2 pairs ","BOX","PR",65.679999999999993,21674.399999999998]
[null,"Y254A/10",null,null,null,null,"2 pairs ","BOX","PR",65.679999999999993,21674.399999999998]
[]
[null,"CSM SLEEVE "]
[null,"YSL2027",null,null,null,null,"2 pairs ","BOX","EA",161.88363636363636,53421.599999999999]
[]
[null,"DRYBOX NITRILE"]
[null,"8LA1832A/9Q",null,null,null,null,"5 pairs","BOX","PR",191.43272727272728,63172.800000000003]
[null,"10LA1832A/10H",null,null,null,null,"5 pairs","BOX","PR",284.78545454545451,93979.199999999983]

{"sheet":"Footwear ","index":6,"n_rows":159,"n_cols":12,"rows_kept":159,"cut":false,"hidden":false,"merged":[[116,1,116,3],[34,1,34,8],[48,1,48,4],[69,1,69,2],[90,1,90,3],[96,1,96,3],[109,1,109,3],[33,1,33,3],[0,1,0,3],[4,1,4,8],[11,1,11,3],[12,1,12,8],[17,1,17,2]]}
[null,"Safety Footwear |  NEW PRODUCTS INTRODUCTION",null,null,null,null,""]
[null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per",null,"NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,"Global Footwear OPTIMA range",null,null,null,null,""]
[null,"Optima range, safety with comfort on all surafacess, perfectly adapted to hot, dry environments, and some models ideal for humid outdoor environments and unever terrain."]
[null,6200673,null,"GFW LIDER (S1P CI SRC)\nGrey perforated suede upper and textile, PU2D outsole injected, 200J Premium™ toe cap in injected polymer, Flexium metal free anti-puncture midsole","EN ISO\n20345: 2011\nS1P CI SRC","35 to 47","1 unit","BOX","PR",null,41.080984848484846,13556.724999999999]
[null,6200674,null,"GFW BRAVO (S1P CI SRC)\nBeige perforated suede upper and textile, PU2D outsole injected, 200J Premium™ toe cap in injected polymer, Flexium metal free anti-puncture midsole","EN ISO\n20345: 2011\nS1P CI SRC","35 to 47","1 unit","BOX","PR",null,41.080984848484846,13556.724999999999]
[null,6200675,null,"GFW GRIP (S1P CI SRC)\nBeige perforated suede upper and textile, PU2D outsole injected, 200J Premium™ toe cap in injected polymer, Flexium metal free anti-puncture midsole","EN ISO\n20345: 2011\nS1P CI SRC","35 to 47","1 unit","BOX","PR",null,42.87143939393939,14147.574999999999]
[null,6200670,null,"GFW LEON (S3 CI SRC)\nFull grain S3 water repellent leather with reflective bands, PU2D outsole injected, 200J Premium™ toe cap in injected polymer, Flexium metal free anti-puncture midsole","EN ISO\n20345: 2011\nS3 CI SRC","35 to 47","1 unit","BOX","PR",null,41.080984848484846,13556.724999999999]
[null,6200671,null,"GFW JAGUAR (S3 CI SRC)\nFull grain S3 water repellent leather with reflective bands, PU2D outsole injected, 200J Premium™ toe cap in injected polymer, Flexium metal free anti-puncture midsole","EN ISO\n20345: 2011\nS3 CI SRC","35 to 47","1 unit","BOX","PR",null,44.654242424242419,14735.899999999998]
[null,6200672,null,"GFW LINCE (S3 CI SRC)\nFull grain S3 water repellent leather with reflective bands, PU2D outsole injected, 200J Premium™ toe cap in injected polymer, Flexium metal free anti-puncture midsole. Bellows and spark resistant flap held in place by a self- adhesive strip.","EN ISO\n20345: 2011\nS3 CI SRC","35* to 47 ( 35 to 37 by special order)","1 unit","BOX","PR",null,44.654242424242419,14735.899999999998]
[null,"AIRFIRE footwear range"]
[null,"Honeywell has developed a new range of technical footwear specially designed to meet the needs of firefighters' during rescue and emergency work"]
[null,6246280,null,"FIREPRO (F2A HI3 SRC)\nPremium full grain leather, waterproof and breathable Sympatex®  Moisture Tech membrane, 200 J non metallic toe cap, anti-picture midsole.","EN 15090:2012 and F2A HI3 CI SRC  and ASQUAL certified VEPSP branded","38 to 48","1 unit","BOX","PR",null,178.62462121212118,58946.124999999993]
[null,6246281,null,"FIRESTORM (F2A HI3 SRC)\nPremium full grain leather, waterproof and breathable Sympatex®  Moisture Tech membrane, 200 J non metallic toe cap, anti-picture midsole ","EN 15090:2012 and F2A HI3 CI SRC  and ASQUAL certified VEPSP branded","38 to 48","1 unit","BOX","PR",null,186.39090909090908,61508.999999999993]
[null,6246282,null,"FIREFAST (F2A HI3 SRC)\nPremium full grain leather, 3D technical and innovative lining ( Eucalyptus treated) , 200 J non metallic toe cap, anti-picture midsole ","EN 15090:2012 and F2A HI3 CI SRC  and ASQUAL certified VEPSP branded","38 to 48","1 unit","BOX","PR",null,170.85833333333335,56383.250000000007]
[null,6246283,null,"FIRETRIAL (F1PA HI3 SRC)\nPremium full grain leather, 3D technical and innovative lining ( Eucalyptus treated) , soft toe resistant to 500N non metallic, flexible and light.","EN 15090:2012 and F1PA HI3  R CI SRC  and ASQUAL certified VEPSP branded","38 to 48","1 unit","BOX","PR",null,170.85833333333335,56383.250000000007]
[null,"(i)XTREM Range "]
[null,"The new (i)XTREM range is based on a brand new PU /Nitrile outsole. Intergating the latest technologies."]
[null,"This new range is designed for the hardest and most difficult environments."]
[]
[null,6246212,null,"Quad (i)XTREM S3 HRO HI CI SRC. Mid Full grain leather upper. Ankle foam comfort. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.","EN ISO 20345: 2011 S3 CI SRC","35 to 49","1 unit","BOX","PR",null,87.992424242424249,29037.500000000004]
[null,6246201,null,"HIKE (i)XTREM S3 HRO HI CI SRC.Brown full grain leather shoe.Non metallic safety components.PU/Nitrile outsole..A strong upper construction with an innovative outsole for extrem performances. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.","EN ISO 20345: 2011 S3 CI SRC","35 to 49","1 unit","BOX","PR",null,82.536893939393934,27237.174999999999]
[null,6246202,null,"COLLECT (i)XTREM S3 HRO HI CI SRC\nMid Full grain leather upper.Non metallic safety element.\nPU/Nitril outsole.Smartium toe cap in injected polymer. Non metallic, 50% lighter than style with a thin design.Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.","EN ISO 20345: 2011 S3 CI SRC","37 to 48","1 unit","BOX","PR",null,97.319621212121191,32115.474999999995]
[null,6246210,null,"COLLECT ICE (i)XTREM S3 HRO HI CI SRC. Mid Full grain leather upper.Thermal insulation lining.\nNon metallic safety element.\nPU/Nitril outsole.","EN ISO 20345: 2011 S3 CI SRC","37 to 48","1 unit","BOX","PR",null,118.04757575757576,38955.699999999997]
[null,6246203,null,"FORCE (i)XTREM S3 HRO HI CI SRC\nBlack full grain leather shoe.Non metallic  footwear.\nPU/Nitrile outsole","EN ISO 20345: 2011 S3 CI SRC","37 to 48","1 unit","BOX","PR",null,70.003712121212118,23101.224999999999]
[null,6246204,null,"PROTECT (i)XTREM S3 HRO HI CI SRC\nBlack full grain leather shoe.\nNon metallic footwear.\nPU/Nitrile outsole.","EN ISO 20345: 2011 S3 CI SRC","37 to 48","1 unit","BOX","PR",null,75.023106060606054,24757.624999999996]
[null,"New Products - Urban Line Extension!"]
[null,6244416,null,"REPORTER S3 CI SRC. Full grain calf leather upper, 3D Lining, padded ankle collar. 100% metal free. PU double density outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.","EN ISO 20345: 2011 S3 CI SRC","35-49","1 unit ","BOX","PR",null,56.506439393939388,18647.124999999996]
[null,6244411,null,"PIONEER S3 CI SRC. Water resistan nubuck outer layer, 3D Lining, padded ankle collar. 100% metal free. PU double density outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.","EN ISO 20345: 2011 S3 CI SRC","35-49","1 unit ","BOX","PR",null,65.114393939393935,21487.75]
[null,6244413,null,"PIONEER BLACK S3 CI SRC. Full grain calf leather upper, 3D Lining, padded ankle collar. 100% metal free. PU double density outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.","EN ISO 20345: 2011 S3 CI SRC","35-49","1 unit ","BOX","PR",null,70.393939393939391,23230]
[null,6244456,null,"EXPLORER RIPPER (S3 CI SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, water-resistant full grain leather upper  with Cordura® Flexible reinforcements, Poromax® 3D lining, removable antistatic, antibacterial insole","EN ISO 20345: 2011 S3 CI SRC","35-49","1 unit ","BOX","PR",null,87.112499999999997,28747.125]
[null,6244457,null,"FLYER RIPPER (S3 CI SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, water-resistant full grain leather upper  with Cordura® Flexible reinforcements, Poromax® 3D lining, removable antistatic, antibacterial insole","EN ISO 20345: 2011 S3 CI SRC","35-49","1 unit ","BOX","PR",null,77.961287878787871,25727.224999999999]
[null,"Oil & Gas footwear range"]
[null,"This new range is dedicated to the oil and gas industry. The premium raw materials have been selected to guarantee the best protection in harsh and tough environments, the non-metallic toe cap and anti-puncture midsole ensure lightness and thermal insulation, while the injected outsole brings flexibility and slip resistance on any surface."]
[null,6246220,null,"SYNERGIC S3 CI HI SRC.  Water resistant full grain leather upper.Poromax® 3D lining : breathable, absorbent, fast drying. Padded and ergonomic collar.PU coated microfibre scuff cap.Reflective piping at the heel. Specific patterns for improved fluid evacuation. PU2D Injected outsole.","EN ISO 20345: 2011 S3 CI SRC","35-49 ",1,"BOX ","PR ",null,77.05840909090908,25429.274999999998]
[null,6246221,null,"ENERGIC S3 CI HI SRC.  Water resistant full grain leather upper. Poromax® 3D lining : breathable, absorbent, fast drying. Padded and ergonomic collar. PU coated microfibre scuff cap. Lace and lateral zipper with watertight bellows. Specific patterns for improved fluid evacuation. PU 2D Injected outsole.","EN ISO 20345: 2011 S3 CI SRC","35-49 ",1,"BOX ","PR ",null,104.24424242424243,34400.6]
[null,6246222,null,"XPLORE S3 HRO CI HI SRC.  Water resistant full grain leather upper. Poromax® 3D lining : breathable, absorbent, fast drying. Padded and ergonomic collar. PU coated microfibre scuff cap. Lace and lateral zipper with watertight bellows. Specific patterns for improved fluid evacuation. PU/NItril Injected outsole.","EN ISO 20345: 2011 S3 CI SRC","37-48",1,"BOX ","PR ",null,110.87045454545455,36587.25]
[null,"EXECUTIVE footwear range"]
[null,"The new Executive range of footwear has been developped in the pure shoemaking tradition. A new last designed to provide the best comfort with the finest style."]
[null,6543019,null,"EPIK S1P SRC. Brown Microfiber upper. No lining. 100% non metallic footwear. Cemented PU outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility. Smartium toe cap in injected polymer. Non metallic, 50% lighter than style with a thin design. ","EN ISO 20345:2011","38-48","1 unit","BOX","PR",null,67.807727272727277,22376.550000000003]
[null,6543020,null,"ELIPSE S1P CI SRC. Brown Microfiber upper. No lining. 100% non metallic footwear. Cemented PU outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility. Padded ankle collar. Smartium toe cap in injected polymer. Non metallic, 50% lighter than style with a thin design. ","EN ISO 20345:2011","38-48","1 unit","BOX","PR",null,67.807727272727277,22376.550000000003]
[null,6543010,null,"BACOU ERRO (S3 CI SRC)\nBlack brogue shoe with smooth full grain leather upper, fully lined in leather, 200 Joule non-metallic toe cap, non-metallic puncture resistant midsole, non-magnetic","EN ISO 20345: 2011 S3 CI SRC","38 to 48","1 unit","BOX","PR",null,62.558787878787882,20644.400000000001]
[null,6543011,null,"BACOU ENRO (S3 CI SRC)\nBlack Oxford lace up ankle boot with smooth full grain leather upper, fully lined in leather, black loop to pull on/off, 200 Joule non-metallic toe cap, non-metallic puncture resistant midsole, non-magnetic","EN ISO 20345: 2011 S3 CI SRC","38 to 48","1 unit","BOX","PR",null,71.962499999999991,23747.624999999996]
[null,6543012,null,"BACOU EXCEPTIO (S3 CI SRC)\nBlack Chelsea boot with smooth full grain leather upper, fully lined in leather, black loop to pull on/off, 200 Joule non-metallic toe cap, non-metallic puncture resistant midsole, non-magnetic","EN ISO 20345: 2011 S3 CI SRC","38 to 48","1 unit","BOX","PR",null,79.116666666666674,26108.500000000004]
[null,6543014,null,"BACOU ENVIO (S3 CI SRC)\nBlack Derby-style shoe with smooth full grain leather upper, fully lined in leather, 200 Joule non-metallic toe cap, non-metallic puncture resistant midsole, non-magnetic","EN ISO 20345: 2011 S3 CI SRC","38 to 48","1 unit","BOX","PR",null,69.544621212121214,22949.725000000002]
[null,6543015,null,"BACOU ELANO (S3 CI SRC)\nBlack loafer with smooth full grain leather upper, fully lined in leather, 200 Joule non-metallic toe cap, non-metallic puncture resistant midsole, non-magnetic","EN ISO 20345: 2011 S3 CI SRC","38 to 48","1 unit","BOX","PR",null,66.813030303030288,22048.299999999996]
[null,6543016,null,"BACOU ELEGIO (S3 CI SRC)\nBlack Oxford shoe with smooth full grain leather upper, fully lined in leather, 200 Joule non-metallic toe cap, non-metallic puncture resistant midsole, non-magnetic\n","EN ISO 20345: 2011 S3 CI SRC","38 to 48","1 unit","BOX","PR",null,68.748863636363623,22687.124999999996]
[null,"Safety Footwear |  BACOU ORIGINAL",null,null,null,null,"",null,null,null,0,0]
[null,6246101,null,"BACOU CALEO (S3 HI CI SRC)\nWater-resistant, oiled full grain leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",50.836666666666666,16776.099999999999]
[null,6246102,null,"BACOU CERATA (S3 HI CI SRC)\nWater-resistant, oiled full grain leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",53.667727272727276,17710.350000000002]
[null,6246103,null,"BACOU SMILO (S3 HI CI SRC)\nWater-resistant full grain leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",49.413484848484842,16306.449999999997]
[null,6246104,null,"BACOU SINRA (S3 HI CI SRC)\nWater-resistant full grain leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",52.62712121212121,17366.95]
[null,6246105,null,"BACOU PLATEO (S3 HI CI SRC)\nWater-resistant leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",44.233409090909092,14597.025]
[null,6246106,null,"BACOU PLOMITA (S3 HI CI SRC)\nWater-resistant leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",47.064469696969695,15531.275]
[null,6246107,null,"BACOU ACANTO (S1P HI CI SRC)\nPerforated suede leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS1P HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",43.950303030303026,14503.599999999999]
[null,6246108,null,"BACOU ACANTI (S1 HI CI SRC)\nPerforated suede leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer","EN ISO\n20345: 2011\nS1 HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",41.402348484848481,13662.775]
[null,6246109,null,"BACOU SILUO (S1P HI CI SRC)\nSuede leather upper with ventilated mesh, PU2D outsole injected, 200J Spacium™  toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS1P HI CI SRC","39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",45.082727272727269,14877.3]
[null,6246110,null,"BACOU SOLANA (S1P HI CI SRC)\nSuede leather upper with ventilated mesh, PU2D outsole injected, 200J Spacium™   toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS1P HI CI SRC","39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",47.814318181818187,15778.725000000002]
[null,6246111,null,"BACOU SOLANUM (S1P SRC)\nBreathable microfibre upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS1P SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",46.11568181818182,15218.175000000001]
[null,6246112,null,"BACOU HEPTO (S3 HI CI SRC)\nWater-resistant full grain leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",47.63068181818182,15718.125]
[null,6246113,null,"BACOU HALTICA (S3 HI CI SRC)\nWater-resistant full grain leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 HI CI SRC","39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",50.270454545454541,16589.25]
[null,6246120,null,"BACOU TYLEX (S3 SRC)\nOiled full grain leather upper, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",64.226818181818174,21194.85]
[null,6246121,null,"BACOU SILVEX (S3 CI SRC)\nOiled full grain leather upper, Warm fleece lining, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nS3 CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",67.340984848484851,22222.525000000001]
[null,"BACOU ORIGINAL ESD",null,null,null,null,""]
[null,6246133,null,"BACOU ELEC ESD (S3 HI CI SRC)\nWater-resistant, full grain leather upper, ESD certified, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nESD S3 HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",55.075606060606063,18174.95]
[null,6246134,null,"BACOU PLUG ESD (S1P SRC)\nBreathable microfibre upper, ESD certified, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nESD S1P SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",50.836666666666666,16776.099999999999]
[null,6246135,null,"BACOU MICREL ESD (S3 HI CI SRC)\nWater-resistant, full grain leather upper, ESD certified, PU2D outsole injected, 200J Spacium™ toe cap in injected polymer, Stainless steel anti-puncture midsole","EN ISO\n20345: 2011\nESD S3 HI CI SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",58.289242424242424,19235.45]
[null,"Safety Footwear |  BACOU ORIGINAL FREE",null,null,null,null,""]
[null,"BACOU ORIGINAL FREE",null,null,null,null,""]
[null,6246155,null,"NEW BACOU TRACK AMG (S3 CI SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, black oiled water resistant full grain leather upper with POROMAX® lining, watertight leather bellows, padded collar and tongue, removable antistatic, antibacterial insole, non-magnetic","EN ISO\n20345: 2011\nS3 CI SRC\n","38 to 47","1 unit","BOX","PR",null,61.120303030303027,20169.7]
[null,6246156,null,"NEW BACOU MARSH AMG (S3 CI SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, black water resistant full grain leather upper with POROMAX® lining, padded collar and tongue, removable antistatic, antibacterial insole, non-magnetic","EN ISO\n20345: 2011\nS3 CI SRC","38 to 47","1 unit","BOX","PR",null,56.269242424242428,18568.850000000002]
[null,6246157,null,"Best seller! NEW BACOU PEAK AMG (S3 CI SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, smooth oiled leather upper, oil and water repellent with textile Cordura® inserts and POROMAX® lining, padded ankle collar and tongue, watertight bellows, reinforcement at the front and back, removable antistatic, antibacterial insole, non-magnetic","EN ISO\n20345: 2011\nS3 CI SRC","35 to 49","1 unit","BOX","PR",null,61.120303030303027,20169.7]
[null,6246158,null,"Best seller! NEW BACOU CREEK AMG (S3 CI SRC) 200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, smooth oiled leather upper, oil and water repellent with textile Cordura® inserts and POROMAX® lining, padded ankle collar and tongue, watertight bellows, reinforcement at the front and back, removable antistatic, antibacterial insole, non-magnetic","EN ISO\n20345: 2011\nS3 CI SRC","35 to 49","1 unit","BOX","PR",null,58.182121212121217,19200.100000000002]
[null,6246159,null,"NEW BACOU SUMMIT AMG (S1P SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, perforated grey suede leather shoe with black textile panels, removable antistatic, antibacterial insole, non-magnetic","EN ISO\n20345: 2011\nS1P SRC","35 to 49","1 unit","BOX","PR",null,53.124469696969697,17531.075000000001]
[null,6246160,null,"NEW BACOU CROSS AMG (S1P SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole, perforated grey suede leather ankle boot with black textile panels, removable antistatic, antibacterial insole, non-magnetic","EN ISO\n20345: 2011\nS1P SRC","35 to 49","1 unit","BOX","PR",null,58.319848484848485,19245.55]
[null,"Safety Footwear |  BACOU ORGINAL SPECIFICS CONSTRUCTION",null,null,null,null,""]
[null,6246150,null,"BACOU PRO BTP (S3 CI SRC)\n200 Joule non-metallic toe cap, stainless steel midsole with added anti-puncture for optimal protection against the puncture risks specific to\nconstruction, dual density PU sole, water resistant oiled full grain leather upper, Poromax® 3D lining, removable antistatic, antibacterial insole","EN ISO\n20345: 2011\nS3 CI SRC","38 to 49","1 unit","BOX","PR",null,71.908939393939391,23729.95]
[null,6246153,null,"BACOU HISTRIO BTP (S3 SRC)\n200 Joule non-metallic toe cap, stainless steel midsole with added anti-puncture for optimal protection against the puncture risks specific to\nconstruction, dual density PU sole, breathable microfibre ankle  work boot, removable antistatic, antibacterial insole","EN ISO\n20345: 2011\nS3 SRC","38 to 49","1 unit","BOX","PR",null,54.455833333333338,17970.425000000003]
[null,6246154,null,"BACOU HULSO BTP (S3 SRC)\n200 Joule non-metallic toe cap, stainless steel midsole with added anti-puncture for optimal protection against the puncture risks specific to\nconstruction, dual density PU sole, breathable microfibre high leg ankle work boot, removable antistatic, antibacterial insole","EN ISO\n20345: 2011\nS3 SRC","35 to 49","1 unit","BOX","PR",null,81.19022727272727,26792.774999999998]
[null,"BACOU ORIGINAL SPECIFICS"]
[null,6246125,null,"BACOU VENATO (S3 WR SRC)\n200 Joule non-metallic toe cap, stainless steel anti-puncture midsole, dual density PU sole, water resistant oiled full grain leather upper with black textile panels, lined with Sympatex® waterproof breathable membrane, removable antistatic, antibacterial insole","EN ISO\n20345: 2011\nS3 WR SRC","39 to 47","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",115.38484848484849,38077]
[null,"Safety Footwear |   BACOU OUTDOOR"]
[null,6245564,null,"BACOU BALLAST (S3 HRO CI HI SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole with TPU inserts adapted for irregular surfaces, reflective textile panels, Coolmax® lining and Coolmax® removable insole with antibacterial carbon treatment","EN ISO\n20345: 2011\nS3 HRO CI HI SRC","35 to 49","1 unit","BOX","PR",null,91.336136363636371,30140.925000000003]
[null,6246217,null,"BACOU BALLAST ICE (S3 HRO CI HI SRC)\n200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, dual density PU sole with TPU inserts adapted for irregular surfaces, reflective textile panels, Coolmax® lining and Coolmax® removable insole with antibacterial carbon treatment","EN ISO\n20345: 2011\nS3 HRO CI HI SRC","37 to 48","1 unit","BOX","PR",null,118.43780303030302,39084.474999999999]
[null,"Safety Footwear |  BAC'RUN PU.N",null,null,null,null,""]
[null,6245858,null,"BACOU EXONO (S3 HRO SRC)\nChemical resistant boot with 200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, PU/NITRILE outsole with high slip resistance and heat resistance to 300C, microfibre water resistant upper, Nomex® flame resistant stitching, fully lined in highly absorbent POROMAX® fabric, ergonomic padded collar, removable antistatic, antibacterial insole, non-magnetic, resistant to contact with corrosive fluids and acids in low concentration","EN ISO 20345: 2011 S3 HRO SRC","38 to 48","1 unit","BOX","PR",null,75.612272727272725,24952.05]
[null,6245868,null,"BACOU ARGONO (S3 HRO SRC)\nWelders boot wth 200 Joule non-metallic toe cap, lightweight, flexible non-metallic midsole, PU/NITRILE outsole with high slip resistance and heat resistance to 300C, full grain water resistant  leather upper, Nomex® flame resistant stitching, fully lined in highly absorbent POROMAX® fabric, ergonomic padded collar, full grain leather spark-proof flap with quick release fastening system, removable antistatic, antibacterial insole, non-magnetic","EN ISO 20345: 2011 S3 HRO SRC","38 to 48","1 unit","BOX","PR",null,81.496287878787882,26893.775000000001]
[null,6245867,null,"BACOU FREEROAD HRO HI3 SRC. Full grain leather.Padded ankle collar. 3D Poromax ® lining .Hydrophobic laces. No lateral sew. SPACIUM 200J non metallic toecap: ultra light (50% lighter than steel),  amagnétic and unalterable. (1100 N) FLEXIUM ™ non-metallic antipuncture midsole: light and flexible, amagnétic and unalterable, protects to whole surface of the foot. Thermal insulation complexe for HI3 performances:Isolates untill 250°C","EN ISO 20345 : 2011","38 to 48","1 unit","BOX","PR",null,107.64151515151515,35521.699999999997]
[null,6245877,null,"BACOU PROTECTOR (S3 M HRO SRC)\nMETA-TEC flexible 100 Joule metatarsal protection (M), 200 Joule non-metallic toe cap, steel puncture resistant midsole, PU/NITRILE outsole with high slip resistance and heat resistance to 300C, full grain pigmented leather upper, laces beneath the flexible metatarsal protection with a quick release buckle, removable antistatic and anti-bacterial insole","EN ISO 20345: 2011 S3 M HRO SRC","38 to 48","1 unit","BOX","PR",null,91.297878787878787,30128.3]
[null,"Safety Footwear |  BACOU NIT'LITE® ",null,null,null,null,""]
[null,6213303,null,"BACOU SUPER BOOT BK (S1P HRO SRC)\n200 Joule steel toe cap, steel puncture resistant midsole, Nitrile outsole with expanded cell structure is lightweight, flexibile and resistant to extremes of temperature (-30C to 300C), pigmented black leather upper and padded ankle collar\n","EN ISO 20345: 2011 S1P HRO SRC","38 to 47","1 unit","BOX","PR",null,29.856212121212121,9852.5499999999993]
[null,6213403,null,"BACOU HORALO (S1P HRO SRC)\nFoundry / welder's boot with 200 Joule steel toe cap, stainless steel puncture resistant midsole, Nitrile outsole with expanded cell structure is lightweight, flexibile and resistant to extremes of temperature (-30C to 300C), pigmented black leather upper with spark guard and padded ankle collar","EN ISO 20345: 2011 S1P HRO SRC","38 to 47","1 unit","BOX","PR",null,39.214015151515149,12940.624999999998]
[null,6213503,null,"BACOU NTL MAXI BOOT (S3 HRO SRC)\n200 Joule steel toe cap, steel puncture resistant midsole, Nitrile outsole with expanded cell structure is lightweight, flexibile and resistant to extremes of temperature (-30C to 300C), pigmented water resistant leather upper and padded leather ankle protection","EN ISO 20345: 2011 S3 HRO SRC","38 to 47","1 unit","BOX","PR",null,41.241666666666667,13609.75]
[null,6213703,null,"BACOU TRAINING LUX (S3 HRO SRC)\n200 Joule steel toe cap, steel puncture resistant midsole, Nitrile outsole with expanded cell structure is lightweight, flexibile and resistant to extremes of temperature (-30C to 300C), pigmented water resistant black full grain leather upper ","EN ISO 20345: 2011 S3 HRO SRC","38 to 47","1 unit","BOX","PR",null,37.484772727272727,12369.975]
[null,6213953,null,"BACOU RIGGER (S3 HRO SRC)\n200 Joule steel toe cap, steel puncture resistant midsole, Nitrile outsole with expanded cell structure is lightweight, flexibile and resistant to extremes of temperature (-30C to 300C), water resistant tan full grain leather upper with heat/fire resistant stitching, pull on lugs","EN ISO 20345: 2011 S3 HRO SRC","38 to 47","1 unit","BOX","PR",null,77.150227272727278,25459.575000000001]
[null,"Safety Footwear | ATHLETIC"]
[null,6243829,null,"BACOU PODIUM (S3 CI SRC)\n200J non-metallic toe cap, non-metallic puncture resistant midsole, water-resistant nubuck leather upper, Poromax 3D lining, breathable, absorbent, fast drying, removable Coolmax insole, injected PU/TPU dual density outsole, non-magnetic, 100% metal free ","EN ISO 20345: 2011 S3 CI SRC","37 to 47 ","1 unit","BOX","PR",null,70.608181818181805,23300.699999999997]
[null,6243850,null,"BACOU ASCENDER (S3 CI SRC)\n200J non-metallic toe cap, non-metallic puncture resistant midsole, water-resistant leather and textile upper, Poromax 3D lining, breathable, absorbent, fast drying, removable Coolmax insole, injected PU/TPU dual density outsole, non-magnetic, 100% metal free ","EN ISO 20345: 2011 S3 CI SRC","37 to 47 ","1 unit","BOX","PR",null,59.459924242424236,19621.774999999998]
[null,6243851,null,"BACOU ASCENDER MID (S3 CI SRC)\n200J non-metallic toe cap, non-metallic puncture resistant midsole, water-resistant leather and textile upper, Poromax 3D lining, breathable, absorbent, fast drying, removable Coolmax insole, injected PU/TPU dual density outsole, non-magnetic, 100% metal free ","EN ISO 20345: 2011 S3 CI SRC","37 to 47 ","1 unit","BOX","PR",null,64.785378787878784,21379.174999999999]
[null,6243853,null," BACOU BOOSTER BLACK (S1P CI SRC) 200J non-metallic toe cap, non-metallic puncture resistant midsole, suede leather and mesh upper, moisture management lining, removable Coolmax insole, injected PU/TPU dual density outsole, non-magnetic, 100% metal free ","EN ISO 20345: 2011 S1P CI SRC","37 to 47 ","1 unit","BOX","PR",null,52.321060606060605,17265.95]
[null,6243854,null,"BACOU FRESCO (S1P CI SRC)\n200J non-metallic toe cap, non-metallic puncture resistant midsole, suede leather and mesh upper, Poromax 3D lining, breathable, absorbent, fast drying, removable Coolmax insole, injected PU/TPU dual density outsole, non-magnetic, 100% metal free ","EN ISO 20345: 2011 S1P CI SRC","37 to 47 ","1 unit","BOX","PR",null,54.210984848484841,17889.624999999996]
[null,6243855,null,"BACOU FRESCO MID (S1P CI SRC)\n200J non-metallic toe cap, non-metallic puncture resistant midsole, suede leather and mesh upper, Poromax 3D lining, breathable, absorbent, fast drying, removable Coolmax insole, injected PU/TPU dual density outsole, non-magnetic, 100% metal free ","EN ISO 20345: 2011 S1P CI SRC","37 to 47 ","1 unit","BOX","PR",null,57.409318181818179,18945.075000000001]
[null,"ATHLETIC ESD"]
[null,6243857,null,"BACOU ASCENDER ESD (S3 CI SRC)\n200J non-metallic toe cap, non-metallic puncture resistant midsole, water-resistant leather and textile upper, Poromax 3D lining, breathable, absorbent, fast drying, specific ESD insole, injected PU/TPU dual density outsole, non-magnetic, 100% metal free ","EN ISO 20345: 2011 S3 CI SRC\nEN61340-4-3:2001 Class 3","37 to 47 ","1 unit","BOX","PR",null,65.122045454545457,21490.275000000001]
[null,"STITCHED Originals"]
[null,6530316,null,"NEW BACOU ANNAPURNA (S3 SRC)\n200 Joule non-metallic toe cap, stainless steel puncture resistant midsole, PU outsole with welted stitched construction, natural tanned full grain leather upper, waterproof 6 hours, no lateral stitching, lined with suede leather, padded ankle collar and padded bellowed tongue, removable antistatic and anti-bacterial insole","EN ISO 20345: 2011 S3 SRC","39 to 47","1 unit","BOX","PR",null,112.72212121212119,37198.299999999996]
[null,6530331,null,"NEW BACOU NEBRASKA (S3 SRC)\n200 Joule non-metallic toe cap, stainless steel puncture resistant midsole, PU outsole with welted stitched construction, full grain oiled nubuck leather upper, oil and water resistant, lined with suede leather, padded ankle collar and padded bellowed tongue, removable antistatic and anti-bacterial insole","EN ISO 20345: 2011 S3 SRC","39 to 47","1 unit","BOX","PR",null,96.990606060606055,32006.899999999998]
[null,6539060,null,"NEW BACOU MONTANA (S3 HRO CI SRC)\n200J non-metallic toe cap, non-metallic puncture resistant midsole, Nitrile outsole with welted stitched construction,  water-resistant oiled leather upper with warm fleece lining and side pull-on tabs, antistatic and anti-bacterial insole","EN ISO 20345: 2011 S3 HRO CI SRC","37 to 48","1 unit","BOX","PR",null,118.64439393939394,39152.65]
[null,"Safety Footwear |  WHITE  FOR MEN",null,null,null,null,""]
[null,6233216,null,"BACOU MONT BLANC (S2 SRC) \nWhite moccasin style slip-on shoe with epoxy treated 200J steel toe cap, anti-bacterial treated leather upper, limited stitching, double-density PU sole","EN ISO 20345: 2011 S2 SRC","35 to 47","1 unit","BOX","PR",null,39.956212121212118,13185.55]
[null,6233215,null,"BACOU MONT BLANC (S3 SRC) \nWhite moccasin style slip-on shoe with epoxy treated 200J steel toe cap, stainless steel puncture resistant midsole, anti-bacterial treated leather upper, limited stitching, double-density PU sole","EN ISO 20345: 2011 S3 SRC","35 to 47","1 unit","BOX","PR",null,43.667196969696967,14410.174999999999]
[null,6240748,null,"BACOU SUPER MONT BLANC (S2 SRC)\nWhite moccasin style ankle boot with epoxy treated 200J steel toe cap, anti-bacterial treated leather upper, padded collar, limited stitching, double-density PU sole","EN ISO 20345: 2011 S2 SRC","35 to 47","1 unit","BOX","PR",null,44.019166666666663,14526.324999999999]
[null,6246127,null,"BACOU PROCLEAN S2 SRC High slip resistance and durability for intensive usage. White mocrofibre upper for easy cleaning.(Chemical, Food Services, Medical, Pharmaceutical, Automotive..).All models Bacou Pro'Clean comply with the EN ISO 20345:2011 standard. ","EN ISO 20345:2011 S2 SRC","39 to 49","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",40.805530303030295,13465.824999999997]
[null,6246130,null,"BACOU PROCLEAN BLACK S2 SRC. Breathable water resistant microfibre upper. PU2D outsole injected. SRC certified. 200J Spacium toe cap in injected polymer. Complies with EN ISO 20345:2011 Standard. High slip resistance and durability for intensive usage. No stiching on a forefoot to minimize source of contamination. ",null,"39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",58.472878787878791,19296.050000000003]
[null,6246129,null,"BACOU SUPER PRO CLEAN (S2 SRC)\nWhite ankle boot with 200J non-metallic toe cap, breathable water resistant microfibre upper, limited stitching, double-density PU sole, metal free, non-magnetic","EN ISO 20345: 2011 S2 SRC","39 to 48","1 unit","BOX","PR","NOTICE !\nCurrently available new sizes !",46.88848484848485,15473.2]
[null,"Safety Footwear |  COCOON WOMAN RANGE",null,null,null,null,""]
[null,"A comfortable, light and exclusive range of safety footwear dedicated to woman."]
[null,6551608,null,"SWEET S1P HI CI SRC. Ventilated mesh and microfiber, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.Smartium toe cap in injected polymer. Non metallic, 50% lighter than style with a thin design",null,"35 to 42","1 unit","BOX","PR",null,60.890757575757569,20093.949999999997]
[null,6551607,null,"SPICE S1P HI CI SRC.Ventilated mesh and full grain leather, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole. 100% metal free model.  Non metallic antipuncture midsole protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.",null,"35 to 42","1 unit","BOX","PR",null,61.594696969696969,20326.25]
[null,6551611,null,"SPICE ESD S1P HI CI SRC.Ventilated mesh and full grain leather, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole. 100% metal free model.  Non metallic antipuncture midsole protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.",null,"35 to 42","1 unit","BOX","PR",null,68.634090909090915,22649.250000000004]
[null,6551604,null,"GLEE S3 HI CI SRC. Microfibre and water repellant textile, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole.",null,"35 to 42","1 unit","BOX","PR",null,63.278030303030299,20881.75]
[null,6551602,null,"COSY GREY S3 HI CI SRC. Microfiber upper, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.Smartium toe cap in injected polymer. Non metallic, 50% lighter than style with a thin design",null,"35 to 42","1 unit","BOX","PR",null,63.278030303030299,20881.75]
[null,6551601,null,"COSY BLACK S3 HI CI SRC Full grain leather upper, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.",null,"35 to 42","1 unit","BOX","PR",null,66.728863636363627,22020.524999999998]
[null,6551609,null,"COSY BLACK ESD S3 HI CI SRC Full grain leather upper, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole. Non metallic antipuncture midsole. protects 100% of the foot surface, provides flexibility and complies with EN ISO 20345:2011.",null,"35 to 42","1 unit","BOX","PR",null,69.368636363636355,22891.649999999998]
[null,6551603,null,"COSY MID S3 HI CI SRC. Full grain leather upper, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole",null,"35 to 42","1 unit","BOX","PR",null,73.913636363636357,24391.499999999996]
[null,6551610,null,"COSY MID ESD S3 HI CI SRC. Full grain leather upper, Poromax Lining, padded ankle collar. 100% metal free. PU/Rubber outsole",null,"35 to 42","1 unit","BOX","PR",null,84.472727272727269,27876]
[null,"TEMPTATION CITY",null,null,null,null,""]
[null,6551125,null,"BACOU SUCCESS (S2 SRC)\nBlack tennis style shoe with full grain leather upper, leather lining, black mono-density PU sole with fine design for improved grip ","EN ISO 20345: 2011 S2 SRC","35 to 42","1 unit","BOX","PR",null,66.376893939393938,21904.375]
[null,6551126,null,"BACOU SUCCESS (S3 SRC)\nAs above with composite midsole ","EN ISO 20345: 2011 S3 SRC","35 to 42","1 unit","BOX","PR",null,66.376893939393938,21904.375]
[null,6551131,null,"BACOU TOP (S3 SRC)\nAs above with composite midsole ","EN ISO 20345: 2011 S3 SRC","35 to 42","1 unit","BOX","PR",null,70.654090909090911,23315.850000000002]
[null,6551135,null,"BACOU IMAGE (S2 SRC)\nBlack slip-on shoe with buckle, full grain leather upper, leather lining, black mono-density PU sole with fine design for improved grip ","EN ISO 20345: 2011 S2 SRC","35 to 42","1 unit","BOX","PR",null,72.689393939393938,23987.5]
[null,6551140,null,"BACOU EASY (S2 SRC)\nNavy blue loafer style slip-on shoe, full grain leather upper and leather lining, black monodensity PU sole with fine design for improved grip ","EN ISO 20345: 2011 S2 SRC","35 to 42","1 unit","BOX","PR",null,63.170909090909085,20846.399999999998]
[null,6551505,null,"BACOU BLUE LABO (SB EA SRC)\nNavy blue sling back shoe with top-grain leather upper, perforated for breathability and white leather lining, monodensity PU sole built up at the heel to 40mm","EN ISO\n20345\nSB EA SRC","35 to 42","1 unit","BOX","PR",null,47.768409090909088,15763.574999999999]
[null,6551155,null,"BACOU FINE (S1 SRC)\nBlack suede leather upper with full grain leather lining and leather insole, very comfortable anatomic design, anti-slip monodensity PU outsole\n","EN ISO 20345: 2011 S1 SRC","35 to 42","1 unit","BOX","PR",null,74.938939393939393,24729.85]
[null,6551525,null,"BACOU OFFICE (P1 SRA)\nBlack Court shoe with full grain leather upper and lining, Nitrile sole built up at the heel to 40mm, 100J steel toe cap","EN ISO\n20346\nP1 SRA","35 to 42","1 unit","BOX","PR",null,72.689393939393938,23987.5]
[]
[null,"Safety Footwear |  WHITE RANGE - LADIES"]
[null,"WHITE RANGE - LADIES",null,null,null,null,""]
[null,6551150,null,"BACOU LITE (S1 SRC)\nWhite perforated grain leather upper for breathability, leather lining and insole, strap and buckle fastening, very comfortable anatomic design, anti-slip monodensity PU outsole\n","EN ISO 20345: 2011 S1 SRC","35 to 42","1 unit","BOX","PR",null,68.519318181818178,22611.375]
[null,"ACCESSORIES",null,null,null,null,""]
[null,6000301,null,"Triple action \"Image\" insole; anti-fungal, anti-bacterial and anti-odour, honeycomb structure",null,"35 to 47","5 units","BAG","PR",null,6.9781818181818176,2302.7999999999997]
[null,6000310,null,"Double action perforated blue insole, anti-bacterial and anti-odour",null,"38 to 47","1 unit","BAG","PR",null,4.3690151515151516,1441.7750000000001]
[null,6000320,null,"BACOU Bac'Run Insole",null,"38 to 47","1 unit","BAG","PR",null,8.730378787878788,2881.0250000000001]
[null,6000321,null,"BAC'RUN insole",null,"35 to 47","1 unit","BAG","PR",null,5.8381060606060604,1926.575]
[null,6000604,null,"Black Leather Laces 115cm",null,null,"10 units","BAG","PR",null,3.0835606060606064,1017.5750000000002]
[null,6000601,null,"Black Laces 75cm ",null,null,"25 units","BAG","PR",null,1.4996969696969698,494.90000000000003]
[null,6000607,null,"Black Laces  90cm ",null,null,"25 units","BAG","PR",null,1.5379545454545454,507.52499999999998]
[null,6000608,null,"Black Laces 120cm ",null,null,"25 units","BAG","EA",null,1.6297727272727272,537.82499999999993]
[null,6000609,null,"Black Laces 150cm ",null,null,"25 units","BAG","PR",null,2.1194696969696967,699.42499999999995]
[null,6000602,null,"Grey Laces  90cm ",null,null,"25 units","BAG","PR",null,1.5379545454545454,507.52499999999998]
[null,6000350,null,"BACOU X'MAX BLACK Insole. Dual denisty PU foam for intensive use . Antistatic in the body: maximum efficiency. Prevents injury and muscule fatigue thanks to cushion. Evacuation channels: ensures that circulation of air under the foot when walking. ",null,"35 to 49","1 unit","BAG","PR",null,8.5166666666666675,2810.5000000000005]
[]
[null,"Safety Footwear |  GLOBAL RANGE "]
[null,6200611,null,"GLOBAL CONFORT 2 S1P SRA -   ",null," 35 to 48","1 unit ","BOX","PR",null,26.405378787878785,8713.7749999999996]
[null,6200615,null,"GLOBAL CONFORT 2 S3 SRA ",null," 38 to 48","1 unit ","BOX","PR",null,26.405378787878785,8713.7749999999996]
[null,6200601,null,"GLOBAL TURBO 2 S1P SRA  ",null," 35 to 48","1 unit ","BOX","PR",null,26.405378787878785,8713.7749999999996]
[null,6200605,null,"GLOBAL TURBO 2 S3 SRA ",null," 38 to 48","1 unit ","BOX","PR",null,26.405378787878785,8713.7749999999996]
[null,6200621,null,"GLOBAL SPORT 2 S1P SRA ",null," 35 to 48","1 unit ","BOX","PR",null,26.405378787878785,8713.7749999999996]

{"sheet":"SU Clothing","index":7,"n_rows":81,"n_cols":11,"rows_kept":81,"cut":false,"hidden":false,"merged":[[69,1,69,3]]}
[null,"PPE Clothing |  SINGLE USE CLOTHING",null,null,null,null,""]
[null,null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per","NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,"PPE Clothing |  SINGLE USE CLOTHING",null,null,null,null,""]
[null,"CAT III. Type 5&6"]
[null,4509805,null,"NEW Ne-Hon™ 5+  High Visibility Single Use Coverall dedicated to the protection of workers facing serious to fatal hazards. Conform to EN 20471 class 3 and cabin test Type 5 & 6. Model with reinforced knees, without hood.\n",null,"S-XXXL","20 units","CAS","EA",21.060606060606059,6949.9999999999991]
[null,4509807,null,"NEW Ne-Hon™ 5+  High Visibility Single Use Coverall dedicated to the protection of workers facing serious to fatal hazards. Conform to EN 20471 class 3 and cabin test Type 5 & 6. Model with reinforced knees, with hood.\n",null,"S-XXXL","20 units","CAS","EA",21.893939393939391,7224.9999999999991]
[null,4509446,null," Ne-Hon 6 . High Visibility Single Use Coverall (class 3) dedicated to the protection of workers facing serious to fatal hazards. The 1st certified High Visibility single use coverall on the market. EN20471, Class 3, Type 6",null,"S-XXXL","20 units","CAS","EA",22.327121212121209,7367.9499999999989]
[null,4500101,null," Mutex E LIGHT type 5 and 6, antistatic and radioactive particles certified coverall with elasticated hood, waist, wrists and ankles, made of white breathable polypropylene, 3-layer, 56g/m², silicone and latex-free\n● PPE Category 3 - types 5 and 6\n● EN ISO 13982-1:2004 - Type 5\n● EN 13034:2005 - Type 6\n● EN 1149-5:2008 - Antistatic\n● EN 1073-2:2002 - Protection against radioactive particles",null,"S, M, L. XL, XXL, XXXL","50 units","CAS","EA",3.7875000000000001,1249.875]
[null,4500200,null,"Essian 2. Coverall designed to protect workers from chemicals under the form of splashes or particles. Its ergonomics offer a good fitting and protection. Model with elasticated wrists and ankles. 4-layer polypropylene 55g/m² - SMMS Special design at the crotch to prevent from cracking Bounded seams to increase seams resistance Adhesive flap to get a better protection at zipper level, Type 5&6, EN1073-2, EN1149",null," S to XXXL","25 units  individually packed","CAS","EA",4.9887878787878783,1646.3]
[null,4500210,null,"Essian 2 Blue. Coverall designed to protect workers from chemicals under the form of splashes or particles. Its ergonomics offer a good fitting and protection. Model with elasticated wrists and ankles. 4-layer polypropylene 55g/m² - SMMS Special design at the crotch to prevent from cracking Bounded seams to increase seams resistance Adhesive flap to get a better protection at zipper level, Type 5&6, EN1073-2, EN1149",null,"L","25 units  individually packed","CAS","EA",5.1724242424242428,1706.9]
[null,4500501,null,"MUTEX LlGHT+, type 5 and 6, antistatic, radioactive particles and biological agents certified coverall with elasticated hood, waist, wrists and ankles, made of white non-woven polypropylene laminated with a microporous film, 65g/m², silicone and latex-free\n● PPE Category 3 - types 5 and 6\n● EN ISO 13982-1:2004 - Type 5\n● EN 13034:2005 / A1:2009 - Type 6\n● EN 1149-5:2008 - Antistatic\n● EN 14126:2003 - Protection against biological agents\n● EN 1073-2:2002 - Protection against radioactive particles",null,"S, M, L. XL, XXL, XXXL","25 units","CAS","EA",5.8304545454545451,1924.05]
[null,4500505,null,"NEW!!! Mutex Light BS.  Single use protective coverall specific for the use of fall protection devices. Ideal use over a harness - back sleeve designed to pass lanyard.Protects the harness during from chemicals / dirt / paiting etc. Protects the evironment from the harness in the food industry for example",null,"S-XXXL","25 units","CAS","EA",6.9552272727272735,2295.2250000000004]
[null,4180002,null," MUTEX 2. Single use coverall type 5 & 6 which protects against biological agents. Silicone & latex free.Breathable .Antistatic Honeywell exclusive material. Excellent liquid tightness.No seams on arms and shoulders. Double Outer & inner flap Excellent resistance: Maxi-wide seams .Special design at crotch prevents from tearing.  has hood, ankles, wrists & back elasticated. Material: 69g/m².",null,"S-XXXL","25 units","CAS","EA",6.7333333333333325,2221.9999999999995]
[null,4571450,null," Deltasafe. Type 5 & 6, antistatic, fire-retardant certified coverall. Breathable & flame-retardant single use non ventilated protective suit designed to protect against particles contamination and chemical splashes. FIRE-RETARDANT & M1 CERTIFIED DELTASAFE has been developped especially to avoid any risk when manipulating flammable substances. BREATHABILITY DELTASAFE offers a breathability equal to a T-shirt. ANTISTATIC DELTASAFE is antistatic certified to avoid accumulation of electrostatic charges on the garnement that may cause a risk of explosion or fire.",null,"S to XXXL",null,null,"EA",9.9546212121212125,3285.0250000000001]
[null,4500300,null,"ESSIAN FR type 5 and 6, Flame-Retardant, antistatic and radioactive particles certified coverall with elasticated hood, waist, wrists and ankles, made of blue breathable viscose, 90 g/m², silicone and latex-free\n● PPE Category 3 - types 5 and 6\n● EN 13982-1:2004 - Type 5\n● EN 13034:2005 - Type 6\n● EN 1149-1:1995 - Antistatic\n● EN 1073-2:2002 - Protection against radioactive particles\n● EN ISO 14116:2008 - Limited spread of flames",null,"S, M, L. XL, XXL, XXXL","25 units","CAS","EA",13.589090909090912,4484.4000000000005]
[null,"Overall in blue polyethylene. Thickness 50μ with full hood and zip fastening. PPE Category 1 offers protection against minor"]
[null,"risks in the work environment. Suitable for use in industrial cleaning and maintenance operations, pharmaceutical industry, "]
[null,"poor weather conditions, etc."]
[null,4180130,null,"SPACEL 2000 EBJ overall with elasticated wrists and ankles, PPE Category 1",null,"M, L, XL, XXL","50 units","BOX","EA",7.2689393939393945,2398.75]
[null,4180131,null,"Spacel 2000 AP EBJ. type 5 & 6, single use. Product use: Pharmaceutical industry, industrial cleaning, industrial maintenance, sanitation, bad weather conditions working.Excellent liquid tightness: Seamless; Smooth surface for an excellent evacuation of liquids; Special designed hood for a just right tightness around the mask. Security: 100% PE, 50µ, Excellent arm and leg resistance ensures safety when moving. Excellent fit and comfort: Ventilation valve for hot environment Back-elastic Elasticated ankles and wrists; Blue colour for a better visibility;",null,"M to XXXL",null,null,null,7.8274999999999997,2583.0749999999998]
[null,"SPACEL 3000"]
[null,"Overall in multilayered polyethylene. Thickness 100μ with full hood and zip fastening.  Yellow exterior and white interior. PPE"]
[null,"Category 2 for intermediate risks and Category 3 for serious or fatal risks. Suitable for use in pharmaceutical industry, "]
[null,"chemistry, laboratory work, etc."]
[null,4503002,null,"SPACEL 3000 EBJ overall with elasticated wrists and ankles, PPE Category 2 - type 6 (replaces 4180140)",null,"S, M, L, XL, XXL, XXXL","25 units","BOX","EA",9.7633333333333319,3221.8999999999996]
[null,"PPE Clothing |  SINGLE USE CLOTHING",null,null,null,null,""]
[null,"Cat III. Type 3,4,5,6",null,null,null,null,""]
[null,4503004,null,"SPACEL 3000 AP/EBJ overall with elasticated wrists and ankles, plus valve ventilation, PPE Category 2 - type 6 (replaces 4180133)",null,"S, M, L, XL, XXL, XXXL","25 units","BOX","EA",10.32189393939394,3406.2249999999999]
[null,4503000,null,"SPACEL 3000 RA/EBJ overall with elasticated wrists and ankles, plus adhesive flap over zip\nPPE Category 3 - types 3, 4, 5, 6 (replaces 4180149)",null,"S, M, L, XL, XXL, XXXL","25 units","BOX","EA",8.7074242424242421,2873.45]
[null,4503003,null,"SPACEL 3000 AP/RA/EBJ overall with elasticated wrists and ankles, adhesive flap over zip\nand valve ventilation, PPE Category 3 - types 3, 4, 5, 6",null,"S, M, L, XL, XXL, XXXL","25 units","BOX","EA",11.576742424242425,3820.3250000000003]
[null,4503001,null,"SPACEL 3000 RA GC PS incorporates glued gloves, welded feet and adhesive flap over zip \nPPE Category 3 - types 3, 4, 5, 6 (replaces 4573020)",null,"S, M, L, XL, XXL, XXXL","10 units","BOX","EA",21.087575757575756,6958.9]
[null,"NEW SPACEL 3000 APRON"]
[null,"Long sleeved apron in multilayered polyethylene, thickness 100μ, yellow exterior, PB[4] (partial Body)"]
[null,4503005,null,"SPACEL 3000 APRON\nLong sleeved apron with elasticated wrists, no seams, two adjustment straps ",null,"M, L, XL, XXL, XXXL","50 units","BOX","EA",6.0446969696969699,1994.75]
[null,null,null,null,null,null,""]
[null,"SPACEL 4000"]
[null,"Overall in multilayered polyethylene. Thickness 150μ with full hood and zip fastening. Green exterior and white interior."]
[null,"PPE Category 3 for exposure to high risk substances. Suitable for use in chemistry/petrochem industry, inshore/offshore"]
[null,"oil industry, transportation of hazardous materials, etc."]
[null,4504000,null,"SPACEL 4000 RA EBJ with elasticated wrists and ankles, plus adhesive flap over zip\nPPE Category 3 - types 3, 4, 5, 6 \n(replaces 4180161)",null,"S, M, L. XL, XXL, XXXL","25 units","BOX","EA",16.267121212121214,5368.1500000000005]
[null,4504001,null,"SPACEL 4000 RA GC EBJ incorporates glued gloves, welded feet and adhesive flap over zip\nPPE Category 3 - types 3, 4, 5, 6 \n(replaces 4574040)",null,"S, M, L. XL, XXL, XXXL","10 units","BOX","EA",25.647878787878788,8463.7999999999993]
[null,null,null,null,null,"Size","Height"]
[null,null,"Type 1    ●   Protection against gases",null,null,"S - 1","5'5\" - 5'7\""]
[null,null,"Type 2    ●   Limited protection against gases",null,null,"M - 2","5'7\" - 5'10\""]
[null,null,"Type 3    ●   Protection against chemical projections (jet)",null,null,"L - 3","5'10\" - 6'"]
[null,null,"Type 4    ●   Protection against chemical sprays (aerosol)",null,null,"XL - 4","6' - 6'2\""]
[null,null,"Type 5    ●   Protection against dust",null,null,"XXL - 5","6'2\" - 6'4\""]
[null,null,"Type 6    ●   Protection against chemical splash",null,null,"XXXL - 6","6'4\" - 6'7\""]
[null,null,null,null,null,null,""]
[null,"PPE Clothing |  SINGLE USE CLOTHING",null,null,null,null,""]
[null,"SPACEL COMFORT",null,null,null,null,""]
[null,4506001,null,"SPACEL COMFORT MEDIUM type 3, 4, 5 and 6, antistatic, radioactive particles and biological agents certified coverall with elasticated hood, waist, wrists and ankles, made of non-woven polypropylene laminated with polyethylene film, orange, 80 g/m², silicone and latex-free\n● PPE Category 3 - types 3, 4, 5, 6\n● EN 14605:2005 / A1:2009 - Type 3\n● EN 14605:2005 / A1:2009 - Type 4\n● EN ISO 13982-1:2004 - Type 5\n● EN 13034:2005 / A1:2009 - Type 6\n● EN 1149-5:2008 - Antistatic\n● EN 14126:2003 - Protection against biological agents\n● EN 1073-2:2002 - Protection against radioactive particles\n",null,"S, M, L. XL, XXL, XXXL","25 units","CAS","EA",16.695606060606064,5509.5500000000011]
[null,4507000,null,"SPACEL COMFORT HEAVY type 3, 4, 5 and 6, antistatic, radioactive particles and biological agents certified coverall with elasticated hood, waist, wrists and ankles, stitched and taped seams, double adhesive flap with double zipper and knee pads, made of non-woven polypropylene laminated with complex polyethylene-EVOH film, grey, 155 g/m², silicone and latex-free\n● PPE Category 3 - types 3, 4, 5, 6\n● EN 14605:2005 / A1:2009 - Type 3\n● EN 14605:2005 / A1:2009 - Type 4\n● EN ISO 13982-1:2004 - Type 5\n● EN 13034:2005 / A1:2009 - Type 6\n● EN 1149-5:2008 - Antistatic\n● EN 14126:2003 - Protection against biological agents\n● EN 1073-2:2002 - Protection against radioactive particles\n",null,"S, M, L. XL, XXL, XXXL","10 units","CAS","EA",40.813181818181818,13468.35]
[null,4508000,null,"SPACEL COMFORT FR is a type 3 and 4, Flame-Retardant and antistatic certified coverall with elasticated hood, waist, wrists and ankles, stitched and taped seams, double adhesive flap with double zipper, made of non-woven coated viscose, grey, 138g/m², silicone and latex-free\n● PPE Category 3 - types 3 and 4\n● EN 14605:2005 / A1:2009 - Type 3\n● EN 14605:2005 / A1:2009 - Type 4\n● EN 1149-5:2008 - Antistatic\n● EN ISO 14116:2008 - Limited spread of flames",null,"S, M, L. XL, XXL, XXXL","10 units","CAS","EA",33.391212121212128,11019.100000000002]
[null,"PPE Clothing |  SINGLE USE CLOTHING",null,null,null,null,"",null,null,0,0]
[null,null,null,"Spacel T4/ Spacel C4P polypropylene overall laminated with a microporous film, 65g/m2, antistatic with three-piece hood, elasticated wrists and ankles, double (inside and out) flap protecting the zip\n● PPE Category 3 - Types 4, 5 and 6\n● EN 14605 - Type 4\n● EN ISO 13982-1 - Type 5\n● EN 13034 - Type 6\n● EN 1149-5 - Antistatic\n● EN 1073-2 - Radioactive particles\n● EN 14126 - Protection against biological agents"]
[null,4500601,null,"● Spacel C4",null,"S-XXXL","25 units","CAS","EA",7.8198484848484853,2580.5500000000002]
[null,4500611,null,"● Spacel C4P",null,"S-XXXL","25 units","CAS","EA",8.1871212121212107,2701.7499999999995]
[null,"MS 3.5.6 OVERALL",null,null,null,null,""]
[null,"NEW RAINLIGHT",null,null,null,null,""]
[null,4575045,null,"RAINLIGHT set comprises tunic and trousers in 3-layer 100μ polyethylene film, PPE Category 1\n● Hooded tunic with elasticated wrists and 25cm zip at the collar assists putting on/removing\n● Trousers with elasticated waist and ankles\n",null,"M, L, XL, XXL","25 units","BOX","EA",9.7786363636363625,3226.95]
[null,"JUMPSUITS",null,null,null,null,""]
[null,4180143,null,"White polypropylene coverall, 40g/m², light, breathable and comfortable with elasticated hood, wrists and ankles",null,"L, XL, XXL","25 units","BOX","EA",2.4484848484848487,808.00000000000011]
[null,4571435,null,"Blue polypropylene coverall, 40g/m², light, breathable and comfortable with elasticated hood, wrists and ankles, 2 pockets",null,"L, XL, XXL","25 units","BOX","EA",2.6321212121212123,868.6]
[null,"KITS"]
[null,4598104,null,"Asbestos bag 80µ 40X60CM",null,null,null,null,null,1.0941666666666667,361.07500000000005]
[null,4598105,null,"Asbestos bag with ZIPPER 80µ 40X60CM",null,null,null,null,null,2.5403030303030301,838.3]
[null,4598106,null,"Asbestos bag- 90X100CM",null,null,null,null,null,2.8693181818181817,946.875]
[null,"PPE Clothing |  SINGLE USE CLOTHING",null,null,null,null,""]
[null,4552000,null,"NEW MUTEX LIGHT sleeves, white non-woven polypropylene laminated with a microporous polyethylene film, antistatic, 65g/m2, length 50cm, silicone and latex free",null,null,"100 units","BOX","PR",1.1859848484848485,391.375]
[null,4570001,null,"SPACEL sleeves, white polyethylene film, liquid tight, 130μ, length 45cm",null,null,"200 units","BOX","EA",0.47439393939393937,156.54999999999998]
[null,"OVERBOOTS",null,null,null,null,""]
[null,4550000,null,"MUTEX LIGHT overboots, non-woven polypropylene laminated with a microporous film, white, 65g/m2, antistatic, non-slip, elasticated calves, length 32cm, width 13cm, height 57cm",null,null,"100 units","CAS","PR",2.0506060606060603,676.69999999999993]
[null,4560001,null,"SPACEL COMFORT MEDIUM overboots, non-woven polypropylene laminated with polyethylene film, orange, 80g/m2, antistatic, liquid tight, non-slip, elasticated calves, length 32cm, width 13cm, height 57cm",null,null,"25 units","BOX","PR",4.644469696969697,1532.675]
[null,4570000,null,"SPACEL COMFORT HEAVY overboots, non-woven polypropylene laminated with a complex polyethylene-EVOH film, grey, 155g/m2, antistatic, liquid tight, non-slip, elasticated calves, length 32cm, width 13cm, height 57cm",null,null,"10 units","BOX","PR",10.084696969696969,3327.95]
[null,4579911,null,"PE 70μ textured overboots, transparent textured polyethylene film is liquid tight, non-slip, low particle release, elasticated calves, length 40cm, width 13cm, height 57cm",null,null,"250 units","CAS","PR",0.51265151515151508,169.17499999999998]
[null,"OVERSHOES",null,null,null,null,""]
[null,4551000,null,"MUTEX light overshoes, white non-woven polypropylene laminated with a polyethylene microporous film, antistatic, non-slip sole, elasticated ankles, length 32cm, width 13cm, height 15cm",null,null,"100 units","CAS","PR",1.1400757575757576,376.22500000000002]
[null,4559811,null,"PE 130μ textured overshoes, white textured polyethylene film is liquid tight and non-slip, elasticated ankles, length 32cm, width 13cm, height 19.5cm",null,null,"100 units","CAS","PR",0.82636363636363652,272.70000000000005]
[null,null,null,null,null,null,""]

{"sheet":"Chemical Coveralls","index":8,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[[4,3,4,8]]}
[null,"REUSABLE HEAVY CHEMICAL COVERALLS |  Chemical protection"]
[null,"A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per","NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,"NEW EASYCHEM - Protective suits made of polyamide coated with elastomer, 650g/m2, for use with SCBA - PPE Category 3"]
[null,null,null,"EASYCHEM 1A suit, EN943-1:2002 Type 1a gas tight suit with BA inside"]
[null,"CC8907072-M/42",null,"● Size M/42",null,null,"1 unit",null,"EA",2381.0750000000003,785754.75000000012]
[null,"CC8907072-M/44",null,"● Size M/44",null,null,"1 unit",null,"EA",2381.0750000000003,785754.75000000012]
[null,"CC8907073-L/42",null,"● Size L/42",null,null,"1 unit",null,"EA",2381.0750000000003,785754.75000000012]
[null,"CC8907073-L/44",null,"● Size L/44",null,null,"1 unit",null,"EA",2381.0750000000003,785754.75000000012]
[null,"CC8907073-L/46",null,"● Size L/46",null,null,"1 unit",null,"EA",2381.0750000000003,785754.75000000012]
[null,"CC8907074-XL/44",null,"● Size XL/44",null,null,"1 unit",null,"EA",2381.0750000000003,785754.75000000012]
[null,null,null,"EASYCHEM 1B, Chemical reusable protective suit. Gastight available with SCBA outside or inside."]
[null,"CC8807072-M/42",null,"● Size M/42",null,null,"1 unit",null,"EA",1836.3636363636363,606000]
[null,"CC8807072-M/44",null,"● Size M/44",null,null,"1 unit",null,"EA",1836.3636363636363,606000]
[null,"CC8807073-L/42",null,"● Size L/42",null,null,"1 unit",null,"EA",1836.3636363636363,606000]
[null,"CC8807073-L/44",null,"● Size L/44",null,null,"1 unit",null,"EA",1836.3636363636363,606000]
[null,"CC8807073-XL/42",null,"● Size L/46",null,null,"1 unit",null,"EA",1836.3636363636363,606000]
[null,"CC8807073-XL/44",null,"● Size XL/44",null,null,"1 unit",null,"EA",1836.3636363636363,606000]
[null,"A160366",null,"GAS TIGHT TEST KIT for Patrol suit, integrated inflation and measurement system includes accessories to close the face aperture of the Patrol suit, also suitable to test other suits depending on connection types (requires external air supply)",null,null,"1 unit"]
[null,"Technical Workwear |  VENTILATED CHEMICAL PROTECTION"]
[null,"CHEMICAL RESISTANT ANTISTATIC VENTILATED SUITE"]
[]
[null,"CC9480XY1T",null,"HAPICHEM Suit / option : Standard Sole",null,"1 to 5","1 unit","BOX","EA",176.75,58327.5]
[null,"CC9480XY2T",null,"HAPICHEM Suit / option : Anti Slip Sole Sole",null,"1 to 5","1 unit","BOX","EA",184.40151515151513,60852.499999999993]
[null,"CC9480XY3T",null,"HAPICHEM Suit / option : Antistatic Sole",null,"1 to 5","1 unit","BOX","EA",192.81818181818181,63630]

{"sheet":"Fall Protection","index":9,"n_rows":1194,"n_cols":12,"rows_kept":1194,"cut":false,"hidden":false,"merged":[[69,1,69,6],[39,1,39,4],[40,1,40,4],[41,1,41,4],[66,1,66,6],[67,1,67,6],[68,1,68,6]]}
[null,"Fall Protection| NEW PRODUCTS INTRODUCTION"]
["A PIROSSAL MEGJELÖLT MINIMUM RENDELÉSI EGYSÉGEK A KÉSZLET EREJÉIG RENDELHETŐEK! "]
[null,"Reference Number",null,"Product Name / Description","Standard Info","Sizes","Minimum Order / Packaging Unit","Packaging Type","Price Per",null,"NETTÓ EUR LISTA ÁR","NETTÓ FT LISTA ÁR"]
[null,"New Honeywell Miller Falcon Edge for construction/power utilities/O&G"]
[null,1034052,null,"FALCON EDGE 6,2m G 2.Twist 2.Swivel FI","EN 360",null,"1 unit",null,"EA","New",466.16550000000001,153834.61499999999]
[null,1034053,null,"FALCON EDGE 9m G 2.Twist 2.Swivel FI","EN 360",null,"1 unit",null,"EA","New",481.71949999999998,158967.435]
[null,1034054,null,"FALCON EDGE 15m G 2.Twist 2.Swivel FI","EN 360",null,"1 unit",null,"EA","New",567.16549999999995,187164.61499999999]
[null,1034055,null,"FALCON EDGE 18m G 2.Twist 2.Swivel FI","EN 360",null,"1 unit",null,"EA","New",590.49649999999997,194863.845]
[null,1034056,null,"FALCON EDGE 6.2m SS 2.Twist 2Swivel FI","EN 360",null,"1 unit",null,"EA","New",637.10799999999995,210245.63999999998]
[null,1034057,null,"FALCON EDGE 9m SS 2.Twist 2.Swivel FI","EN 360",null,"1 unit",null,"EA","New",668.16549999999995,220494.61499999999]
[null,1034058,null,"FALCON EDGE 15m SS 2.Twist 2.Swivel FI","EN 360",null,"1 unit",null,"EA","New",761.38850000000002,251258.20500000002]
[null,1034059,null,"FALCON EDGE 18m SS 2.Twist 2.Swivel FI","EN 360",null,"1 unit",null,"EA","New",792.49649999999997,261523.845]
[]
[null,"Miller H-Design Quick-fit Vest Harnesses"]
[null,"Miller H-Design harnesses fitted with a new lightweight vest to put them on in an even easier and quicker way."]
[null,"This removable vest is available with 2 points H-Design harnesses with stretch webbing, automatic buckles, sternal loops or D-ring version"]
[null,1032880,null,"Miller H-D Quick-fit",null,null,1,"BAG ","EA","Price increase",24.6738,8142.3540000000003]
[null,1032887,null,"Miller H-D with stretch webbing, quick-fit vest 2pts with automatic buckles, 2 loops, size 1",null,"Size 1 ",1,"BAG ","EA","Price increase",127.58319999999999,42102.455999999998]
[null,1032888,null,"Miller H-D with stretch webbing, quick-fit vest, 2pts with automatic buckles 2 loops, size 2",null,"Size 2 ",1,"BAG ","EA","Price increase",127.58319999999999,42102.455999999998]
[null,1032889,null,"Miller H-D with stretch webbing, quick-fit vest, 2pts with automatic buckles; 2 loops , size 3",null,"Size 3 ",1,"BAG ","EA","Price increase",127.58319999999999,42102.455999999998]
[null,1032890,null,"Miller H-D with stretch webbing, quick-fit vest, D-ring, automatic buckles,size 1",null,"Size 1 ",1,"BAG ","EA","Price increase",133.19160000000002,43953.22800000001]
[null,1032891,null,"Miller H-D with stretch webbing, quick-fit vest, D-ring, automatic buckles, size 2",null,"Size 2 ",1,"BAG ","EA","Price increase",133.19160000000002,43953.22800000001]
[null,1032892,null,"Miller H-D with stretch webbing, quick-fit vest, D-ring, automatic buckles",null,"Size 3 ",1,"BAG ","EA","Price increase",133.19160000000002,43953.22800000001]
[null,1032895,null,"H-Design high visibility yellow vest. ",null,"Size 1-2 ",1,"BAG ","EA","Price increase",113.1384,37335.671999999999]
[null,1032896,null,"H-Design high visibility yellow vest\n",null,"Size 1-2 ",1,"BAG ","EA","Price increase",113.1384,37335.671999999999]
[null,1032897,null,"H-Design high visibility orange vest.",null,"Size 1-2",1,"BAG ","EA","Price increase",113.1384,37335.671999999999]
[null,1032898,null,"H-Design high visibility orange vest. ",null,"Size 2-3",1,"BAG ","EA","Price increase",113.1384,37335.671999999999]
[null,1032917,null,"Miller H-Design harness with stretch webbing, 2 loops, auto buckles + high visibility yellow vest. ",null,"Size 1 ",1,"BAG ","EA","Price increase",216.3218,71386.194000000003]
[null,1032918,null,"Miller H-Design harness with stretch webbing, 2 loops, auto buckles + high visibility yellow vest, size. ",null,"Size 2 ",1,"BAG ","EA","Price increase",216.3218,71386.194000000003]
[null,1032919,null,"Miller H-Design harness with stretch webbing, 2 loops, auto buckles + high visibility yellow vest. ",null,"Size 3 ",1,"BAG ","EA","Price increase",216.3218,71386.194000000003]
[null,1032929,null,"Miller H-Design harness with stretch webbing, 2 loops, auto buckles + high visibility orange vest. ",null,"Size 1 ",1,"BAG ","EA","Price increase",220.60560000000001,72799.847999999998]
[null,1032930,null,"Miller H-Design harness with stretch webbing, 2 loops, auto buckles + high visibility orange vest. ",null,"Size 2 ",1,"BAG ","EA","Price increase",220.60560000000001,72799.847999999998]
[null,1032931,null,"Miller H-Design harness with stretch webbing, 2 loops, auto buckles + high visibility orange vest. ",null,"Size 3 ",1,"BAG ","EA","Price increase",220.60560000000001,72799.847999999998]
[null,1032920,null,"Miller H-Design harness with stretch webbing, 2 D-rings, auto buckles + high visibility yellow vest, size 1. Miller H-Design harness with stretch webbing, 2 D-rings, ref 1032875 with high visiblity yellow vest.",null,"Size 1 ",1,"BAG ","EA","Price increase",223.16579999999999,73644.713999999993]
[null,1032921,null,"Miller H-Design harness with stretch webbing, 2 D-rings, auto buckles + high visibility yellow vest, size 2. Miller H-Design harness with stretch webbing, 2 D-rings, ref 1032876 with high visiblity yellow vest.",null,"Size 2 ",1,"BAG ","EA","Price increase",223.16579999999999,73644.713999999993]
[null,1032922,null,"Miller H-Design harness with stretch webbing, 2 D-rings, auto buckles + high visibility yellow vest, size 3. Miller H-Design harness with stretch webbing, 2 D-rings, ref 1032877 with high visiblity yellow vest.",null,"Size 3 ",1,"BAG ","EA","Price increase",223.16579999999999,73644.713999999993]
[null,1032932,null,"Miller H-Design harness with stretch webbing, 2 D-rings, auto buckles + high visibility orange vest - size 1. Miller H-Design harness with stretch webbing, 2 D-rings, ref 1032875 with high visiblity orange vest.",null,"Size 1 ",1,"BAG ","EA","Price increase",223.16579999999999,73644.713999999993]
[null,1032933,null,"Miller H-Design harness with stretch webbing, 2 D-rings, auto buckles + high visibility orange vest - size 2. Miller H-Design harness with stretch webbing, 2 D-rings, ref 1032876 with high visiblity orange vest.",null,"Size 2 ",1,"BAG ","EA","Price increase",223.16579999999999,73644.713999999993]
[null,1032934,null,"Miller H-Design harness with stretch webbing, 2 D-rings, auto buckles + high visibility orange vest - size 3. Miller H-Design harness with stretch webbing, 22 D-rings, ref 1032877 with high visiblity orange vest.",null,"Size 3 ",1,"BAG ","EA","Price increase",223.16579999999999,73644.713999999993]
[null,"MILLER EDGE TESTED SELF- RETRACTKING LIFELINES "]
[null,"Whilst the risk of failure on an edge is often present during work at height, this hazard is relatively unkown. Miller developed a solution to this problem with a range of Edge-Tested self-retracting lifelines to ensure safety in the event of falls on edges !"]
[null,"One product fits all work situations : "]
[null,1033464,null,"Miller edge-tested 2 meter webbing self-retracting lifeline with a twist lock karabiner and a scaffold hook 60 mm with integrated swivel.",null,null,1,"BAG ","EA","Price increase",211.191,69693.03]
[null,1033465,null,"Miller Edged tested 2 meter webbing self-retracting lifeline with 1 alu. twist lock karabiner & 1 swivel alu. twist lock karabiner 21 mm.",null,null,1,"BAG ","EA","Price increase",190.58699999999999,62893.71]
[null,1033466,null,"Miller Edged tested 2 meter webbing self-retracting lifeline with a twist lock karabiner and a swivel scaff hook GO60 opening 60 mm.",null,null,1,"BAG ","EA","Price increase",224.8159,74189.247000000003]
[null,1033467,null,"Miller Edged tested 2 meter webbing self- retracting lifeline without karabiner.",null,null,1,"BAG ","EA","Price increase",167.3065,55211.144999999997]
[]
[null,"NEW!!"]
[null,"Miller H-Design™ confined space harness"]
[null,"Harness with unique quick access to respiratory mask for self-rescue.A new harness dedicated to working in confined spaces, especially water treatment operations.This innovative H-shaped harness "]
[null,"provides a unique comfort solution and is equipped with a comfortable belt to wear a self-rescuer mask."]
[null,1033860,null,"NEW! Miller H-Design™ Confined Space Harness Size 1.2 points harness with 2 webbing loops at the front and automatic buckles on chest and legs straps.This harness includes the confined space belt - Size 1. Shoulder Straps : Duraflex Stretch 44,5 mm webbing PES with PTFE treatment (water repellent / anti stain) Colour : green with a black drawing Breaking strength : > 2200 daN. Other Straps : Standard black webbing 44 mm PES with PTFE treatment (water repellent / anti stain) Breaking strength :> 2700 daN. Back Anchorage D-ring : Material : steel Finish : Zinc plated Silver Breaking strength : > 2300 daN","EN 361","Size 1",1,null,"EA","Price increase",129.45840000000001,42721.272000000004]
[null,1033861,null,"NEW! Miller H-Design™ Confined Space Harness Size 2. 2 points harness with 2 webbing loops at the front and automatic buckles on chest and legs straps.This harness includes the confined space belt - Size 2.","EN 361","Size 2",1,null,"EA","Price increase",129.45840000000001,42721.272000000004]
[null,1033862,null,"NEW!! Miller H-Design™ Confined Space Harness Size 3. 2 points harness with 2 webbing loops at the front and automatic buckles on chest and legs straps.This harness includes the confined space belt - Size 3.","EN 361","Size 3",1,null,"EA","Price increase",129.45840000000001,42721.272000000004]
[null,1033561,null,"NEW!! Miller H-Design ‘confined space' Belt S/M. A newly designed belt, specifically developed to wear a self-rescuer mask, fits perfectly on the state-of-the-art Miller H-Design harness. The belt together with the H-shaped harness offer a unique safety solution for people working in confined spaces, especially in the water treatment sector. Available in 2 sizes. QUICK ACCESS FOR MORE SAFETY: The self-rescuer mask slides smoothly along the belt (from back to front and reverse) enabling quick access in case of an emergency. The soft, flexible and lightweight padded belt is adjustable in height for more comfort, improving the worker’s focus on the job. The self-rescuer mask can be placed either on the front, side, or back of the harness for great freedom of movement. Weight: 0,6 kg",null,null,1,null,"EA","Price increase",58.364399999999996,19260.252]
[null,1033562,null,"NEW!! Miller H-Design ‘confined space' Belt L/XL",null,null,1,null,"EA","Price increase",58.364399999999996,19260.252]
[]
[null,"Miller H-Design™ BodyFix harness"]
[null,"This new harness range dedicated to the utilities sector is a unique solution which offers improved freedom of movement and is less restrictive due to its exclusive and innovate "]
[null,"H shaped harness, with a comfortable waist belt. The new range is available with two easy-to-access front anchor point options: two large, thin webbing loops, or a patented sternal D-ring"]
[null,1033512,null,"Miller H-Design™ BodyFix mating 2LO, with 2 sternal webbing loops at the front and mating buckles on chest and legs straps. Size 1.",null,1,1,null,"EA","Price increase",111.0168,36635.544000000002]
[null,1033513,null,"Miller H-Design™ BodyFix harness with 2 sternal webbing loops at the front and mating buckles on chest and legs straps. Size 2. ",null,2,1,null,"EA","Price increase",111.0168,36635.544000000002]
[null,1033514,null,"Miller H-Design™ BodyFix harness with 2 sternal webbing loops at the front and mating buckles on chest and legs straps. Size 3.\n",null,3,1,null,"EA","Price increase",111.0168,36635.544000000002]
[null,1033516,null,"Miller H-Design™ BodyFix harness with 1 D-ring at the front and mating buckles on chest and legs straps. Size 1.",null,1,1,null,"EA","Price increase",118.36080000000001,39059.064000000006]
[null,1033517,null,"Miller H-Design™ BodyFix harness with 1 D-ring at the front and mating buckles on chest and legs straps. Size 2.",null,2,1,null,"EA","Price increase",118.36080000000001,39059.064000000006]
[null,1033518,null,"Miller H-Design™ BodyFix harness with 1 D-ring at the front and mating buckles on chest and legs straps. Size 3.",null,3,1,null,"EA","Price increase",118.36080000000001,39059.064000000006]
[null,"Miller H-Design™ BodyFit harness"]
[null,"This new harness range dedicated to the utilities sector, which due to its exclusive and innovative H shaped harness, rotating and vertical adjustment waist belt, provides a uniquely comfortable"]
[null,"solution and a perfect fit to all body shapes. The new range is available with two easy-to-access front anchor point options: two large, thin webbing loops , or a patented sternal D-ring."]
[null,"Mating buckles or automatic buckles can also be selected."]
[]
[null,1033528,null,"Miller H-Design™ BodyFit harness with 2 sternal webbing loops and mating buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",1,null,"1 unit","EA","Price increase",126.4722,41735.826000000001]
[null,1033529,null,"Miller H-Design™ BodyFit harness with 2 sternal webbing loops and mating buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",2,null,"1 unit","EA","Price increase",126.4722,41735.826000000001]
[null,1033530,null,"Miller H-Design™ BodyFit harness with 2 sternal webbing loops and mating buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",3,null,"1 unit","EA","Price increase",126.4722,41735.826000000001]
[null,1033532,null,"Miller H-Design™ BodyFit harness with 1 D-ring at the front and mating buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",1,null,"1 unit","EA","Price increase",133.6533,44105.589]
[null,1033533,null,"Miller H-Design™ BodyFit harness with 1 D-ring at the front and mating buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",2,null,"1 unit","EA","Price increase",133.6533,44105.589]
[null,1033534,null,"Miller H-Design™ BodyFit harness with 1 D-ring at the front and mating buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",3,null,"1 unit","EA","Price increase",133.6533,44105.589]
[null,1033536,null,"Miller H-Design™ BodyFit  Auto harness with 2 sternal webbing loops and automatic buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",1,null,"1 unit","EA","Price increase",171.29599999999999,56527.68]
[null,1033537,null,"Miller H-Design™ BodyFit auto 2LO Size 2,  with 2 sternal webbing loops and automatic buckles on chest and legs straps and DuraFlex stretch webbing","EN 361\nEN 358",2,null,"1 unit","EA","Price increase",171.29599999999999,56527.68]
[null,1033538,null,"Miller H-Design™ BodyFit auto 2LO Size 3,  with 2 sternal webbing loops and automatic buckles on chest and legs straps and DuraFlex stretch webbing.","EN 361\nEN 358",3,null,"1 unit","EA","Price increase",171.29599999999999,56527.68]
[null,1033540,null,"Miller H-Design™ BodyFit auto 2D - size 1, full body harness with automatic buckles on chest and legs straps, 1 front D ring and DuraFlex stretch webbing","EN 361\nEN 358",1,null,"1 unit","EA","Price increase",174.48759999999999,57580.907999999996]
[null,1033541,null,"Miller H-Design™ BodyFit auto 2D - size 2, ull body harness with automatic buckles on chest and legs straps, 1 front D ring and DuraFlex stretch webbing.","EN 361\nEN 358",2,null,"1 unit","EA","Price increase",174.48759999999999,57580.907999999996]
[null,1033542,null,"Miller H-Design™ BodyFit auto 2D - size 3,  full body harness with automatic buckles on chest and legs straps, 1 front D ring and DuraFlex stretch webbing","EN 361\nEN 358",3,null,"1 unit","EA","Price increase",174.48759999999999,57580.907999999996]
[null,1033442,null,"NEW!! Miller Universal Kit with 2 pts HDD harness. \nKit composed of a H-design Duraflex 2 pts harness with auto. buckles -size 2 (ref 1032872) and a turbolite Self retractile lifeline with scaffold hook (ref 1018013) + anchorage sling 1,2M (ref 1008363). Supplied into the Miller black backbag.",null,null,1,"1 unit","EA","Price increase",254.7422,84064.925999999992]
[null,1033870,null,"NEW!! Miller H-D Duraflex 1 pt rapco Backpack kit. \nKit composed of a H-design Duraflex 1 pt harness size 2 (ref 1032856) and a Manyard 2M with scaffold hook (ref 1005325). Supplied into the Miller black backbag.",null,null,1,"1 unit","EA","Price increase",165.42789999999999,54591.206999999995]
[null,1033777,null,"NEW!!! Miller Roofing Kits . All in one solution for Roofers looking for a lightweight and comfortable solution to work safely and freely on roofs.",null,null,1,"1 unit","EA","Price increase",211.66569999999999,69849.680999999997]
[null,1033778,null,"NEW!!! Miller H-Design Starter Scaffolding Kit.\nKit composed of a H-design Duraflex 2 loops auto. buckle harness size 2 (ref 1032872) and a Twin edge tested fall arrest kernmentel lanyard 1,5 M + 2 GO55 (ref 1032388). Supplied into the Miller black backbag.",null,null,1,"1 unit","EA","Price increase",220.62440000000001,72806.051999999996]
[null,1033811,null,"NEW !!! Lanyard Fastening Ring Kit.Replacement rings for park points on Miller H-Design or Revolution harnesses. Supplied by set of 10 pcs.",null,null,1,"1 unit","EA","Price increase",8.5068000000000001,2807.2440000000001]
[null,1008331,null,"NEW !!!  AVIABLOC 2,5m + 2 CS20 SANS CARTER",null,null,1,"1 unit","EA","Price increase",84.686599999999999,27946.578000000001]
[null,1010893,null,"NEW !!!AVIABLOC 2,5m+CS20+MOUSQ.TOURILLON",null,null,1,"1 unit","EA","Price increase",111.82709999999999,36902.942999999999]
[]
[null,"MILLER H-DESIGN HARNESS"]
[null,"The Miller H-Design™ harnesses are the new generation ofharnesses dedicated to construction and general industry sectors "]
[null,"and safety to workers. providing more comfort, freedom of movements."]
[null,"It 's brand new innovative and ergonomically-defined H-architecture has been specially designed to provide a unique"]
[null," comfort and freedom of movements to users to let them concentrate on their job and do a great work at height."]
[null,"This new range is declined with Mating buckles or Automatic buckles. "]
[null,1032831,null,"Miller  H-Design Non Stretch, 1 point ","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",52.193400000000004,17223.822]
[null,1032832,null,"Miller  H-Design Non Stretch, 1 point ","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",52.193400000000004,17223.822]
[null,1032833,null,"Miller  H-Design Non Stretch, 1 point ","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",52.193400000000004,17223.822]
[null,1032835,null,"Miller  H-Design Non Stretch, 1 point","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",75.163799999999995,24804.054]
[null,1032836,null,"Miller  H-Design Non Stretch, 1 point ","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",75.163799999999995,24804.054]
[null,1032837,null,"Miller  H-Design Non Stretch, 1 poin","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",75.163799999999995,24804.054]
[null,1032839,null,"Miller  H-Design Non Stretch , 2 points, 2 web loops","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",58.456200000000003,19290.546000000002]
[null,1032840,null,"Miller  H-Design Non Stretch , 2 points, 2 web loops","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",58.456200000000003,19290.546000000002]
[null,1032841,null,"Miller  H-Design Non Stretch , 2 points, 2 web loops","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",58.456200000000003,19290.546000000002]
[null,1032847,null,"Miller  H-Design Non Stretch , 2 points, 2 web loops","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",81.426599999999993,26870.777999999998]
[null,1032848,null,"Miller  H-Design Non Stretch , 2 points, 2 web loops","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",81.426599999999993,26870.777999999998]
[null,1032849,null,"Miller  H-Design Non Stretch , 2 points, 1 D ring ","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",81.426599999999993,26870.777999999998]
[null,1032843,null,"Miller  H-Design Non Stretch , 2 points, 1 D ring ","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",61.067399999999999,20152.241999999998]
[null,1032844,null,"Miller  H-Design Non Stretch , 2 points, 1 D ring ","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",61.067399999999999,20152.241999999998]
[null,1032845,null,"Miller  H-Design Non Stretch , 2 points, 1 D ring ","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",61.067399999999999,20152.241999999998]
[null,1032851,null,"Miller  H-Design Non Stretch , 2 points, 1 D ring ","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",84.037800000000004,27732.474000000002]
[null,1032852,null,"Miller  H-Design Non Stretch , 2 points, 1 D ring ","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",84.037800000000004,27732.474000000002]
[null,1032853,null,"Miller  H-Design Non Stretch , 2 points, 1 D ring ","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",84.037800000000004,27732.474000000002]
[null,1032855,null,"Miller  H-Design Duraflex, Stretch, 1 point","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",73.699699999999993,24320.900999999998]
[null,1032856,null,"Miller  H-Design Duraflex, Stretch, 1 point ","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",73.699699999999993,24320.900999999998]
[null,1032857,null,"Miller  H-Design Duraflex, Stretch, 1 point","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",73.699699999999993,24320.900999999998]
[null,1032859,null,"Miller  H-Design Duraflex, Stretch, 1 point","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",98.124000000000009,32380.920000000002]
[null,1032860,null,"Miller  H-Design Duraflex, Stretch, 1 point","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",98.124000000000009,32380.920000000002]
[null,1032861,null,"Miller  H-Design Duraflex, Stretch, 1 point ","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",98.124000000000009,32380.920000000002]
[null,1032863,null,"Miller  H-Design Duraflex, Stretch, 2 points, 2 web loops","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",79.325400000000002,26177.382000000001]
[null,1032864,null,"Miller  H-Design Duraflex, Stretch, 2 points, 2 web loops","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",79.325400000000002,26177.382000000001]
[null,1032865,null,"Miller  H-Design Duraflex, Stretch, 2 points, 2 web loops","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",79.325400000000002,26177.382000000001]
[null,1032871,null,"Miller  H-Design Duraflex, Stretch, 2 points, 2 web loops","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",101.8484,33609.972000000002]
[null,1032872,null,"Miller  H-Design Duraflex, Stretch, 2 points, 2 web loops","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",101.8484,33609.972000000002]
[null,1032873,null,"Miller  H-Design Duraflex, Stretch, 2 points, 2 web loops","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",101.8484,33609.972000000002]
[null,1032867,null,"Miller  H-Design Duraflex, Stretch, 2 points, 1 D ring ","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",81.890799999999999,27023.964]
[null,1032868,null,"Miller  H-Design Duraflex, Stretch, 2 points, 1 D ring","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",81.890799999999999,27023.964]
[null,1032869,null,"Miller  H-Design Duraflex, Stretch, 2 points, 1 D ring ","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",81.890799999999999,27023.964]
[null,1032875,null,"Miller  H-Design Duraflex, Stretch, 2 points, 1 D ring ","EN 361  ISO 9001",1,"1 unit","1 unit","EA","Price increase",104.41379999999999,34456.553999999996]
[null,1032876,null,"Miller  H-Design Duraflex, Stretch, 2 points, 1 D ring ","EN 361  ISO 9001",2,"1 unit","1 unit","EA","Price increase",104.41379999999999,34456.553999999996]
[null,1032877,null,"Miller  H-Design Duraflex, Stretch, 2 points, 1 D ring ","EN 361  ISO 9001",3,"1 unit","1 unit","EA","Price increase",104.41379999999999,34456.553999999996]
[null,"NEW!!"]
[null,"R'TST  HARNESS"]
[null,"The Miller R’TST 2 points harness is designed specifically for  utility workers, particularly in the electrical high tension sector, "]
[null,"as it provides them with maximum comfort and flexibility when carrying out maintenance on overhead power lines."]
[null,"Delivered with a screw gate karabiner."]
[null,"1003018/R",null,"R'TST. 2-point full body harness with belt and semi-rigid seat strap - Rear and front anchorage loops and side D-rings.Developed for extended reach work where excellent work positioning comfort is required, with long periods of work in suspension.Shoulder straps : Stretched black web. 44 mm Material : 100% polyamide Breaking strength : > 2200 daN.Back D ring and side D rings: stainless steel Ø 7mm Breaking strength: > 5000 daN.Automatic buckles: Stainless steel & aluminium Breaking strength: > 900 daN. Comfortable ,quilted back pad : cordura black foam Provided with 2 fall arrest indicators. Weight: 2,8 Kgs.EN 361: Fall arrest harness - EN 358: work positioning.","EN 361 EN 358","S","1 unit","1 unit","EA","Price increase",393.24059999999997,129769.39799999999]
[null,"1003017/R",null,"R'TST","EN 361 EN 358","M","1 unit","1 unit","EA","Price increase",393.24059999999997,129769.39799999999]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  TITAN",null,null,null,null,""]
[null,"TITAN FULL BODY HARNESSES",null,null,null,null,""]
[null,1011890,null,"TITAN 1-point harness, back D-ring","EN361",null,"1 unit","","EA","Price increase",22.2301,7335.933]
[null,1011891,null,"TITAN 2-point Harness, back D-ring and front webbing loops","EN361",null,"1 unit","","EA","Price increase",27.724499999999999,9149.0849999999991]
[null,1011893,null,"TITAN 1-point harness, back D-ring, with work positioning belt","EN361\nEN358",null,"1 unit","","EA","Price increase",43.5642,14376.186]
[null,1011894,null,"TITAN 2-point harness, back D-ring and front webbing loops, with work positioning belt","EN361\nEN358",null,"1 unit","","EA","Price increase",50.277799999999999,16591.673999999999]
[null,1008232,null,"TITAN work positioning belt","EN358",null,"1 unit","","EA","Price increase",24.398400000000002,8051.4720000000007]
[null,"TITAN ENERGY ABSORBING LANYARDS",null,null,null,null,""]
[null,1008275,null,"TITAN B rope energy absorbing lanyard, no connector,                                    \n● Length 1.8m","EN355",null,"1 unit","","EA","Price increase",34.710599999999999,11454.498]
[null,1008276,null,"TITAN B1 rope energy absorbing lanyard + Karabiner + Snaphook,\n● Length 2m","EN355",null,"1 unit","","EA","Price increase",47.215800000000002,15581.214]
[null,1008281,null,"TITAN C3 rope energy absorbing lanyard + Karabiner + Scaffold hook,\n● Length 2m","EN355",null,"1 unit","","EA","Price increase",54.570300000000003,18008.199000000001]
[null,1014330,null,"TITAN A2 webbing shock absorbing lanyard with 2 screwgate karabiners,\n● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",34.323,11326.59]
[null,null,null,"TITAN A3 webbing energy absorbing lanyard + Karabiner + Scaffold hook",null,null,""]
[null,"Fall Protection |  TITAN",null,null,null,null,""]
[null,1013430,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",51.267599999999995,16918.307999999997]
[null,1015140,null,"● Length 1.75m","EN355",null,"1 unit","","EA","Price increase",49.429200000000002,16311.636]
[null,1013431,null,"TITAN forked webbing energy absorbing lanyard + Karabiner + 2 Scaffold hooks,\n● Length 2m","EN355",null,"1 unit","","EA","Price increase",69.912199999999999,23071.025999999998]
[null,1008282,null,"TITAN N energy absorber, no lanyard","EN355",null,"1 unit","","EA","Price increase",21.572999999999997,7119.0899999999992]
[null,"TITAN POSITIONING AND RESTRAINT LANYARDS",null,null,null,null,""]
[null,1008270,null,"TITAN F12/100 Lanyard, length 1m (no connector)","EN354",null,"1 unit","","EA","Price increase",9.6594000000000015,3187.6020000000003]
[null,1008271,null,"TITAN F12/150 Lanyard, length 1.5m (no connector)","EN354",null,"1 unit","","EA","Price increase",8.7720000000000002,2894.76]
[null,1008272,null,"TITAN F12/200 Lanyard, length 2m (no connector)","EN354",null,"1 unit","","EA","Price increase",10.1286,3342.4380000000001]
[null,1008273,null,"TITAN R14 Adjustable lanyard, length 0.9m to 1.8m (no connector)","EN354",null,"1 unit","","EA","Price increase",15.728400000000001,5190.3720000000003]
[null,1008285,null,"TITAN Work positioning lanyard EN358 lanyard without connectors,\n● Length 1.8m","EN358",null,"1 unit","","EA","Price increase",14.473799999999999,4776.3539999999994]
[null,1008286,null,"TITAN Work positioning lanyard with loop and snap hook,\n● Length 2m","EN358",null,"1 unit","","EA","Price increase",19.5228,6442.5240000000003]
[null,1008287,null,"TITAN Work positioning lanyard with loop and twistlock karabiner,\n● Length 2m","EN358",null,"1 unit","","EA","Price increase",29.259699999999999,9655.7009999999991]
[null,1008288,null,"TITAN Work positioning lanyard with 2 twistlock karabiners,\n● Length 2m","EN358",null,"1 unit","","EA","Price increase",46.490299999999998,15341.798999999999]
[null,"TITAN RETRACTABLE WEBBING LIFELINE",null,null,null,null,""]
[null,1008332,null,"TITAN CMS + Plastic housing, no connectors","EN360",null,"1 unit","","EA","Price increase",64.3673,21241.208999999999]
[null,"TITAN ROPE GRAB AND ANCHORAGE LINE",null,null,null,null,""]
[null,1011190,null,"TITAN Automatic rope grab with 10m x 12mm twisted polyamide rope anchorage line and connector","EN353-2",null,"1 unit","","EA","Price increase",65.78,21707.4]
[null,1011700,null,"TITAN Automatic rope grab with 15m x 12mm twisted rope anchorage line","EN353-2",null,"1 unit","","EA","Price increase",75.358399999999989,24868.271999999997]
[null,1011191,null,"TITAN Automatic rope grab with 20m x 12mm twisted rope anchorage line","EN353-2",null,"1 unit","","EA","Price increase",86.340800000000002,28492.464]
[null,1011192,null,"TITAN Automatic rope grab with 30m x 12mm twisted rope anchorage line","EN353-2",null,"1 unit","","EA","Price increase",101.8056,33595.847999999998]
[null,1011344,null,"TITAN 10m x 12mm twisted polyamide rope anchorage line and connector","EN696",null,"1 unit","","EA","Price increase",41.121600000000001,13570.128000000001]
[null,1011345,null,"TITAN 20m x 12mm twisted polyamide rope anchorage line and connector","EN696",null,"1 unit","","EA","Price increase",57.564,18996.12]
[null,1011346,null,"TITAN 30m x 12mm twisted polyamide rope anchorage line and connector","EN696",null,"1 unit","","EA","Price increase",67.76639999999999,22362.911999999997]
[null,"TITAN ANCHORAGE SLINGS",null,null,null,null,""]
[null,1008360,null,"TITAN Anchorage Sling 0.6m","EN795",null,"1 unit","","EA","Price increase",4.9712000000000005,1640.4960000000001]
[null,1008361,null,"TITAN Anchorage Sling 0.8m","EN795",null,"1 unit","","EA","Price increase",5.3768000000000002,1774.3440000000001]
[null,1008363,null,"TITAN Anchorage Sling 1.2m","EN795",null,"1 unit","","EA","Price increase",7.3423999999999996,2422.9919999999997]
[null,1008364,null,"TITAN Anchorage Sling 1.5m","EN795",null,"1 unit","","EA","Price increase",8.5175999999999998,2810.808]
[null,"Fall Protection |  TITAN",null,null,null,null,""]
[null,"TITAN KITS",null,null,null,null,""]
[null,1011895,null,"TITAN Roofers Kit; 2 point harness and 10m rope with automatic rope grab","EN361\nEN353-2",null,"1 unit","","EA","Price increase",114.4128,37756.224000000002]
[null,1017846,null,"TITAN Scaffolders Kit - Rope; 1 point harness with a 2m energy absorbing rope lanyard, karabiner and scaffold hook","EN361\nEN355",null,"1 unit",null,"EA","Price increase",82.079399999999993,27086.201999999997]
[null,1011896,null,"TITAN Fall Arrest Kit - Rope; 1 point harness with a 2m energy absorbing rope lanyard and 2 karabiners","EN361\nEN355",null,"1 unit","","EA","Price increase",67.235699999999994,22187.780999999999]
[null,1011897,null,"TITAN Restraint Kit; 1 point harness with 2m restraint lanyard and 2 karabiners","EN361\nEN354",null,"1 unit","","EA","Price increase",53.5199,17661.566999999999]
[null,1011898,null,"TITAN Construction kit; 1 point harness with a 2.5m retractable lanyard and 2 karabiners","EN361\nEN360",null,"1 unit","","EA","Price increase",97.787400000000005,32269.842000000001]
[null,1011899,null,"TITAN Work positioning kit; 2 point harness with belt, 2.5m retractable lanyard and positioning lanyard","EN361\nEN360\nEN358",null,"1 unit","","EA","Price increase",147.49199999999999,48672.359999999993]
[null,1013731,null,"TITAN Fall Arrest Kit - Webbing (Kit 6); 1 point harness with a 2m energy absorbing webbing lanyard (stitched to harness D-ring) and karabiner, includes small plastic carry case\n(replaces 1006880 and 1002913)","EN361\nEN355",null,"1 unit","","EA","Price increase",98.531999999999996,32515.559999999998]
[null,1013640,null,"TITAN Scaffolders Kit - Webbing (Kit 7); 1 point harness with a 2m energy absorbing webbing lanyard (stitched to harness D-ring) and scaff hook, includes a small plastic carry case\n(replaces 1006881 and 1002914)","EN361\nEN355",null,"1 unit","","EA","Price increase",118.03440000000001,38951.351999999999]
[null,"Fall Protection |  HARNESSES",null,null,null,null,""]
[null,"ROPAX HARNESS",null,null,null,null,""]
[null,"The ROPAX harness is a full body harness for rope access and rescue. The design combines excellent suspension comfort with"]
[null,"freedom of movement and increased productivity."]
[null,1014434,null,"ROPAX rope access harness with mating leg strap buckles, standard black webbing, size S / M","EN361\nEN358\nEN813",null,"1 unit","","EA","Price increase",229.3707,75692.331000000006]
[null,1014435,null,"ROPAX rope access harness with mating leg strap buckles, standard black webbing, size L / XL","EN361\nEN358\nEN813",null,"1 unit","","EA","Price increase",229.3707,75692.331000000006]
[null,1014432,null,"ROPAX rope access harness with quick connect leg strap buckles, standard black webbing, size S / M","EN361\nEN358\nEN813",null,"1 unit","","EA","Price increase",249.19819999999999,82235.405999999988]
[null,1014433,null,"ROPAX rope access harness with quick connect leg strap buckles, standard black webbing, size L / XL","EN361\nEN358\nEN813",null,"1 unit","","EA","Price increase",249.19819999999999,82235.405999999988]
[null,1015110,null,"ROPAX rope access harness with quick connect leg strap buckles, DualTechTM comfort black / grey webbing, size S / M","EN361\nEN358\nEN813",null,"1 unit","","EA","Price increase",272.12640000000005,89801.712000000014]
[null,1015111,null,"ROPAX rope access harness with quick connect leg strap buckles, DualTechTM comfort black / grey webbing, size L / XL","EN361\nEN358\nEN813",null,"1 unit","","EA","Price increase",272.12640000000005,89801.712000000014]
[null,"ACCESSORIES",null,null,null,null,""]
[null,1015205,null,"Dorsal Ergo soft pad",null,null,"1 unit","","EA","Price increase"]
[null,1015206,null,"Transversal 3D padded support",null,null,"1 unit","","EA","Price increase"]
[null,"ATEX HARNESS",null,null,null,null,""]
[null,null,null,"ATEX 2-point anti-static harness with protective back pad and automatic buckles, front anchorage webbing loops and rear anchorage extension with webbing loop, conforms to ATEX 949CE for use in explosive atmospheres, for use with other ATEX approved equipment, e.g. 1015859 lanyard and 1017921 SRL","EN361\nATEX\n949CE",null,""]
[null,1015074,null,"● Size Small / Medium",null,null,"1 unit","","EA","Price increase",201.654,66545.819999999992]
[null,1015075,null,"● Size Large / XL",null,null,"1 unit","","EA","Price increase",201.654,66545.819999999992]
[null,"WELDER'S HARNESSES",null,null,null,null,""]
[null,"Welder's harnesses combine Kevlar and Nomex for resistance to high temperature and welding spatter"]
[null,null,null,"751K Kevlar / Nomex full body harness with mating buckles and back D-ring, single adjustment point on leg-loops",null,null,""]
[null,null,null,null,null,null,""]
[null,null,null,"650K Kevlar / Nomex full body harness with sub-pelvic support strap, tool belt loops, mating buckles and back D-ring, adjustment points on leg-loop and front webbing strap",null,null,""]
[null,1012336,null,"● Size Small / Medium","EN361",null,"1 unit","","EA","Price increase",367.18979999999999,121172.63399999999]
[null,1012337,null,"● Size Large / XL","EN361",null,"1 unit","","EA","Price increase",367.18979999999999,121172.63399999999]
[null,1012338,null,"● Size XXL","EN361",null,"1 unit","","EA","Price increase",386.77379999999999,127635.35399999999]
[null,"Fall Protection |  HARNESSES",null,null,null,null,""]
[null,"REVOLUTION HARNESS"]
[null,"R1 REVOLUTION Basic construction and maintenance harness"]
[null,1014220,null,"● DuraFlex Webbing - Size S / M","EN361",null,"1 unit","","EA","Price increase",133.77519999999998,44145.815999999992]
[null,1014231,null,"● DuraFlex Webbing - Size L / XL","EN361",null,"1 unit","","EA","Price increase",133.77519999999998,44145.815999999992]
[null,1014232,null,"● DuraFlex Webbing - Size XXL (Made to Order)","EN361",null,"1 unit","","EA","Price increase",147.13919999999999,48555.935999999994]
[null,1014233,null,"● DualTech Webbing - Size S / M","EN361",null,"1 unit","","EA","Price increase",133.77519999999998,44145.815999999992]
[null,1014234,null,"● DualTech Webbing - Size L / XL","EN361",null,"1 unit","","EA","Price increase",133.77519999999998,44145.815999999992]
[null,1014235,null,"● DualTech Webbing - Size XXL (Made to Order)","EN361",null,"1 unit","","EA","Price increase",147.13919999999999,48555.935999999994]
[null,"R2 REVOLUTION Comfort construction and maintenance harness"]
[null,1014236,null,"● DuraFlex Webbing - Size S / M","EN361",null,"1 unit","","EA","Price increase",188.2741,62130.453000000001]
[null,1014237,null,"● DuraFlex Webbing - Size L / XL","EN361",null,"1 unit","","EA","Price increase",188.2741,62130.453000000001]
[null,1014238,null,"● DuraFlex Webbing - Size XXL (Made to Order)","EN361",null,"1 unit","","EA","Price increase",211.2012,69696.395999999993]
[null,1014239,null,"● DualTech Webbing - Size S / M","EN361",null,"1 unit","","EA","Price increase",191.99459999999999,63358.217999999993]
[null,1014240,null,"● DualTech Webbing - Size L / XL","EN361",null,"1 unit","","EA","Price increase",191.99459999999999,63358.217999999993]
[null,1014241,null,"● DualTech Webbing - Size XXL (Made to Order)","EN361",null,"1 unit","","EA","Price increase",211.2012,69696.395999999993]
[null,null,null,null,null,null,""]
[null,"R3 REVOLUTION Premium construction and maintenance harness",null,null,null,null,""]
[null,1014242,null,"● DualTech Webbing - Size S / M","EN361/358",null,"1 unit","","EA","Price increase",257.06720000000001,84832.176000000007]
[null,1014243,null,"● DualTech Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",257.06720000000001,84832.176000000007]
[null,1014244,null,"● DualTech Webbing - Size XXL (Made to Order)","EN361/358",null,"1 unit","","EA","Price increase",285.52160000000003,94222.128000000012]
[null,null,null,null,null,null,""]
[null,"R4 REVOLUTION Telecom and utilities harness",null,null,null,null,""]
[null,1014245,null,"● DuraFlex Webbing - Size S / M","EN361/358",null,"1 unit","","EA","Price increase",229.60080000000002,75768.26400000001]
[null,1014246,null,"● DuraFlex Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",229.60080000000002,75768.26400000001]
[null,1014247,null,"● DuraFlex Webbing - Size XXL (Made to Order)","EN361/358",null,"1 unit","","EA","Price increase",252.57440000000003,83349.552000000011]
[null,1014248,null,"● DualTech Webbing - Size S / M","EN361/358",null,"1 unit","","EA","Price increase",227.39600000000002,75040.680000000008]
[null,1014249,null,"● DualTech Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",227.39600000000002,75040.680000000008]
[null,1014250,null,"● DualTech Webbing - Size XXL (Made to Order)","EN361/358",null,"1 unit","","EA","Price increase",252.57440000000003,83349.552000000011]
[null,null,null,null,null,null,""]
[null,"R5 REVOLUTION Premium telecom and utilities harness",null,null,null,null,""]
[null,1014251,null,"● DuraFlex Webbing - Size S / M","EN361/358",null,"1 unit","","EA","Price increase",247.2278,81585.173999999999]
[null,1014252,null,"● DuraFlex Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",247.2278,81585.173999999999]
[null,1014253,null,"● DuraFlex Webbing - Size XXL (Made to Order)","EN361/358",null,"1 unit","","EA","Price increase",277.33799999999997,91521.54]
[null,1014254,null,"● DualTech Webbing - Size S / M","EN361/358",null,"1 unit","","EA","Price increase",252.12360000000001,83200.788]
[null,1014255,null,"● DualTech Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",252.12360000000001,83200.788]
[null,1014256,null,"● DualTech Webbing - Size XXL (Made to Order)","EN361/358",null,"1 unit","","EA","Price increase",277.33799999999997,91521.54]
[null,null,null,null,null,null,""]
[null,"R6 REVOLUTION 4-point Premium utilities harness",null,null,null,null,""]
[null,1014257,null,"● DuraFlex Webbing - Size S / M","EN361/358",null,"1 unit","","EA","Price increase",308.99440000000004,101968.15200000002]
[null,1014258,null,"● DuraFlex Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",308.99440000000004,101968.15200000002]
[null,1014259,null,"● DuraFlex Webbing - Size XXL (Made to Order)","EN361/358",null,"1 unit","","EA","Price increase",339.88240000000002,112161.19200000001]
[null,1014260,null,"● DualTech Webbing - Size S / M","EN361/358",null,"1 unit","","EA","Price increase",308.99440000000004,101968.15200000002]
[null,1014261,null,"● DualTech Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",308.99440000000004,101968.15200000002]
[null,1014262,null,"● DualTech Webbing - Size XXL (Made to Order)","EN361/358",null,"1 unit","","EA","Price increase",339.88240000000002,112161.19200000001]
[null,null,null,null,null,null,""]
[null,"R7 REVOLUTION Wind harness",null,null,null,null,""]
[null,1035200,null,"R7 WIND II REVOLUTION WORLWIDE S/M - For onshore wind energy application. Fitted with 2pts (Dorsal D and sternal loops), quick connect buckles.","EN361/358",null,"1 unit",null,"EA","NEW",295.03500000000003,97361.55]
[null,1035201,null,"R7 WIND II REVOLUTION WORLWIDE L/XL - For onshore wind energy application. Fitted with 2pts (Dorsal D and sternal loops), quick connect buckles.","EN361/358",null,"1 unit",null,"EA","NEW",295.03500000000003,97361.55]
[null,1035202,null,"R7 WIND II REVOLUTION WORLWIDE XXL - For onshore wind energy application. Fitted with 2pts (Dorsal D and sternal loops), quick connect buckles.","EN361/358",null,"1 unit",null,"EA","NEW",295.03500000000003,97361.55]
[null,null,null,null,null,null,""]
[null,"R7 REVOLUTION Offshore harness",null,null,null,null,""]
[null,"1014807/OFFS",null,"● DualTech Webbing - Size S/M","EN361/358",null,"1 unit",null,"EA","NEW",468.97559999999999,154761.948]
[null,"1014808/OFFS",null,"● DualTech Webbing - Size L / XL","EN361/358",null,"1 unit","","EA","Price increase",468.97559999999999,154761.948]
[null,"1014809/OFFS",null,"● DualTech Webbing - Size XXL","EN361/358",null,"1 unit","","EA","Price increase",515.79359999999997,170211.88799999998]
[null,null,null,null,null,null,""]
[null,"R8 REVOLUTION Worldwide harness",null,null,null,null,""]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  HARNESSES",null,null,null,null,""]
[null,"REVOLUTION ACCESSORIES"]
[null,"The PivotLink™ Connection provides an attachment point for a multitude of accessories and individual tool pouches"]
[null,"Once attached the accessory pivots to maintain a level position"]
[null,null,null,null,null,null,""]
[null,1014270,null,"Mini mobile phone holder ",null,null,"1 unit","","EA","Price increase",13.616999999999999,4493.6099999999997]
[null,1014271,null,"Regular mobile phone / hand-held radio holder",null,null,"1 unit","","EA","Price increase",36.192,11943.36]
[null,1014272,null,"Water bottle holder (bottle not included)",null,null,"1 unit","","EA","Price increase",29.591999999999999,9765.3599999999988]
[null,1014273,null,"Large open bolt and bull pin bag; height: 22cm, width: 31cm, depth: 14cm ",null,null,"1 unit","","EA","Price increase",34.216000000000001,11291.28]
[null,1014274,null,"Medium open bolt and bull pin bag; height: 16cm,  width: 19cm, depth: 13cm ",null,null,"1 unit","","EA","Price increase",32.583199999999998,10752.456]
[null,1014275,null,"Two-pocket nail and tool pouch, height: 16cm, width: 19cm, depth: 13cm ",null,null,"1 unit","","EA","Price increase",25.448799999999999,8398.1039999999994]
[null,1014276,null,"Shoulder / leg pads; Removable foam filled pad for shoulder and thigh comfort / protection",null,null,"1 unit","","EA","Price increase",40.024799999999999,13208.183999999999]
[null,1014277,null,"Universal accessory and belt attachment clip",null,null,"1 unit","","EA","Price increase",3.8045999999999998,1255.518]
[null,1015050,null,"Large Multi-Pouch Tool Bag w/2 Steel Hammer Loops, height:29cm, width: 19cm ",null,null,"1 unit","","EA","Price increase",72.176000000000002,23818.080000000002]
[null,1016080,null,"Padded Hammer Loop",null,null,"1 unit",null,"EA","Price increase",22.943999999999999,7571.5199999999995]
[null,1015510,null,"Zippered Cylindrical Utility Pouch",null,null,"1 unit","","EA","Price increase",47.631999999999998,15718.56]
[null,1016480,null,"Bolt and Tool Bag with Velcro and push fit latch closures, three metal D rings within to secure tools, three drainage holes with integral mesh to prevent loss of small objects, reinforcement at base, 23cm x 8cm x 23cm, Weight 285g",null,null,"1 unit","","EA","Price increase",40.749000000000002,13447.17]
[null,1014278,null,"Blue self-adhesive label with write in window",null,null,"1 unit","","EA","Price increase",22.7864,7519.5119999999997]
[null,1014279,null,"Yellow self-adhesive label with write in window",null,null,"1 unit","","EA","Price increase",22.7864,7519.5119999999997]
[null,1014280,null,"Red self-adhesive label with write in window",null,null,"1 unit","","EA","Price increase",22.7864,7519.5119999999997]
[null,1014281,null,"Green self-adhesive label with write in window",null,null,"1 unit","","EA","Price increase",22.348199999999999,7374.9059999999999]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  ENERGY ABSORBING LANYARDS",null,null,null,null,""]
[null,"BARRACUDA Scaffold Clamp",null,null,null,null,""]
[null,"Barracuda is the ultimate fall protection solution for scaffolders; the innovative scaffold clamp is easily fitted to a vertical"]
[null,"scaffold pole using one hand thus allowing scaffolders to keep one hand free for carrying tools or for steadying themselves"]
[null,"● BSIF Product Innovation Award Winner 2004",null,null,null,null,""]
[null,1010470,null,"BARRACUDA scaffold clamp with Manyard, length 1.75m","EN355\nEN795",null,"1 unit","","EA","Price increase",200.3484,66114.971999999994]
[null,1010141,null,"BARRACUDA scaffold clamp with energy absorbing rope lanyard, length 1.75m","EN355\nEN795",null,"1 unit","","EA","Price increase",187.88399999999999,62001.719999999994]
[null,1008671,null,"BARRACUDA scaffold clamp with adjustable energy absorbing rope lanyard, length 0.7m to 1.2m","EN355\nEN795",null,"1 unit","","EA","Price increase",196.01339999999999,64684.421999999999]
[null,"EDGE-TESTED MANYARDS - Stretchable energy absorbing lanyards tested for use over an edge"]
[null,null,null,"Miller by Honeywell edge-tested Manyards are stretchable for reduced trip hazard and"]
[null,null,null,"are tested for falls over an edge, available with different connectors"]
[null,null,null,"● BSiF Product Innovation Commended Award 2009"]
[null,1017916,null,"EDGE-TESTED MANYARD with aluminium scaffold hook and aluminium screwgate karabiner, length 2m","EN355",null,"1 unit","","EA","Price increase",82.001899999999992,27060.626999999997]
[null,1017918,null,"EDGE-TESTED MANYARD with two aluminium screwgate connectors, length 2m","EN355",null,"1 unit","","EA","Price increase",72.287400000000005,23854.842000000001]
[null,null,null,"TWIN EDGE-TESTED MANYARD with twistlock karabiner and 2 steel 55mm hooks",null,null,"1 unit"]
[null,1028520,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",148.80330000000001,49105.089]
[null,1028521,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",157.98419999999999,52134.785999999993]
[null,null,null,"TWIN EDGE-TESTED MANYARD with twistlock karabiner and 2 aluminium 65mm hooks",null,null,"1 unit"]
[null,1028522,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",176.18440000000001,58140.852000000006]
[null,1028523,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",167.21559999999999,55181.148000000001]
[null,"MANYARD",null,null,null,null,""]
[null,"Stretchable energy absorbing lanyard for reduced tripping hazards",null,null,null,null,""]
[null,null,null,"ME82 MANYARD with 2 galvanised connectors (CS20)",null,null,""]
[null,1005317,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",58.711200000000005,19374.696]
[null,1005318,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",61.118400000000001,20169.072]
[null,null,null,"ME83 MANYARD with snap hook and galvanised connector",null,null,""]
[null,1005326,null,"● Length 1.5m","EN355",null,"1 unit","BOX","EA","Price increase",57.181200000000004,18869.796000000002]
[null,1005327,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",61.179599999999994,20189.267999999996]
[null,null,null,"ME86 MANYARD with scaffold hook and galvanised connector",null,null,""]
[null,1005324,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",77.652599999999993,25625.357999999997]
[null,1005325,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",81.997799999999998,27059.273999999998]
[null,null,null,"Twin MANYARD with galvanised connector and 2 scaffold hooks (63mm)",null,null,""]
[null,1013970,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",131.90639999999999,43529.111999999994]
[null,1013491,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",140.57640000000001,46390.212]
[null,null,null,null,null,null,""]
[null,"NEW SHOCK ABSORBING KERNMANTEL ROPE LANYARDS",null,null,null,null,""]
[null,null,null,"A new comprehensive range of Edge-Tested kernmantel rope lanyards"]
[null,null,null,"Edge-Tested lanyards are designed to withstand falls over an edge"]
[null,null,null,"Manufactured from high quality abrasion resistant kernmantel rope"]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, thimble terminations, no connectors"]
[null,1032363,null," ● Length 0.8m","EN355",null,"1 unit","","EA","Price increase",35.883600000000001,11841.588]
[null,1032364,null," ● Length 1.3m","EN355",null,"1 unit","","EA","Price increase",37.525799999999997,12383.513999999999]
[null,1032365,null," ● Length 1.8m","EN355",null,"1 unit","","EA","Price increase",39.157800000000002,12922.074000000001]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 2 x CS20 steel screwgate karabiners"]
[null,1032366,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",48.949800000000003,16153.434000000001]
[null,1032367,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",50.571599999999997,16688.628000000001]
[null,1032368,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",54.386400000000002,17947.511999999999]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 2 x CS20 steel twistlock karabiners"]
[null,1032369,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",58.741800000000005,19384.794000000002]
[null,1032370,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",60.363599999999998,19919.988000000001]
[null,1032371,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",61.995600000000003,20458.548000000003]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 1 x CS20 steel twistlock karabiner and 1 x GO55 steel scaffold hook"]
[null,1032372,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",67.442400000000006,22255.992000000002]
[null,1032373,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",67.720500000000001,22347.764999999999]
[null,1032374,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",70.696200000000005,23329.746000000003]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 1 x Zicral aluminium twistlock karabiner and 1 x GO60 aluminium double action hook"]
[null,1032375,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",81.579599999999999,26921.268]
[null,1032376,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",81.587800000000001,26923.974000000002]
[null,1032377,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",84.833399999999997,27995.022000000001]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 1 x Zicral aluminium twistlock karabiner and 1 x GO65 aluminium scaffold hook"]
[null,1032378,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",75.592200000000005,24945.426000000003]
[null,1032379,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",75.729799999999997,24990.833999999999]
[null,1032380,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",77.325600000000009,25517.448000000004]
[]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 1 x  Zicral aluminium twistlock karabiner and 1 x aluminium snaphook"]
[null,1032381,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",74.510999999999996,24588.629999999997]
[null,1032382,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",76.132800000000003,25123.824000000001]
[null,1032383,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",77.764799999999994,25662.383999999998]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 2 x Cigale steel triple lock karabiners"]
[null,1032408,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",72.338400000000007,23871.672000000002]
[null,1032409,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",73.9602,24406.866000000002]
[null,null,null,null,null,null,""]
[null,null,null,"Shock absorbing lanyard, kernmantel rope, 1 x Cigale steel triple lock karabiner and 1 x GO65 aluminium scaffold hook"]
[null,1032410,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",83.211600000000004,27459.828000000001]
[null,1032411,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",84.833399999999997,27995.022000000001]
[null,null,null,"\nShock absorbing lanyard, kernmantel rope, 1 x  Zicral aluminium twistlock karabiner and 1 x GO100 aluminium scaffold hook"]
[null,1032610,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",119.646,39483.18]
[null,1032611,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",121.27800000000001,40021.740000000005]
[null,null,null,"\nTwin shock absorbing lanyard, kernmantel rope, thimble terminations, no connectors"]
[null,1032384,null," ● Length 0.8m","EN355",null,"1 unit","","EA","Price increase",55.467600000000004,18304.308000000001]
[null,1032385,null," ● Length 1.3m","EN355",null,"1 unit","","EA","Price increase",58.741800000000005,19384.794000000002]
[null,1032386,null," ● Length 1.8m","EN355",null,"1 unit","","EA","Price increase",61.995600000000003,20458.548000000003]
[null,null,null,"\nTwin shock absorbing lanyard, kernmantel rope, 1 x CS20 steel twistlock karabiner and 2 x GO55 steel scaffold hooks"]
[null,1032387,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",100.0722,33023.826000000001]
[null,1032388,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",101.3232,33436.656000000003]
[null,1032389,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",106.59,35174.700000000004]
[null,null,null,"\nTwin shock absorbing lanyard, kernmantel rope, 1 x Zicral aluminium twistlock karabiner and 2 x GO60 aluminium double action hook"]
[null,1032390,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",130.1284,42942.372000000003]
[null,1032391,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",135.95579999999998,44865.413999999997]
[null,1032392,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",139.22999999999999,45945.899999999994]
[null,null,null,"\nTwin shock absorbing lanyard, kernmantel rope, 1 x Zicral aluminium twistlock karabiner and 2 x GO65 aluminium scaffold hooks"]
[null,1032393,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",113.11800000000001,37328.94]
[null,1032394,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",114.13,37662.9]
[null,1032395,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",119.646,39483.18]
[null,null,null,"\nTwin shock absorbing lanyard, kernmantel rope, 1 x Zicral aluminium twistlock karabiner and 2 x aluminium snaphooks"]
[null,1032396,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",108.7728,35895.023999999998]
[null,1032397,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",112.0368,36972.144]
[null,1032398,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",115.2906,38045.898000000001]
[null,null,null,"\nTwin shock absorbing lanyard, kernmantel rope, 1 x Cigale steel triple lock karabiner and 2 x GO65 aluminium scaffold hooks"]
[null,1032412,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",121.8186,40200.137999999999]
[null,1032413,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",125.0826,41277.258000000002]
[null,null,null,"\nTwin shock absorbing lanyard, kernmantel rope, 1 x Cigale steel triple lock karabiner and 2 x GO100 aluminium scaffold hooks"]
[null,1032414,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",176.20500000000001,58147.65]
[null,1032415,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",179.4588,59221.404000000002]
[null,null,null,null,null,null,""]
[null,"EDGE-TESTED Lanyards - Energy absorbing lanyards tested for use over an edge"]
[null,null,null,"Miller by Honeywell edge-tested lanyards are designed and tested for falls over an edge"]
[null,null,null,"Manufactured from 12mm diameter kernmantel rope and available with different connectors"]
[null,null,null,"● BSIF Product Innovation Commended Award 2009"]
[null,1016847,null,"EDGE-TESTED lanyard with aluminium scaffold hook and aluminium snap hook, length 2m","EN355",null,"1 unit","","EA","Price increase",83.616,27593.279999999999]
[null,1016848,null,"EDGE-TESTED lanyard with 2 steel screwgate connectors, length 2m","EN355",null,"1 unit","","EA","Price increase",63.637599999999999,21000.407999999999]
[null,1016849,null,"EDGE-TESTED lanyard with aluminium scaffold hook and steel screwgate connector, length 2m","EN355",null,"1 unit","","EA","Price increase",87.59920000000001,28907.736000000004]
[null,1016850,null,"EDGE-TESTED lanyard with 2 aluminium scaffold hooks and one steel screwgate connector, length 1.5m","EN355",null,"1 unit","","EA","Price increase",123.94720000000001,40902.576000000001]
[null,"ENERGY ABSORBING WEBBING LANYARDS",null,null,null,null,""]
[null,1002901,null,"ME00 23mm webbing lanyard with energy absorber, no connectors, length 1.8m","EN355",null,"1 unit","","EA","Price increase",41.839199999999998,13806.936]
[null,1002902,null,"ME01 23mm forked webbing lanyard with energy absorber, three galvanised connectors (CS20), 18mm opening, length 2m","EN355",null,"1 unit","","EA","Price increase",90.063999999999993,29721.119999999999]
[null,1002903,null,"ME02 23mm webbing lanyard with energy absorber, two galvanised connectors (CS20), 18mm opening, length 2m","EN355",null,"1 unit","","EA","Price increase",62.462400000000002,20612.592000000001]
[null,1002904,null,"ME03 23mm webbing lanyard with energy absorber, two aluminium connectors (ML06), 17mm opening, length 2m","EN355",null,"1 unit","","EA","Price increase",90.063999999999993,29721.119999999999]
[null,1004590,null,"ME05 Forked webbing energy-absorbing lanyard, c/w karabiner and two 50mm scaffold hooks · Length 2m","EN355",null,"1 unit","","EA","Price increase",100.73439999999999,33242.351999999999]
[null,"ENERGY ABSORBING WEBBING LANYARDS"]
[null,null,null,"ME06 Webbing energy-absorbing lanyard, c/w karabiner and 50mm scaffold hook",null,null,""]
[null,1005279,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",58.645600000000002,19353.047999999999]
[null,1004579,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",60.881599999999999,20090.928]
[null,"ATEX LANYARD",null,null,null,null,""]
[null,1015859,null,"ATEX LANYARD; forked webbing energy-absorbing lanyard with karabiner and two GO60 hooks, length 1.15m","EN355",null,"1 unit","","EA","Price increase",195.75839999999999,64600.271999999997]
[null,"ENERGY ABSORBING ROPE LANYARDS",null,null,null,null,""]
[null,1002905,null,"ME50 12mm polyamide rope lanyard with energy absorber, no connectors, length 1.8m","EN355",null,"1 unit","","EA","Price increase",66.045000000000002,21794.850000000002]
[null,1002906,null,"ME51 12mm polyamide rope lanyard with energy absorber, one galvanised connector (CS20) with 18mm opening and one aluminium connector (ML04) with 63mm opening, length 2m","EN355",null,"1 unit","","EA","Price increase",82.08720000000001,27088.776000000002]
[null,1002907,null,"ME52 12mm polyamide rope lanyard with energy absorber, two galvanised connectors (CS20), 18mm opening, length 2m","EN355",null,"1 unit","","EA","Price increase",59.040800000000004,19483.464]
[null,null,null,"ME53 Rope energy-absorbing lanyard, c/w karabiner and snap hook",null,null,""]
[null,1005290,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",59.602400000000003,19668.792000000001]
[null,1004578,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",63.648000000000003,21003.84]
[null,null,null,"ME54 Rope energy-absorbing lanyard, c/w karabiner and 50mm scaffold hook",null,null,""]
[null,1005278,null,"● Length 1.5m","EN355",null,"1 unit","","EA","Price increase",67.911999999999992,22410.959999999999]
[null,1004591,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",75.992799999999988,25077.623999999996]
[null,"LANYARD ACCESSORY",null,null,null,null,""]
[null,1016334,null,"Pull-away parking point for safe attachment of lanyard when not in use",null,null,"1 unit","","EA","Price increase",3.0090000000000003,992.97000000000014]
[null,"NEW KERNMANTEL ROPE RESTRAINT LANYARDS",null,null,null,null,""]
[null,null,null,"Restraint lanyard, kernmantel rope, thimble terminations, no connectors"]
[null,1032330,null," ● Length 0.8m","EN354",null,"1 unit","","EA","Price increase",14.1372,4665.2759999999998]
[null,1032331,null," ● Length 1.3m","EN354",null,"1 unit","","EA","Price increase",15.769200000000001,5203.8360000000002]
[null,1032332,null," ● Length 1.8m","EN354",null,"1 unit","","EA","Price increase",17.401199999999999,5742.3959999999997]
[null,null,null,"Restraint lanyard, kernmantel rope, 2 x CS20 steel screwgate karabiners"]
[null,1032333,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",24.532899999999998,8095.8569999999991]
[null,1032334,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",26.128700000000002,8622.4710000000014]
[null,1032335,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",27.7346,9152.4179999999997]
[null,null,null,"Restraint lanyard, kernmantel rope, 2 x CS20 steel twistlock karabiners"]
[null,1032336,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",32.629799999999996,10767.833999999999]
[null,1032337,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",34.261800000000001,11306.394]
[null,1032338,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",35.883600000000001,11841.588]
[null,null,null,"Restraint lanyard, kernmantel rope, 1 x CS20 steel twistlock karabiner and 1 x GO55 steel scaffold hook"]
[null,1032339,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",38.076599999999999,12565.278]
[null,1032340,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",38.935499999999998,12848.714999999998]
[null,1032341,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",41.330400000000004,13639.032000000001]
[null,null,null,"Restraint lanyard, kernmantel rope, 1 x Zicral aluminium twistlock karabiner and 1 x GO65 aluminium scaffold hook"]
[null,1032342,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",58.660799999999995,19358.063999999998]
[null,1032343,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",61.444800000000001,20276.784]
[null,1032344,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",63.087000000000003,20818.710000000003]
[null,null,null,"Restraint lanyard, kernmantel rope, 1 x  Zicral aluminium twistlock karabiner and 1 x aluminium snaphook"]
[null,1032345,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",58.741800000000005,19384.794000000002]
[null,1032346,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",60.363599999999998,19919.988000000001]
[null,1032347,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",61.995600000000003,20458.548000000003]
[null,null,null,"Restraint lanyard, kernmantel rope, 1 x Cigale steel triple lock karabiner and 1 x GO65 aluminium scaffold hook"]
[null,1032402,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",68.523600000000002,22612.788]
[null,1032403,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",70.155600000000007,23151.348000000002]
[null,null,null,"Restraint lanyard, kernmantel rope, 2 x Cigale steel triple lock karabiners"]
[null,1032404,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",43.503,14355.99]
[null,1032405,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",45.134999999999998,14894.55]
[null,null,null,null,null,null,""]
[null,"NEW KERNMANTEL ROPE RESTRAINT LANYARDS",null,null,null,null,""]
[null,null,null,"Twin kernmantel rope restraint lanyard, thimble terminations, no connectors"]
[null,1032348,null," ● Length 0.8m","EN354",null,"1 unit","","EA","Price increase",21.756599999999999,7179.6779999999999]
[null,1032349,null," ● Length 1.3m","EN354",null,"1 unit","","EA","Price increase",25.010400000000001,8253.4320000000007]
[null,1032350,null," ● Length 1.8m","EN354",null,"1 unit","","EA","Price increase",28.284600000000001,9333.9179999999997]
[null,null,null,"Twin kernmantel rope restraint lanyard, 1 x CS20 steel twistlock karabiner and 2 x GO55 steel scaffold hooks"]
[null,1032351,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",63.993600000000001,21117.887999999999]
[null,1032352,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",67.185199999999995,22171.115999999998]
[null,1032353,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",71.787599999999998,23689.907999999999]
[null,null,null,"\nTwin kernmantel rope restraint lanyard, 1 x Zicral aluminium twistlock karabiner and 2 x GO60 aluminium double action hooks"]
[null,1032354,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",101.1534,33380.622000000003]
[null,1032355,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",104.4174,34457.741999999998]
[null,1032356,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",107.6712,35531.495999999999]
[null,null,null,"Twin kernmantel rope restraint lanyard, 1 x Zicral aluminium twistlock karabiner and 2 x GO65 aluminium scaffold hooks"]
[null,1032357,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",98.980800000000002,32663.664000000001]
[null,1032358,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",102.2448,33740.784]
[null,1032359,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",107.6712,35531.495999999999]
[null,null,null,"Twin kernmantel rope restraint lanyard, 1 x Zicral aluminium twistlock karabiner and 2 x aluminium snaphooks"]
[null,1032360,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",101.1534,33380.622000000003]
[null,1032361,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",104.4174,34457.741999999998]
[null,1032362,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",107.6712,35531.495999999999]
[null,null,null,"Twin kernmantel rope restraint lanyard, 1 x Cigale steel triple lock karabiner and 2 x GO65 aluminium scaffold hooks"]
[null,1032406,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",107.14080000000001,35356.464000000007]
[null,1032407,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",108.7728,35895.023999999998]
[null,null,null,null,null,null,""]
[null,"RESTRAINT LANYARDS",null,null,null,null,""]
[null,null,null,"MD00 12mm polyamide rope lanyard with loop and galvanised connector (CS20), 18mm opening"]
[null,1002881,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",19.032,6280.56]
[null,1002882,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",23.004799999999999,7591.5839999999998]
[null,null,null,"MD02 12mm polyamide rope lanyard with two galvanised connectors (CS20), 18mm opening"]
[null,1002883,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",27.799199999999999,9173.735999999999]
[null,1004711,null,"● Length 1.5m","EN354",null,"1 unit","","EA","Price increase",29.1616,9623.3279999999995]
[null,1002884,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",30.3888,10028.304]
[null,null,null,"MD04 12mm polyamide rope lanyard with galvanised connector (CS20), 18mm opening, and aluminium connector (ML04), 63mm opening"]
[null,1002885,null,"● Length 1m","EN354",null,"1 unit","","EA","Price increase",72.529599999999988,23934.767999999996]
[null,1002886,null,"● Length 2m","EN354",null,"1 unit","","EA","Price increase",77.708799999999997,25643.903999999999]
[null,1004582,null,"MD08 12mm polyamide rope lanyard with galvanised connector (CS20), 18mm opening and double action hook · Length 2m","EN354",null,"1 unit","","EA","Price increase",34.323,11326.59]
[null,1004576,null,"MD09 12mm polyamide rope lanyard with galvanised connector (CS20), 18mm opening and 50mm scaffold hook · Length 2m","EN354",null,"1 unit","","EA","Price increase",56.191200000000002,18543.096000000001]
[null,"CONNECTION LANYARDS",null,null,null,null,""]
[null,1030951,null,"Forked lanyard, 25mm polyester webbing includes two 1018960 karabiners, use with MA08 / MA58 harness front anchorage to form a front anchorage point, length 0.4m, weight 0.43kg ","EN354",null,"1 unit","","EA","Price increase",34.139400000000002,11266.002]
[null,1002888,null,"MD07 12mm polyamide rope lanyard with galvanised connector (CS20), 18mm opening, for use with MicroLoc rope grab · Length 0.3m","EN354",null,"1 unit","","EA","Price increase",31.376800000000003,10354.344000000001]
[null,1002889,null,"MD50 webbing extension for harness rear anchorage; allows  the user to connect / disconnect to a fall arrest system without assistance · Length 0.3m","EN354",null,"1 unit","","EA","Price increase",17.076800000000002,5635.344000000001]
[null,"HEIGHT SAFETY KITS",null,null,null,null,""]
[null,null,null,"FALL ARREST KIT (Kit 8):  1-point Duraflex harness, lanyard c/w energy absorber and scaffold hook 50mm, (sewn direct to harness), small plastic carry case","EN361\nEN355",null,""]
[]
[null,1013732,null,"● Standard kit - length 2m (replaces 1002915)",null,null,"1 unit",null,"EA","Price increase",146.1558,48231.413999999997]
[null,1013733,null,"● Scaffolder's Kit - length 1.75m (replaces 1005795)",null,null,"1 unit",null,"EA","Price increase",146.1558,48231.413999999997]
[null,"Fall Protection |  WORK POSITIONING, RESTRAINT",null,null,null,null,""]
[null,"NEW MILLER HANDZUP WORK POSITIONING LANYARDS "]
[null,"Made principally in aluminium (side plates and compartment) with an ABS handle, HandZup is lightweight and comfortable to use"]
[null,"Stainless steel cam is designed for optimum strength and to enable flexible/smooth one handed rope adjustments"]
[null,"Patented design allows easy access to the inner mechanism for quick and straightforward rope replacement"]
[null,null,null,"HandZup with twistlock karabiner, snaphook and protective sleeve"]
[null,1032097,null,"● Length 2m","EN358",null,"1 unit","","EA","Price increase",118.60430000000001,39139.419000000002]
[null,1032098,null,"● Length 3m","EN358",null,"1 unit","","EA","Price increase",121.85650000000001,40212.645000000004]
[null,1032099,null,"● Length 4m","EN358",null,"1 unit","","EA","Price increase",125.1087,41285.870999999999]
[null,null,null,"HandZup with twistlock karabiner and  snaphook"]
[null,1032100,null,"● Length 2m","EN358",null,"1 unit","","EA","Price increase",113.73609999999999,37532.913]
[null,1032101,null,"● Length 3m","EN358",null,"1 unit","","EA","Price increase",116.9883,38606.138999999996]
[null,1032102,null,"● Length 4m","EN358",null,"1 unit","","EA","Price increase",120.2304,39676.031999999999]
[null,1032240,null,"● Length 5m","EN358",null,"1 unit","","EA","Price increase",123.48260000000001,40749.258000000002]
[null,null,null,"\nHandZup without connectors"]
[null,1032124,null,"● Length 10m","EN358",null,"1 unit","","EA","Price increase",144.16679999999999,47575.044000000002]
[null,1032125,null,"● Length 20m","EN358",null,"1 unit","","EA","Price increase",177.29640000000001,58507.812000000005]
[null,1032126,null,"● Length 30m","EN358",null,"1 unit","","EA","Price increase",210.3648,69420.384000000005]
[null,null,null,"\nHandZup with 2 x Cigale Cigale steel triple lock karabiners and protective sleeve"]
[null,1032118,null,"● Length 2m","EN358",null,"1 unit","","EA","Price increase",123.45059999999999,40738.697999999997]
[null,1032119,null,"● Length 3m","EN358",null,"1 unit","","EA","Price increase",126.75539999999999,41829.281999999999]
[null,1032120,null,"● Length 4m","EN358",null,"1 unit","","EA","Price increase",130.07040000000001,42923.232000000004]
[null,null,null,"\nHandZup with 2 x Cigale steel triple lock karabiners"]
[null,1032121,null,"● Length 2m","EN358",null,"1 unit","","EA","Price increase",118.473,39096.089999999997]
[null,1032122,null,"● Length 3m","EN358",null,"1 unit","","EA","Price increase",121.78800000000001,40190.04]
[null,1032123,null,"● Length 4m","EN358",null,"1 unit","","EA","Price increase",125.0928,41280.623999999996]
[null,"REPLACEMENT ROPE"]
[null,null,null,"HandZup rope with 1 x snaphook"]
[null,1032128,null,"● Length 2m",null,null,"1 unit","","EA","Price increase",46.389599999999994,15308.567999999997]
[null,1032129,null,"● Length 3m",null,null,"1 unit","","EA","Price increase",49.704599999999999,16402.518]
[null,1032130,null,"● Length 4m",null,null,"1 unit","","EA","Price increase",53.019599999999997,17496.468000000001]
[null,1032241,null,"● Length 5m",null,null,"1 unit","","EA","Price increase",56.344799999999999,18593.784]
[null,null,null,"\nHandZup rope with no connectors"]
[null,1032143,null,"● Length 2m",null,null,"1 unit","","EA","Price increase",36.454799999999999,12030.083999999999]
[null,1032144,null,"● Length 3m",null,null,"1 unit","","EA","Price increase",39.769800000000004,13124.034000000001]
[null,1032145,null,"● Length 4m",null,null,"1 unit","","EA","Price increase",43.084800000000001,14217.984]
[null,1032146,null,"● Length 10m",null,null,"1 unit","","EA","Price increase",62.964599999999997,20778.317999999999]
[null,1032147,null,"● Length 20m",null,null,"1 unit","","EA","Price increase",96.094200000000001,31711.085999999999]
[null,1032148,null,"● Length 30m",null,null,"1 unit","","EA","Price increase",129.24420000000001,42650.586000000003]
[null,"ACCESSORIES"]
[null,1032150,null,"HandZup Protective Sleeve",null,null,"1 unit",null,"EA","Price increase",5.8038000000000007,1915.2540000000001]
[null,1032151,null,"HandZup Locking Set",null,null,"1 unit",null,"EA","Price increase",9.1085999999999991,3005.8379999999997]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  WORK POSITIONING, RESTRAINT, ROPE GRABS",null,null,null,null,""]
[null,"TEEKER",null,null,null,null,""]
[null,null,null,"TEEKER restraint system is an all-in-one solution incorporating a restraint belt complete with self adjusting Kevlar lanyard strap",null,null,""]
[null,1029980,null,"● Size:  S / M","EN358",null,"1 unit","","EA","Price increase",413.79360000000003,136551.88800000001]
[null,1029981,null,"● Size:  L / XL","EN358",null,"1 unit","","EA","Price increase",413.79360000000003,136551.88800000001]
[null,"WORK POSITIONING BELTS",null,null,null,null,""]
[null,"WORK POSITIONING LANYARDS",null,null,null,null,""]
[null,1002877,null,"MC00 Work positioning lanyard in 12mm polyamide rope, Length  2m","EN358",null,"1 unit","","EA","Price increase",37.117800000000003,12248.874000000002]
[null,null,null,"Work positioning lanyard in 16mm polyamide rope with aluminium jaw type adjuster                    ",null,null,""]
[null,1002878,null,"● MC01 Length 2m","EN358",null,"1 unit","","EA","Price increase",100.78790000000001,33260.007000000005]
[null,1002879,null,"● MC02 Length 3m","EN358",null,"1 unit","","EA","Price increase",106.1922,35043.425999999999]
[null,1002880,null,"● MC03 Length 4m","EN358",null,"1 unit","","EA","Price increase",109.9866,36295.578000000001]
[null,"ROPE GRABS",null,null,null,null,""]
[null,1002867,null,"MF00 MicroLoc automatic rope grab, 14mm / 16mm","EN353-2",null,"1 unit","","EA","Price increase",86.767199999999988,28633.175999999996]
[null,"MF51 Automatic and manual rope grab for:",null,null,null,null,""]
[null,1002875,null,"● 14mm / 16mm rope","EN353-2",null,"1 unit","","EA","Price increase",71.011200000000002,23433.696]
[null,1007640,null,"● 10mm / 12mm rope","EN353-2",null,"1 unit","","EA","Price increase",59.675200000000004,19692.816000000003]
[null,"Fall Protection |  WORK POSITIONING, RESTRAINT, ROPE GRABS",null,null,null,null,""]
[null,"MF52 Automatic and manual rope grab with lanyard and galvanised connector (CS20) for:",null,null,null,null,""]
[null,1002876,null,"● 14mm / 16mm rope","EN353-2",null,"1 unit","","EA","Price increase",90.74,29944.199999999997]
[null,1007618,null,"● 10mm / 12mm rope","EN353-2",null,"1 unit","","EA","Price increase",87.36,28828.799999999999]
[null,"CABLE GRAB",null,null,null,null,""]
[null,1002868,null,"MG00 MicroLoc automatic wire rope grab, 8mm","EN353-2",null,"1 unit","","EA","Price increase",84.243700000000004,27800.421000000002]
[null,"ROPE ANCHORAGE LINES",null,null,null,null,""]
[null,"Rope anchorage line with karabiner and rubber weight",null,null,null,null,""]
[null,"14 mm diameter twisted rope:",null,null,null,null,""]
[null,1002891,null,"● MH00 - 10m","EN353-1",null,"1 unit","","EA","Price increase",49.14,16216.2]
[null,1002892,null,"● MH01 - 20m","EN353-1",null,"1 unit","","EA","Price increase",74.349599999999995,24535.367999999999]
[null,1002893,null,"● MH02 - 30m","EN353-1",null,"1 unit","","EA","Price increase",100.568,33187.440000000002]
[null,1002894,null,"● MH03 - 40m","EN353-1",null,"1 unit","","EA","Price increase",122.6056,40459.847999999998]
[null,1002895,null,"● MH04 - 50m","EN353-1",null,"1 unit","","EA","Price increase",147.26399999999998,48597.119999999995]
[null,"10.5 mm diameter kernmantel rope:",null,null,null,null,""]
[null,1007613,null,"● MH00 - 10m","EN353-1",null,"1 unit","","EA","Price increase",55.650399999999998,18364.631999999998]
[null,1007614,null,"● MH01 - 20m","EN353-1",null,"1 unit","","EA","Price increase",79.923999999999992,26374.92]
[null,1007615,null,"● MH02 - 30m","EN353-1",null,"1 unit","","EA","Price increase",105.49759999999999,34814.207999999999]
[null,1007616,null,"● MH03 - 40m","EN353-1",null,"1 unit","","EA","Price increase",128.75200000000001,42488.160000000003]
[null,1007617,null,"● MH04 - 50m","EN353-1",null,"1 unit","","EA","Price increase",152.78639999999999,50419.511999999995]
[null,"Fall Protection |  SELF RETRACTING LIFELINES",null,null,null,null,""]
[null,"PERSONAL FALL LIMITERS",null,null,null,null,""]
[null,"TWIN TURBO"]
[null,"Twin Turbo™ D-Ring Connector adapts two TurboLite™ Personal Fall Limiters for continuous 100% tie-off "]
[null,"● BSIF Product Innovation Commended Award 2011"]
[null,1029715,null,"TWIN TURBO D-Ring Connector supplied without TurboLite PFLs, weight 0.395kg","EN362",null,"1 unit","","EA","Price increase",126.7312,41821.296000000002]
[null,1029716,null,"TWIN TURBO D-Ring Connector and two TurboLite PFLs (1018013), weight 2.1kg","EN360",null,"1 unit","","EA","Price increase",396.55559999999997,130863.34799999998]
[null,"TURBOLITE"]
[null,"TurboLite personal fall arrester; Compact and lightweight (0.86kg) retractable webbing lifeline is adapted for situations"]
[null,"where fall clearance is limited. Approved in fall factor 2, anchorage at foot level, (Max 100kg) and fall factor 0, anchorage "]
[null,"above user, (Max 136kg)",null,null,null,null,""]
[null,1018013,null,"TURBOLITE with scaffold hook and twistlock karabiner","EN360",null,"1 unit","","EA","Price increase",134.9562,44535.546000000002]
[null,1018014,null,"TURBOLITE with scaffold hook and twistlock karabiner","EN360",null,"1 unit","","EA","Price increase",134.9562,44535.546000000002]
[null,1018015,null,"TURBOLITE with 2 twistlock karabiners","EN360",null,"1 unit","","EA","Price increase",126.48230000000001,41739.159]
[null,1017900,null,"TURBOLITE with snap hook and twistlock karabiner","EN360",null,"1 unit","","EA","Price increase",149.9547,49485.050999999999]
[null,"EDGE-TESTED Scorpion - Personal fall limiter tested for use over an edge",null,null,null,null,""]
[null,null,null,"Miller by Honeywell edge-tested Scorpion fall limiters are specifically designed and"]
[null,null,null,"tested for falls over an edge and for fall factor 2, connection below the feet"]
[null,null,null,"● BSIF Product Innovation Commended Award 2009"]
[null,1016840,null,"EDGE-TESTED SCORPION with steel screwgate connector, swivel and steel snaphook, length extended 2.6m","EN360",null,"1 unit","","EA","Price increase",165.56220000000002,54635.526000000005]
[null,1016841,null,"EDGE-TESTED SCORPION with aluminium scaffold hook, swivel and aluminium screwgate karabiner length extended 2.7m","EN360",null,"1 unit","","EA","Price increase",196.2047,64747.550999999999]
[null,1016842,null,"EDGE-TESTED SCORPION with steel scaffold hook, swivel and steel snaphook, length extended 2.7m","EN360",null,"1 unit","","EA","Price increase",170.06330000000003,56120.88900000001]
[null,"SCORPION PFL"]
[null,"Both sturdy and lightweight (1.6kg), Scorpion includes a fall indicator and robust internal corrosion resistant components"]
[null,1008587,null,"SCORPION with karabiner and swivel snap hook, 2.7m","EN360",null,"1 unit","","EA","Price increase",145.82740000000001,48123.042000000001]
[null,1008588,null,"SCORPION with swivel scaffold hook and snap hook, 2.8m","EN360",null,"1 unit","","EA","Price increase",147.65049999999999,48724.665000000001]
[null,1008593,null,"SCORPION with lightweight scaffold hook and swivel snap hook, 2.8m","EN360",null,"1 unit","","EA","Price increase",179.2715,59159.595000000001]
[null,1008594,null,"SCORPION with scaffold hook and swivel karabiner, 2.7m","EN360",null,"1 unit","","EA","Price increase",159.547,52650.51]
[null,null,null,null,null,null,""]
[null,"RETRACTABLE LANYARD",null,null,null,null,""]
[null,1002871,null,"MI20 Block, retractable webbing, length 2.5m","EN360",null,"1 unit","","EA","Price increase",108.98909999999999,35966.402999999998]
[null,"MINILITE PFL"]
[null,"Minilite 3m retractable webbing fall limiter with robust and corrosion resistant composite housing"]
[null,"BLACK RHINO CABLE PFL"]
[null,"Black Rhino PFL with retractable cable is suited to harsh work environments; e.g. concrete construction and welding"]
[null,1012410,null,"BLACK RHINO with swivel snap hook and karabiner, 2.7m","EN360",null,"1 unit","","EA","Price increase",229.6591,75787.502999999997]
[null,1012392,null,"BLACK RHINO with scaffold hook and swivel snap hook, 2.85m","EN360",null,"1 unit","","EA","Price increase",249.64109999999999,82381.562999999995]
[null,"FALCON WEBBING SELF RETRACTING LIFELINE"]
[null,"Compact and lightweight (1.5kg) the 6m Falcon webbing SRL provides an exceptional length/weight ratio"]
[null,1016793,null,"FALCON WEBBING SRL, no connectors","EN360",null,"1 unit","","EA","Price increase",333.71410000000003,110125.65300000001]
[null,1016794,null,"FALCON WEBBING SRL with 63mm scaffold hook and karabiner","EN360",null,"1 unit","","EA","Price increase",369.55899999999997,121954.46999999999]
[null,1016795,null,"FALCON WEBBING SRL with 2 karabiners","EN360",null,"1 unit","","EA","Price increase",353.48990000000003,116651.66700000002]
[null,1016796,null,"FALCON WEBBING SRL with karabiner and double action snap hook","EN360",null,"1 unit","","EA","Price increase",358.42880000000002,118281.504]
[null,1031140,null,"FALCON WEBBING SRL with 2 karabiners and Fall Indicator (no annual factory inspection required, an authorised competent person can inspect Falcon Web SRL with Fall Indicator)","EN360",null,"1 unit","","EA","Price increase",356.66129999999998,117698.22899999999]
[null,"FALCON SELF RETRACTING LIFELINES",null,null,null,null,""]
[null,"Approved for horizontal application when used with an extension sling (1002897) and karabiner (1018960) to the harness"]
[null,"No annual factory recertification required, an authorised competent person can inspect Falcon SRL for lower cost of ownership"]
[null,"Swivel snap hook connector with integral load indicator easily identifies when a fall has been arrested"]
[null,"FALCON SRL - GALVANISED CABLE"]
[null,1011728,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 4kg, length 6.2m","EN360",null,"1 unit","","EA","Price increase",474.62479999999999,156626.18400000001]
[null,1011742,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 5kg, length 10m","EN360",null,"1 unit","","EA","Price increase",485.20160000000004,160116.52800000002]
[null,1011746,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 6.7kg, length 15m","EN360",null,"1 unit","","EA","Price increase",548.87040000000002,181127.23200000002]
[null,1011750,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 7.6kg, length 20m","EN360",null,"1 unit","","EA","Price increase",644.8728000000001,212808.02400000003]
[null,"FALCON SRL - STAINLESS STEEL CABLE",null,null,null,null,""]
[null,1011729,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 4kg, length 6.2m","EN360",null,"1 unit","","EA","Price increase",520.79039999999998,171860.83199999999]
[null,1011743,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 5kg, length 10m","EN360",null,"1 unit","","EA","Price increase",554.30960000000005,182922.16800000001]
[null,1011747,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 6.7kg, length 15m","EN360",null,"1 unit","","EA","Price increase",648.25280000000009,213923.42400000003]
[null,1011751,null,"FALCON with top swivel and karabiner, bottom swivel snap hook, weight 7.6kg, length 20m","EN360",null,"1 unit","","EA","Price increase",700.23199999999997,231076.56]
[null,"FALCON SRL - ATEX",null,null,null,null,""]
[null,"For use in explosive atmosphere as part of an ATEX system",null,null,null,null,""]
[null,1017921,null,"FALCON with stainless steel cable, top karabiner, bottom swivel snap hook, weight 5kg, length 10m","EN360",null,"1 unit","","EA","Price increase",646.03760000000011,213192.40800000002]
[null,"FALCON SRL - OFFSHORE",null,null,null,null,""]
[null,"Stainless steel cable, spring and connector for use in coastal and offshore environments",null,null,null,null,""]
[null,1013960,null,"FALCON with bottom st. steel swivel snap hook, weight 4kg, length 6.2m","EN360",null,"1 unit","","EA","Price increase",501.6232,165535.65599999999]
[null,1012261,null,"FALCON with bottom st. steel swivel snap hook,  weight 5kg, length 10m","EN360",null,"1 unit","","EA","Price increase",594.66159999999991,196238.32799999998]
[null,1012262,null,"FALCON with bottom st. steel swivel snap hook, weight 6.7kg, length 15m","EN360",null,"1 unit","","EA","Price increase",688.59440000000006,227236.15200000003]
[null,1012263,null,"FALCON with bottom st. steel swivel snap hook,  weight 7.6kg, length 20m","EN360",null,"1 unit","","EA","Price increase",765.54399999999998,252629.52]
[null,null,null,null,null,null,""]
[null,"FALCON OFFSHORE KIT",null,null,null,null,""]
[null,"A complete 20m fall arrest system designed for exposed locations",null,null,null,null,""]
[null,1028812,null,"FALCON 20m SRL with top stainless steel swivel, bottom stainless steel swivel snaphook, stainless steel cable and spring, protective UV-resistant cover, 1m stainless steel anchor sling with protective sleeve, stainless steel screwgate karabiner, 20m high-visibility drawdown cord","EN360\nEN795",null,"1 unit","","EA","Price increase",995.49840000000006,328514.47200000001]
[null,"MIGHTYEVAC FALL ARREST BLOCKS",null,null,null,null,""]
[null,"1005149-A",null,"MIGHTEVAC galvanised wire rope, length 15m","EN360    EN1496",null,"1 unit","","EA","Price increase",989.8,326634]
[null,"1005160-A",null,"MIGHTEVAC galvanised wire rope, length 30m","EN360    EN1496"," ","1 unit","","EA","Price increase",1578.7107999999998,520974.56399999995]
[null,"1014390-A",null,"MIGHTEVAC stainless steel wire rope, length 15m","EN360    EN1496",null,"1 unit",null,"EA","Price increase",1323.8777,436879.641]
[null,"MIGHTYLITE FALL ARREST BLOCKS",null,null,null,null,""]
[null,1002820,null,"MI50 MIGHTYLITE block, retractable wire rope, length 6.2m","EN360",null,"1 unit","","EA","Price increase",491.28559999999999,162124.24799999999]
[null,1004571,null,"MI54 MIGHTYLITE block, 4.0mm galvanised wire rope, length10m","EN360",null,"1 unit","","EA","Price increase",559.18719999999996,184531.77599999998]
[null,null,null,"MI55 MIGHTYLITE block, length 15m",null,null,""]
[null,1004573,null,"● 4.8mm galvanised wire rope","EN360",null,"1 unit","","EA","Price increase",633.27679999999998,208981.34399999998]
[null,1004592,null,"● 4.8mm stainless steel wire rope","EN360",null,"1 unit","","EA","Price increase",727.58169999999996,240101.96099999998]
[null,1002827,null,"MI70 MIGHTYLITE block, retractable webbing, length 6.2m","EN360",null,"1 unit","","EA","Price increase",529.05840000000001,174589.272]
[null,1002828,null,"MI71 MIGHTYLITE block, retractable webbing, length 15.5m","EN360",null,"1 unit","","EA","Price increase",704.39639999999997,232450.81199999998]
[null,null,null,"MI56 MIGHTYLITE block, length 20m ",null,null,""]
[null,1004572,null,"● 4.8mm galvanised wire rope","EN360",null,"1 unit","","EA","Price increase",753.6880000000001,248717.04000000004]
[null,1004593,null,"● 4.8mm stainless steel wire rope ","EN360",null,"1 unit","","EA","Price increase",895.14210000000003,295396.89299999998]
[null,null,null,"MI57 MIGHTYLITE block, length 30m",null,null,""]
[null,1004574,null,"● 4.8mm galvanised wire rope","EN360",null,"1 unit","","EA","Price increase",967.34559999999999,319224.04800000001]
[null,1004594,null,"● 4.8mm stainless steel wire rope ","EN360",null,"1 unit","","EA","Price increase",1458.1813,481199.82899999997]
[null,null,null,"MI58 MIGHTYLITE block, length 40m ",null,null,""]
[null,1004575,null,"● 4.8mm galvanised wire rope","EN360",null,"1 unit","","EA","Price increase",1570.5976000000001,518297.20800000004]
[null,1004595,null,"● 4.8mm stainless steel wire rope ","EN360",null,"1 unit","","EA","Price increase",1716.5155999999999,566450.14799999993]
[null,"DURASEAL SELF-RETRACTING LIFELINE"]
[null,"1034130-E",null,"DuraSeal Sealed SRL with tagline and 1 karabiner, 15m galvanized steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",1333.4482999999998,440037.93899999995]
[null,"1034131-E",null,"DuraSeal Sealed SRL with tagline and 1 karabiner, 15m stainless steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",1357.7048,448042.58399999997]
[null,"1034132-E",null,"DuraSeal Sealed SRL with tagline and 1 karabiner, 30m galvanized steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",1625.6284000000001,536457.37199999997]
[null,"1034135-E",null,"DuraSeal Sealed SRL with tagline and 1 karabiner, 30m stainless steel cable","EN360",null,"1 unit",{"$f":"$H$693","v":"1 unit"},"EA","Price increase",1875.3519000000001,618866.12700000009]
[null,"1034137-E",null,"DuraSeal Sealed SRL with tagline and 1 karabiner, 40m galvanized steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",2298.0742,758364.48600000003]
[null,"1034139-E",null,"DuraSeal Sealed SRL with tagline and 1 karabiner, 40m stainless steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",2389.4764,788527.21200000006]
[]
[null,"1034133-E",null,"DuraSeal Sealed SRL with tagline, 1 karabiner and 4-hole mounting plate, 30m galvanized steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",1707.2353000000001,563387.64899999998]
[null,"1034136-E",null,"DuraSeal Sealed SRL with tagline, 1 karabiner and 4-hole mounting plate, 30m stainless steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",1956.9588000000001,645796.40399999998]
[null,"1034138-E",null,"DuraSeal Sealed SRL with tagline, 1 karabiner and 4-hole mounting plate, 40m galvanized steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",2379.6810999999998,785294.76299999992]
[null,"1034140-E",null,"DuraSeal Sealed SRL with tagline, 1 karabiner and 4-hole mounting plate, 40m stainless steel cable","EN360",null,"1 unit","1 unit","EA","Price increase",2471.0935999999997,815460.88799999992]
[null,"*Contact us for details of your regional Miller Service Centre for inspection and maintenance of Miller fall arrest blocks "]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  ANCHORAGE POINTS",null,null,null,null,""]
[null,"QUICKLOCK",null,null,null,null,""]
[null,1009728,null,"QUICKLOCK reusable anchor point for concrete applications, suitable for 16mm drill, 90mm deep hole, one hand installation and removal","EN795b",null,"1 unit","","EA","Price increase",96.830300000000008,31953.999000000003]
[null,"TRAVERSE",null,null,null,null,""]
[null,1029585,null,"TRAVERSE temporary internal door anchor for use in a restraint system, suitable for openings up to 900mm  (2 users) or 1100mm (1 user)","EN795",null,"1 unit","","EA","Price increase",198.2441,65420.553]
[null,"TELESCOPIC POLE",null,null,null,null,""]
[null,1002898,null,"MK00 Telescopic pole, length 7.5m",null,null,"1 unit","","EA","Price increase",185.92080000000001,61353.864000000001]
[null,1002899,null,"MK01 Connector for pole, opening: 150mm","EN795",null,"1 unit","","EA","Price increase",136.07330000000002,44904.189000000006]
[null,1002900,null,"MK02 Connector for pole, opening: 63mm","EN795",null,"1 unit","","EA","Price increase",104.46259999999999,34472.657999999996]
[null,"WEBBING SLINGS",null,null,null,null,""]
[null,"Webbing strap anchorage point",null,null,null,null,""]
[null,1002916,null,"Length 0.6m","EN795",null,"1 unit","","EA","Price increase",7.0864000000000003,2338.5120000000002]
[null,1002917,null,"Length 0.8m","EN795",null,"1 unit","","EA","Price increase",7.5808,2501.6640000000002]
[null,1003245,null,"Length 1m","EN795",null,"1 unit","","EA","Price increase",8.2194000000000003,2712.402]
[null,1002918,null,"Length 1.2m","EN795",null,"1 unit","","EA","Price increase",8.9919000000000011,2967.3270000000002]
[null,1002919,null,"Length 1.5m","EN795",null,"1 unit","","EA","Price increase",10.5472,3480.576]
[null,"STEEL SLING",null,null,null,null,""]
[null,1002897,null,"Steel Sling, 1m","EN795",null,"1 unit","","EA","Price increase",34.865500000000004,11505.615000000002]
[null,1003178,null,"Steel Sling, 2m","EN795",null,"1 unit","","EA","Price increase",40.365699999999997,13320.680999999999]
[null,1003179,null,"Steel Sling, 3m","EN795",null,"1 unit","","EA","Price increase",48.234899999999996,15917.516999999998]
[null,"WIRE GIRDER GRIPS",null,null,null,null,""]
[null,1018979,null,"Opening: 75mm","EN362",null,"1 unit","","EA","Price increase",36.513500000000001,12049.455]
[null,1018980,null,"Opening: 100mm ","EN362",null,"1 unit","","EA","Price increase",38.140900000000002,12586.497000000001]
[null,1018981,null,"Opening: 140mm","EN362",null,"1 unit","","EA","Price increase",41.982799999999997,13854.323999999999]
[null,"SERPENT HORIZONTAL LIFELINE",null,null,null,null,""]
[null,1007610,null,"SERPENT 20m horizontal life line, supplied with two webbing slings","EN795",null,"1 unit","","EA","Price increase",347.6044,114709.452]
[null,"ANCHORAGE DEVICE"]
[null,1002996,null,"Anchorage point only","EN795A",null,"1 unit","","EA","Price increase",11.4536,3779.6880000000001]
[null,1003272,null,"Anchorage point with chemical bolt","EN795A",null,"1 unit","","EA","Price increase",23.834199999999999,7865.2860000000001]
[null,1003273,null,"Anchorage point with M12 bolt and nut","EN795A",null,"1 unit","","EA","Price increase",13.729900000000001,4530.8670000000002]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  CONNECTORS",null,null,null,null,""]
[null,"CONNECTORS",null,null,null,null,""]
[null,1018960,null,"CS20 Galvanised screwgate karabiner\nlength 105mm, width 58mm, diameter 10mm, weight 0.18kg, breaking strength: >25kN, opening 17mm (replaces 1002832)","EN362",null,"1 unit","","EA","Price increase",5.7267000000000001,1889.8110000000001]
[null,1009276,null,"CS20 Aluminium screwgate karabiner\nweight 0.085kg, opening 17mm","EN362",null,"1 unit","","EA","Price increase",9.2616999999999994,3056.3609999999999]
[null,1018963,null,"CS20 Galvanised steel twistlock karabiner\nweight 0.172kg, opening 17mm","EN362",null,"1 unit","","EA","Price increase",11.3726,3752.9580000000001]
[null,1008342,null,"Aluminium twistlock karabiner, length 110mm, width 60mm, thickness 18mm, weight 0.090kg, breaking strength: >23KN, opening 18mm","EN362",null,"1 unit","","EA","Price increase",13.9565,4605.6450000000004]
[null,1018961,null,"Light alloy screwgate karabiner, opening 21mm (replaces 1002838)","EN362",null,"1 unit","","EA","Price increase",8.775599999999999,2895.9479999999999]
[null,1018969,null,"ML02 Light alloy twistlock karabiner\nlength 124mm, width 72mm, diameter 11mm, weight 0.085kg, breaking strength: >22kN, opening 20mm (replaces 1002834)","EN362",null,"1 unit","","EA","Price increase",18.395799999999998,6070.6139999999996]
[null,1018968,null,"Twistlock Polished light alloy karabiner, 16mm (replaces 1004316)","EN362",null,"1 unit","","EA","Price increase",17.866900000000001,5896.0770000000002]
[null,1028630,null,"Aluminium triple action twistlock karabiner, \nopening 20mm","EN362",null,"1 unit","","EA","Price increase",20.1983,6665.4390000000003]
[null,1018971,null,"ML03 Light alloy triple action twistlock karabiner, opening 23mm (replaces 1002835)","EN362",null,"1 unit","","EA","Price increase",18.462800000000001,6092.7240000000002]
[null,"1004300/A",null,"GO30 Karabiner Light alloy connector with self locking gate and rope latch, length 160mm, width 75mm, thickness 12mm, weight 0.140kg, breaking strength: >25 kN, opening 30mm","EN362",null,"1 unit","","EA","Price increase",35.1539,11600.787]
[null,1018972,null,"GO60 Karabiner; Light alloy connector 62mm with self locking gate and rope latch (replaces 1004318)","EN362",null,"1 unit","","EA","Price increase",43.904699999999998,14488.550999999999]
[null,1018977,null,"ML04 Aluminium double action scaffold hook, opening: 63mm (replaces 1002836)","EN362",null,"1 unit","","EA","Price increase",48.166899999999998,15895.076999999999]
[null,1002837,null,"ML05 Zinc finished captive eye, twistlock karabiner, opening: 58mm","EN362",null,"1 unit","","EA","Price increase",64.498599999999996,21284.538]
[null,"Fall Protection |  SAFESCAPE ELITE",null,null,null,null,""]
[null,"SAFESCAPE ELITETM controlled rate rope descender device",null,null,null,null,""]
[null,"Supplied in red rope bag with rescue logo",null,null,null,null,""]
[null,1028750,null,"rope length 20m",null,null,"1 unit","","EA","Price increase",832.8374,274836.342]
[null,1028751,null,"rope length 30m",null,null,"1 unit","","EA","Price increase",858.72130000000004,283378.02900000004]
[null,1028752,null,"rope length 40m",null,null,"1 unit","","EA","Price increase",884.62580000000003,291926.51400000002]
[null,1028753,null,"rope length 50m",null,null,"1 unit","","EA","Price increase",910.50970000000007,300468.201]
[null,1028754,null,"rope length 60m",null,null,"1 unit","","EA","Price increase",936.40390000000002,309013.28700000001]
[null,1028755,null,"rope length 70m",null,null,"1 unit","","EA","Price increase",962.27750000000003,317551.57500000001]
[null,1028756,null,"rope length 80m",null,null,"1 unit","","EA","Price increase",988.17169999999999,326096.66100000002]
[null,1028757,null,"rope length 90m",null,null,"1 unit","","EA","Price increase",1014.0658999999999,334641.74699999997]
[null,1028758,null,"rope length 100m",null,null,"1 unit","","EA","Price increase",1039.9601,343186.83299999998]
[null,1028759,null,"rope length 110m",null,null,"1 unit","","EA","Price increase",1065.8336999999999,351725.12099999998]
[null,1028760,null,"rope length 120m",null,null,"1 unit","","EA","Price increase",1091.7279000000001,360270.20700000005]
[null,1028761,null,"rope length 130m",null,null,"1 unit","","EA","Price increase",1129.1580999999999,372622.17299999995]
[null,1028762,null,"rope length 140m",null,null,"1 unit","","EA","Price increase",1155.0420000000001,381163.86000000004]
[null,1028763,null,"rope length 150m",null,null,"1 unit","","EA","Price increase",1180.9259,389705.54699999996]
[null,1028764,null,"rope length 160m",null,null,"1 unit","","EA","Price increase",1206.8201000000001,398250.63300000003]
[null,1028765,null,"rope length 170m",null,null,"1 unit","","EA","Price increase",1232.7142999999999,406795.71899999998]
[null,1028766,null,"rope length 180m",null,null,"1 unit","","EA","Price increase",1258.6085,415340.80499999999]
[null,1028767,null,"rope length 190m",null,null,"1 unit","","EA","Price increase",1284.4820999999999,423879.09299999999]
[null,1028768,null,"rope length 200m",null,null,"1 unit","","EA","Price increase",1310.3763000000001,432424.17900000006]
[null,"SAFESCAPE ELITETM controlled rate rope descender device  with handwheel",null,null,null,null,""]
[null,"Supplied in red rope bag with rescue logo",null,null,null,null,""]
[null,1028769,null,"rope length 20m",null,null,"1 unit","","EA","Price increase",1122.4939999999999,370423.01999999996]
[null,1028770,null,"rope length 30m",null,null,"1 unit","","EA","Price increase",1148.3882000000001,378968.10600000003]
[null,1028771,null,"rope length 40m",null,null,"1 unit","","EA","Price increase",1174.2927,387516.59100000001]
[null,1028772,null,"rope length 50m",null,null,"1 unit","","EA","Price increase",1200.1663000000001,396054.87900000002]
[null,1028773,null,"rope length 60m",null,null,"1 unit","","EA","Price increase",1226.0604999999998,404599.96499999997]
[null,1028774,null,"rope length 70m",null,null,"1 unit","","EA","Price increase",1251.9444000000001,413141.652]
[null,1028775,null,"rope length 80m",null,null,"1 unit","","EA","Price increase",1277.8385999999998,421686.73799999995]
[null,1028776,null,"rope length 90m",null,null,"1 unit","","EA","Price increase",1303.7225000000001,430228.42500000005]
[null,1028777,null,"rope length 100m",null,null,"1 unit","","EA","Price increase",1329.6167,438773.511]
[null,1028778,null,"rope length 110m",null,null,"1 unit","","EA","Price increase",1355.5006000000001,447315.19800000003]
[null,1028779,null,"rope length 120m",null,null,"1 unit","","EA","Price increase",1381.3948,455860.28399999999]
[null,1028780,null,"rope length 130m",null,null,"1 unit","","EA","Price increase",1418.8146999999999,468208.85099999997]
[null,1028781,null,"rope length 140m",null,null,"1 unit","","EA","Price increase",1444.6985999999999,476750.538]
[null,1028782,null,"rope length 150m",null,null,"1 unit","","EA","Price increase",1470.6031,485299.02299999999]
[null,1028783,null,"rope length 160m",null,null,"1 unit","","EA","Price increase",1496.4973,493844.109]
[null,1028784,null,"rope length 170m",null,null,"1 unit","","EA","Price increase",1522.3812,502385.79600000003]
[null,1028785,null,"rope length 180m",null,null,"1 unit","","EA","Price increase",1548.2651000000001,510927.48300000001]
[null,1028786,null,"rope length 190m",null,null,"1 unit",null,"EA","Price increase",1574.1489999999999,519469.17]
[null,1028787,null,"rope length 200m",null,null,"1 unit","","EA","Price increase",1600.0432000000001,528014.25600000005]
[null,"SAFESCAPE ELITETM controlled rate descender device with handwheel and fold-out handle",null,null,null,null,""]
[null,"Supplied in red rope bag with rescue logo",null,null,null,null,""]
[null,1029150,null,"rope length 20m",null,null,"1 unit","","EA","Price increase",1193.1107999999999,393726.56399999995]
[null,1029151,null,"rope length 30m",null,null,"1 unit","","EA","Price increase",1219.0050000000001,402271.65]
[null,1029152,null,"rope length 40m",null,null,"1 unit","","EA","Price increase",1244.8889000000001,410813.33700000006]
[null,1029153,null,"rope length 50m",null,null,"1 unit","","EA","Price increase",1270.7934,419361.82199999999]
[null,1029154,null,"rope length 60m",null,null,"1 unit","","EA","Price increase",1296.6670000000001,427900.11000000004]
[null,1029155,null,"rope length 70m",null,null,"1 unit","","EA","Price increase",1322.5611999999999,436445.19599999994]
[null,1029156,null,"rope length 80m",null,null,"1 unit","","EA","Price increase",1348.4451000000001,444986.88300000003]
[null,1029157,null,"rope length 90m",null,null,"1 unit","","EA","Price increase",1374.3392999999999,453531.96899999998]
[null,1029158,null,"rope length 100m",null,null,"1 unit","","EA","Price increase",1400.2232000000001,462073.65600000002]
[null,1029159,null,"rope length 110m",null,null,"1 unit","","EA","Price increase",1426.1173999999999,470618.74199999997]
[null,1029160,null,"rope length 120m",null,null,"1 unit","","EA","Price increase",1452.0116,479163.82800000004]
[null,1029161,null,"rope length 130m",null,null,"1 unit","","EA","Price increase",1489.4418000000001,491515.79399999999]
[null,1029162,null,"rope length 140m",null,null,"1 unit","","EA","Price increase",1515.3154,500054.08199999999]
[null,1029163,null,"rope length 150m",null,null,"1 unit","","EA","Price increase",1541.2095999999999,508599.16799999995]
[null,1029164,null,"rope length 160m",null,null,"1 unit","","EA","Price increase",1567.0934999999999,517140.85499999998]
[null,1029165,null,"rope length 170m",null,null,"1 unit","","EA","Price increase",1592.9979999999998,525689.34]
[null,1029166,null,"rope length 180m",null,null,"1 unit","","EA","Price increase",1618.8715999999999,534227.62800000003]
[null,1029167,null,"rope length 190m",null,null,"1 unit","","EA","Price increase",1644.7657999999999,542772.71399999992]
[null,1029168,null,"rope length 200m",null,null,"1 unit","","EA","Price increase",1670.6496999999999,551314.40099999995]
[null,"SAFESCAPE ELITETM controlled rate descender device with ladder bracket and handwheel",null,null,null,null,""]
[null,"Supplied in red rope bag with rescue logo",null,null,null,null,""]
[null,1028788,null,"rope length 20m",null,null,"1 unit","","EA","Price increase",1681.1557,554781.38100000005]
[null,1028789,null,"rope length 30m",null,null,"1 unit","","EA","Price increase",1707.3382999999999,563421.63899999997]
[null,1028790,null,"rope length 40m",null,null,"1 unit","","EA","Price increase",1733.7474999999999,572136.67499999993]
[null,1028791,null,"rope length 50m",null,null,"1 unit","","EA","Price increase",1760.1464000000001,580848.31200000003]
[null,1028792,null,"rope length 60m",null,null,"1 unit","","EA","Price increase",1786.5555999999999,589563.348]
[null,1028793,null,"rope length 70m",null,null,"1 unit","","EA","Price increase",1812.9648000000002,598278.38400000008]
[null,1028794,null,"rope length 80m",null,null,"1 unit","","EA","Price increase",1839.3636999999999,606990.02099999995]
[null,1028795,null,"rope length 90m",null,null,"1 unit","","EA","Price increase",1868.5127,616609.19099999999]
[null,1028796,null,"rope length 100m",null,null,"1 unit","","EA","Price increase",1894.9116000000001,625320.8280000001]
[null,1028797,null,"rope length 110m",null,null,"1 unit","","EA","Price increase",1921.3208,634035.86399999994]
[null,1028798,null,"rope length 120m",null,null,"1 unit","","EA","Price increase",1947.73,642750.9]
[null,1028799,null,"rope length 130m",null,null,"1 unit","","EA","Price increase",1974.1289000000002,651462.53700000001]
[null,1028800,null,"rope length 140m",null,null,"1 unit","","EA","Price increase",2062.0909000000001,680489.99700000009]
[null,1028801,null,"rope length 150m",null,null,"1 unit","","EA","Price increase",2088.5001000000002,689205.03300000005]
[null,1028802,null,"rope length 160m",null,null,"1 unit","","EA","Price increase",2114.9092999999998,697920.0689999999]
[null,1028803,null,"rope length 170m",null,null,"1 unit","","EA","Price increase",2141.3081999999999,706631.70600000001]
[null,1028804,null,"rope length 180m",null,null,"1 unit","","EA","Price increase",2167.7174,715346.74199999997]
[null,1028805,null,"rope length 190m",null,null,"1 unit","","EA","Price increase",2194.1369,724065.17700000003]
[null,1028806,null,"rope length 200m",null,null,"1 unit","","EA","Price increase",2220.5358000000001,732776.81400000001]
[null,"Miller Automatic Self Descenders"]
[null,1029169,null,"Miller Safescape ELITE with host and handle and ladder adaptater. 20m rope",null,null,"1 unit","1 unit",null,"Price increase",1635.0735,539574.255]
[null,1029170,null,"SafEscape hoist+handle+adapt 30m rope",null,null,"1 unit","1 unit",null,"Price increase",1659.9685999999999,547789.63799999992]
[null,1029171,null,"SafEscape hoist+handle+adapt 40m rope",null,null,"1 unit","1 unit",null,"Price increase",1684.8534,556001.62199999997]
[null,1029172,null,"SafEscape hoist+handle+adapt 50m rope",null,null,"1 unit","1 unit",null,"Price increase",1709.7485000000001,564217.005]
[null,1029173,null,"SafEscape hoist+handle+adapt 60m rope",null,null,"1 unit","1 unit",null,"Price increase",1734.6333,572428.98899999994]
[null,1029174,null,"SafEscape hoist+handle+adapt 70m rope",null,null,"1 unit","1 unit",null,"Price increase",1759.5387000000001,580647.77100000007]
[null,1029175,null,"SafEscape hoist+handle+adapt 80m rope",null,null,"1 unit","1 unit",null,"Price increase",1784.4235000000001,588859.755]
[null,1029176,null,"SafEscape hoist+handle+adapt 90m rope",null,null,"1 unit","1 unit",null,"Price increase",1811.9039,597928.28700000001]
[null,1029177,null,"SafEscape hoist+handle+adapt 100m rope",null,null,"1 unit","1 unit",null,"Price increase",1836.799,606143.67000000004]
[null,1029178,null,"SafEscape hoist+handle+adapt 110m rope",null,null,"1 unit","1 unit",null,"Price increase",1861.6735000000001,614352.255]
[null,1029179,null,"SafEscape hoist+handle+adapt 120m rope",null,null,"1 unit","1 unit",null,"Price increase",1886.5789000000002,622571.03700000001]
[null,1029180,null,"SafEscape hoist+handle+adapt 130m rope",null,null,"1 unit","1 unit",null,"Price increase",1911.4637,630783.02099999995]
[null,1029181,null,"SafEscape hoist+handle+adapt 140m rope",null,null,"1 unit","1 unit",null,"Price increase",1994.3889999999999,658148.37]
[null,1029182,null,"SafEscape hoist+handle+adapt 150m rope",null,null,"1 unit","1 unit",null,"Price increase",2019.2841000000001,666363.75300000003]
[null,1029183,null,"SafEscape hoist+handle+adapt 160m rope",null,null,"1 unit","1 unit",null,"Price increase",2044.1586,674572.33799999999]
[null,1029184,null,"SafEscape hoist+handle+adapt 170m rope",null,null,"1 unit","1 unit",null,"Price increase",2069.0639999999999,682791.12]
[null,1029185,null,"SafEscape hoist+handle+adapt 180m rope",null,null,"1 unit","1 unit",null,"Price increase",2093.9488000000001,691003.10400000005]
[null,1029186,null,"SafEscape hoist+handle+adapt 190m rope",null,null,"1 unit","1 unit",null,"Price increase",2118.8541999999998,699221.88599999994]
[null,1029187,null,"SafEscape hoist+handle+adapt 200m rope",null,null,"1 unit","1 unit",null,"Price increase",2143.739,707433.87]
[null,1029350,null,"SAFESCAPE KIT 20M",null,null,"1 unit","1 unit",null,"Price increase",1116.0534,368297.62200000003]
[null,1029920,null,"SAFESCAPE KIT 40m",null,null,"1 unit","1 unit",null,"Price increase",1165.3602000000001,384568.86600000004]
[null,"*SafEscape ELITETM is also available with ladder bracket, handwheel and fold-out handle",null,null,null,null,""]
[null,"*Rope lengths up to 400m are available on request",null,null,null,null,""]
[null,"SAFESCAPE ELITETM Rescue Kit",null,null,null,null,""]
[null,"Rescue kit contains a comprehensive selection of accessories to facilitate recovery in many different scenarios"]
[null,1028811,null,"Rescue Kit contains SAFESCAPE ELITETM with ladder bracket and hand wheel, fitted with 80m rope, 2 x 1.2m slings, rescue rope grab, edge protector, T-bar, pulley, 4 x karabiners, rescue rope bag",null,null,"1 unit","","EA","Price increase",2232.6882000000001,736787.10600000003]
[null,"SAFESCAPE ELITETM Evacuation Kit"]
[null,"Complete evacuation kit designed as a solution for wind turbines, cranes and situations where the equipment is stored for"]
[null,"extended periods, the case design permits components to be inspected every 10 years for reduced downtime and lower costs"]
[null,"Safescape kit with rescue red bag stored in the peli case that offers a solution of storing PPE safely without the need of costly inspection up to 10 Years"]
[]
[null,1031770,null,"Safescape case kit 30 m with Evacuation bag",null,null,"1 unit","PELI CASE","EA","Price increase",2556.4566,843630.67799999996]
[null,1031680,null,"Safescape case  kit 40 m with Evacuation bag",null,null,"1 unit","PELI CASE","EA","Price increase",2580.6102000000001,851601.36600000004]
[null,1031681,null,"Safescape case kit 80 m with Evacuation bag",null,null,"1 unit","PELI CASE","EA","Price increase",2683.6710000000003,885611.43]
[null,1031682,null,"Safescape case kit 120 m with Evacuation bag",null,null,"1 unit","PELI CASE","EA","Price increase",2786.7521999999999,919628.22600000002]
[null,1031820,null,"Safescape kit 120 m + case 1600. For evacuation kit with safescape with 120 m rope. composed of a Miller Safescape Elite 120 M without wheel\npacked into the Miller Blue rescue bag 60 L ref 1004444",null,null,"1 unit","PELI CASE","EA","Price increase",1876.6061999999999,619280.04599999997]
[null,1031821,null,"Safescape kit 120 m + case 1610. For rescue kit with safescape with 120 m rope. SafEscape +wheel & 120 m rope (ref 1028760)\nTwistlock Carabiner ref 1018971 : 4 pcs\nSling 1,2 m ref 1002918 : 2 pcs\nSling 0,6 m ref 1002916 : 2 pcs\nWork positioning lanyard ref 1002878\nSingle swivel cheek pulley ref 1007038\nRescue Rope grab ref 1028807",null,null,"1 unit","PELI CASE","EA","Price increase",3063.8249999999998,1011062.2499999999]
[]
[null,1010191,null,"Medium (23cm x 59cm), holds 100m of 11mm rope",null,null,"1 unit","","EA","Price increase",77.703199999999995,25642.055999999997]
[null,1010190,null,"Large (26cm x 69cm), holds 200m of 11mm rope",null,null,"1 unit","","EA","Price increase",80.432699999999997,26542.790999999997]
[null,1029340,null,"XL (48cm x 69cm), holds 400m of 11mm rope",null,null,"1 unit","","EA","Price increase",86.2136,28450.488000000001]
[null,"*Capacity of bag shown is for rope only / reduced rope lengths are accommodated if other equipment is also stored "]
[null,"Rescue Triangle",null,null,null,null,""]
[null,1004876,null,"Fully adjustable rescue triangle - usable for adults and children","EN1498B",null,"1 unit","","EA","Price increase",122.20950000000001,40329.135000000002]
[null,"Aluminium Pulley",null,null,null,null,""]
[null,1007038,null,"Single aluminium pulley suitable for ropes up to 12.7mm diameter, weight 0.12kg, used to alter the line of the rope away from the anchor point",null,null,"1 unit","","EA","Price increase",44.547499999999999,14700.674999999999]
[null,"Rescue Rope Grab",null,null,null,null,""]
[null,1028807,null,"Rescue rope grab attaches to the live rope coming from the SafEscape Elite and connects inverted to a suspended casualty's rope or lanyard to lift the casualty",null,null,"1 unit","","EA","Price increase",75.816000000000003,25019.280000000002]
[null,"Edge protector ",null,null,null,null,""]
[null,1028808,null,"Stainless steel edge protector guides the rope over an edge to prevent abrasion or cut when lifting or lowering a person",null,null,"1 unit","","EA","Price increase",109.7568,36219.743999999999]
[null,"T-bar",null,null,null,null,""]
[null,1028809,null,"T-bar levers a rope away from an edge and into the Edge protector device",null,null,"1 unit","","EA","Price increase",112.7026,37191.858]
[null,"Telescopic reach pole",null,null,null,null,""]
[null,1017824,null,"4 metre telescopic reach pole is used to connect the live rope coming from the SafEscape Elite to the D-ring on a suspended casualty's harness to facilitate recovery",null,null,"1 unit","","EA","Price increase",103.8549,34272.116999999998]
[null,"EVAC BODY SPLINT",null,null,null,null,""]
[null,1007046,null,"EVAC Body Splint",null,null,"1 unit","","EA","Price increase",419.50870000000003,138437.87100000001]
[null,1031786,null,"KIT EVAC BODY STRETCHER. The Evac Body Splint and every lifting straps of the stretcher can support a 300kg static load.Although the Evac Body Splint and the Spider Stretcher are not made to support falls, both together connected loaded with a 140 kg dummy can support dynamically a fall of 0,50m",null,null,null,"BAG ","EA","Price increase",656.78819999999996,216740.106]
[null,1030285,null,"SPIDER lanyard for STRETCHER",null,null,null,"BAG ","EA","Price increase",243.48169999999999,80348.960999999996]
[null,1032320,null,"BAG FOR KIT EVAC BODY",null,null,null,"BAG ","EA","Price increase",56.5779,18670.706999999999]
[null,"Fall Protection |  CONFINED SPACE ACCESS",null,null,null,null,""]
[null,"CONFINED SPACES EQUIPMENT",null,null,null,null,""]
[null,1034430,null,"Miller DuraHoist 3Pod","EN795 B",null,"1 unit",null,"EA","Price increase",1010,333300]
[null,1034511,null,"Miller DuraHoist 3Pod bag",null,null,"1 unit",null,"EA","Price increase",149.1669,49225.076999999997]
[null,1034431,null,"MightEvac Bracket 15m",null,null,"1 unit",null,"EA","Price increase",217.53379999999999,71786.153999999995]
[null,1034750,null,"MightEvac Bracket 30m",null,null,"1 unit",null,"EA","Price increase",217.53379999999999,71786.153999999995]
[null,1034611,null,"DuraHoist Winch 15m stainless steel",null,null,"1 unit",null,"EA","Price increase",1051.9554000000001,347145.28200000001]
[null,1034612,null,"DuraHoist Winch 30m stainless steel",null,null,"1 unit",null,"EA","Price increase",1704.5669,562507.07700000005]
[null,1034613,null,"DuraHoist Winch Bracket for 15 & 30m",null,null,"1 unit",null,"EA","Price increase",217.53379999999999,71786.153999999995]
[null,"DuraHoist 3Pod & Accessories Kits"]
[null,1034910,null,"DuraHoist 3Pod + MightEvac galva 15m + Bracket",null,null,"1 unit",null,"EA","Price increase",2206.4661999999998,728133.8459999999]
[null,1034911,null,"DuraHoist 3Pod + MightEvac galva 15m + Winch 15m + 2 Brackets",null,null,"1 unit",null,"EA","Price increase",3480.6115,1148601.7949999999]
[null,1034912,null,"DuraHoist 3Pod + MightEvac SS 15m + Bracket",null,null,"1 unit",null,"EA","Price increase",2548.3107999999997,840942.5639999999]
[null,1034913,null,"DuraHoist 3Pod + MightEvac SS 15m + Winch 15m + 2 Brackets",null,null,"1 unit",null,"EA","Price increase",3806.9223000000002,1256284.3590000002]
[null,1034914,null,"DuraHoist 3Pod + MightEvac galva 30m + Bracket",null,null,"1 unit",null,"EA","Price increase",2796.9223000000002,922984.35900000005]
[null,1034915,null,"DuraHoist 3Pod + MightEvac galva 30m + Winch 30m + 2 Brackets",null,null,"1 unit",null,"EA","Price increase",4723.6891999999998,1558817.436]
[null,"PIVOTING DAVIT SYSTEM",null,null,null,null,""]
[null,1002920,null,"MN50 Pivoting davit system c/w winch and H-base","EN795b",null,"1 unit","","EA","Price increase",2230.4567999999999,736050.74399999995]
[null,1004232,null,"MN51 Davit arm c/w winch (arm only - no base included)",null,null,"1 unit","","EA","Price increase",1255.5919999999999,414345.36]
[null,1004233,null,"MN61 Wall mount base for davit arm",null,null,"1 unit","","EA","Price increase",529.81759999999997,174839.80799999999]
[null,1004234,null,"MN62 Floor mount base for davit arm",null,null,"1 unit","","EA","Price increase",709.42560000000003,234110.448]
[null,1004236,null,"MN64 Truck attachment base for davit arm",null,null,"1 unit","","EA","Price increase",1469.2229,484843.55699999997]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  ACCESSORIES",null,null,null,null,""]
[null,"BANDIT TOOL LANYARDS"]
[null,"When performing jobs at height, workers can sometimes lose their grip. Tools are often dropped, reducing on-the-job "]
[null,"efficiencies and potentially causing serious injury to workers below.  With Bandit tool lanyards this doesn’t have to be "]
[null,"the case. In accordance with the Work at Height Regulations 2005, every employer should take suitable and sufficient "]
[null,"steps to prevent the fall of any material or object."]
[null,1012490,null,"BANDIT Tool Lanyard, bulk pack",null,null,"36 units","BOX","BOX","Price increase",471.96290000000005,155747.75700000001]
[null,1100210,null,"BANDIT Tool Lanyard, standard pack",null,null,"12 units","BOX","BOX","Price increase",170.3466,56214.377999999997]
[null,1012491,null,"BANDIT Wrist Lanyard, standard pack",null,null,"36 units","BOX","BOX","Price increase",317.72579999999999,104849.514]
[null,"PROTECTIVE SHOULDER PAD",null,null,null,null,""]
[null,"RELIEF STEP",null,null,null,null,""]
[null,1100211,null,"RELIEF-STEP safety device alleviates the effects of suspension trauma. If a fall occurs, a person becomes suspended in a harness and remains both vertical and sedentary for a period of time, causing blood to ‘pool’ in the veins of the legs. The Relief-Step is designed to provide a short-term solution in preventing suspension trauma.",null,null,"1 unit","","EA","Price increase",299.55589999999995,98853.446999999986]
[null,"CARRY CASES AND BAGS",null,null,null,null,""]
[null,1002864,null,"MM00 Plastic storage box, 500 x 300 x 200mm, 1,7 kg  (PVC)",null,null,"1 unit","","EA","Price increase",40.652500000000003,13415.325000000001]
[null,1002865,null,"MM01 Holdall, 590 x 270 x 270mm",null,null,"1 unit","","EA","Price increase",43.945099999999996,14501.882999999998]
[null,1004602,null,"MM02 Small plastic carry case (example kits 6,7,8)",null,null,"1 unit","","EA","Price increase",22.0382,7272.6059999999998]
[null,1002866,null,"MR00 Tools bag, for use with Miller waistbelts",null,null,"1 unit","","EA","Price increase",79.396100000000004,26200.713]
[null,1007067,null,"Backpack (as supplied with kits)",null,null,"1 unit","","EA","Price increase",21.967500000000001,7249.2750000000005]
[null,1004443,null,"Miller back pack 30L (PVC)",null,null,"1 unit","1 unit","EA","Price increase",51.722099999999998,17068.292999999998]
[null,1004444,null,"Miller back pack 60L (PVC)",null,null,"1 unit","1 unit","EA","Price increase",78.386099999999999,25867.413]
[null,null,null,null,null,null,""]
[null,"Fall Protection |  TREE PRUNING",null,null,null,null,""]
[null,"THROWING BAGS AND LINES",null,null,null,null,""]
[null,1030991,null,"Throwing bag 250g\n(replaces 1011721)",null,null,"1 unit",null,"EA","Price increase",20.614100000000001,6802.6530000000002]
[null,1030992,null,"Throwing bag 350g\n(replaces 1011722)",null,null,"1 unit",null,"EA","Price increase",22.290700000000001,7355.9310000000005]
[null,1003182,null,"Throwing line 50m x Ø2mm used with throwing bag",null,null,"1 unit",null,"EA","Price increase",7.8383000000000003,2586.6390000000001]
[null,1031013,null,"Dyneema throwing line 50m ",null,null,"1 unit",null,"EA","Price increase",39.788900000000005,13130.337000000001]
[null,1031011,null,"Bag for throwing accessories (bag only)",null,null,"1 unit",null,"EA","Price increase",34.552100000000003,11402.193000000001]
[null,1031012,null,"Kit : Throwing line Dyneema + Throwing bag + Bag",null,null,"1 unit",null,"EA","Price increase",71.756999999999991,23679.809999999998]
[null,"AMAZONE CLIMBING LINES",null,null,null,null,""]
[null,"12mm nylon rope climbing line with two stitched splices, no ‘flabbing effect’ - the rope is particularly adapted for use with"]
[null,"Prussik knot method and manual ascenders, easily inserted through the Cambium Saver rings"]
[null,1011726,null,"AMAZONE climbing line 2 stitched splices 25m","EN1891",null,"1 unit",null,"EA","Price increase",150.84350000000001,49778.355000000003]
[null,1011723,null,"AMAZONE climbing line 2 stitched splices 35m","EN1891",null,"1 unit",null,"EA","Price increase",211.81950000000001,69900.434999999998]
[null,1011724,null,"AMAZONE climbing line 2 stitched splices 45m","EN1891",null,"1 unit",null,"EA","Price increase",266.12110000000001,87819.963000000003]
[null,"SPLIT TAILS",null,null,null,null,""]
[null,1003428,null,"SPLIT TAIL 1.10m - 12mm polyester rope with two stitched splices, length 1.1m, weight 0.155kg, breaking strength 28kN, suitable for Prussik, Swabish and Blake knots",null,null,"1 unit",null,"EA","Price increase",33.659999999999997,11107.8]
[null,1003429,null,"SPLIT TAIL 1m - 10mm polyester rope with two stitched splices, length 1m, weight 0.115kg, breaking strength: 15kN, suitable for Prussik, Swabish and Valdotain knots",null,null,"1 unit",null,"EA","Price increase",30.304200000000002,10000.386]
[null,"ARBORIST ASCENDER / DESCENDER DEVICES",null,null,null,null,""]
[null,1003045,null,"DOUBLE JUMAR manual ascender attaches to either side of the climbing line, anodised light alloyed aluminium, 0.4kg","EN567",null,"1 unit",null,"EA","Price increase",134.2088,44288.904000000002]
[null,1018870,null,"DOUBLE CROCHE used for climbing and descent, anodised aluminium, 0.42 kg","EN567/EN795b",null,"1 unit",null,"EA","Price increase",167.20080000000002,55176.264000000003]
[null,1028691,null,"KIT DOUBLE CROCHE includes 1 double croche device, 1 pulley and  2  triple action karabiners",null,null,"1 unit",null,"EA","Price increase",208.9984,68969.471999999994]
[null,"NEW MILLER HANDZUP WORK POSITIONING LANYARDS ",null,null,null,null,""]
[null,null,null,"HandZup with wire rope, Cigale steel triple lock karabiner and Elix3 aluminium triple lock swivel karabiner"]
[null,1032105,null,"● Length 5m","EN358",null,"1 unit","","EA","Price increase",207.12120000000002,68349.995999999999]
[null,null,null,"\nHandZup with wire rope, 2 x Cigale steel triple lock karabiners"]
[null,1032106,null,"● Length 3m","EN358",null,"1 unit","","EA","Price increase",186.405,61513.65]
[null,1032107,null,"● Length 4m","EN358",null,"1 unit","","EA","Price increase",196.36019999999999,64798.865999999995]
[null,1032108,null,"● Length 5m","EN358",null,"1 unit","","EA","Price increase",206.29499999999999,68077.349999999991]
[null,null,null,"\nHandZup with Cigale steel triple lock karabiner and Elix3 aluminium triple lock swivel karabiner"]
[null,1032110,null,"● Length 4m","EN358",null,"1 unit","","EA","Price increase",129.24420000000001,42650.586000000003]
[null,1032111,null,"● Length 5m","EN358",null,"1 unit","","EA","Price increase",132.5694,43747.902000000002]
[null,1032115,null,"● Length 20m","EN358",null,"1 unit","","EA","Price increase",202.14360000000002,66707.388000000006]
[null,1032116,null,"● Length 30m","EN358",null,"1 unit","","EA","Price increase",235.2834,77643.521999999997]
[null,1032117,null,"● Length 40m","EN358",null,"1 unit","","EA","Price increase",268.43340000000001,88583.021999999997]
[null,null,null,"\nHandZup with Cigale steel triple lock karabiner, Elix3 aluminium triple lock swivel karabiner and protective sleeve"]
[null,1032112,null,"● Length 3m","EN358",null,"1 unit","","EA","Price increase",130.9068,43199.243999999999]
[null,1032113,null,"● Length 4m","EN358",null,"1 unit","","EA","Price increase",134.2116,44289.828000000001]
[null,1032114,null,"● Length 5m","EN358",null,"1 unit","","EA","Price increase",137.5266,45383.777999999998]
[null,"REPLACEMENT ROPE"]
[null,null,null,"HandZup wire rope with Elix3 aluminium triple lock swivel karabiner"]
[null,1032132,null,"● Length 4m",null,null,"1 unit","","EA","Price increase",137.5266,45383.777999999998]
[null,1032133,null,"● Length 5m",null,null,"1 unit","","EA","Price increase",147.4614,48662.262000000002]
[null,null,null,"\nHandZup wire rope with no connectors"]
[null,1032134,null,"● Length 3m",null,null,"1 unit","","EA","Price increase",114.3216,37726.128000000004]
[null,1032135,null,"● Length 4m",null,null,"1 unit","","EA","Price increase",124.2666,41007.977999999996]
[null,1032136,null,"● Length 5m",null,null,"1 unit","","EA","Price increase",134.2116,44289.828000000001]
[null,null,null,"\nHandZup rope with Elix3 aluminium triple lock swivel karabiner"]
[null,1032137,null,"● Length 3m",null,null,"1 unit","","EA","Price increase",66.279600000000002,21872.268]
[null,1032139,null,"● Length 5m",null,null,"1 unit","","EA","Price increase",72.8994,24056.802]
[null,1032141,null,"● Length 30m",null,null,"1 unit","","EA","Price increase",177.29640000000001,58507.812000000005]
[null,1032142,null,"● Length 40m",null,null,"1 unit","","EA","Price increase",210.42600000000002,69440.58]
[]
[null,"Fall Protection |  TECHNICAL ACCESS AND RESCUE",null,null,null,null,""]
[null,"TECHNICAL HARNESSES",null,null,null,null,""]
[null,"IBEXX",null,null,null,null,""]
[null,"4-point harness designed for specialists working hands-free at heights or in rescue. This full-body harness offers "]
[null,"excellent suspension comfort with upgraded backpad and leg pads, black polyester webbing, green stitching."]
[null,null,null,"IBEX2 Full Body Harness with two front webbing attachment points (ventral and sternal), one rear D-ring and side D-rings","EN361\nEN358\nEN813 "]
[null,1007021,null,"● Size M / L",null,null,"1 unit",null,"EA","Price increase",300.99690000000004,99328.977000000014]
[null,null,null,"IBX2R Full Body Harness with two front webbing attachment points (ventral and sternal), one rear D-ring, side D-rings and racking system","EN361\nEN358\nEN813 "]
[null,1007386,null,"● Size S",null,null,"1 unit",null,"EA","Price increase",303.91920000000005,100293.33600000001]
[null,1007022,null,"● Size M / L",null,null,"1 unit",null,"EA","Price increase",303.91920000000005,100293.33600000001]
[null,1007387,null,"● Size XL",null,null,"1 unit",null,"EA","Price increase",303.91920000000005,100293.33600000001]
[null,null,null,"RAM Sit Harness; Sit harness for the industrial access and rescue technician with padded waist and leg straps","EN813"]
[null,1010251,null,"● Black webbing - Size S",null,null,"1 unit",null,"EA","Price increase",117.9568,38925.743999999999]
[null,1010252,null,"● Black webbing - Size M / L",null,null,"1 unit",null,"EA","Price increase",117.9568,38925.743999999999]
[null,1010253,null,"● Black webbing - Size XL",null,null,"1 unit",null,"EA","Price increase",117.9568,38925.743999999999]
[null,"COMBI SLING (1007030) and karabiner (1002833) to attach to ITC"]
[null,1007030,null,"COMBI SLING - 21cm","EN354",null,"1 unit",null,"EA","Price increase",17.940000000000001,5920.2000000000007]
[null,1002833,null,"ML01 Anodised alloy screwgate karabiner, length 110mm, width 62.5mm, diameter 11mm, weight 0.065mm, breaking strength: >28kN, opening 18mm","EN362",null,"1 unit",null,"EA","Price increase",14.090399999999999,4649.8319999999994]
[null,"TECHNICAL HARNESSES",null,null,null,null,""]
[null,null,null,"HYRAX Full Body Harness with ABS shoulder adjustment and single back dorsal connection point and front webbing loops (now supplied in black webbing with green stitching)","EN361\nEN358",null,""]
[null,1007023,null,"● Size M / L",null,null,"1 unit","","EA","Price increase",146.4528,48329.423999999999]
[null,1007388,null,"● Size XL",null,null,"1 unit","","EA","Price increase",146.4528,48329.423999999999]
[null,1007024,null,"LYNXX Full Body Harness with ABS shoulder adjustment and front and back attachment points for fall arrest","EN361 ",null,"1 unit","","EA","Price increase",126.86959999999999,41866.967999999993]
[null,1003438,null,"RM Harness with elasticated webbing on the shoulder straps and padded belt and leg loops","EN361\nEN358","S/M","1 unit",null,"EA",null,245.12639999999999,80891.712]
[null,1003439,null,"RM Harness with elasticated webbing on the shoulder straps and padded belt and leg loops","EN361\nEN358","L/XL","1 unit","","EA","Price increase",245.12639999999999,80891.712]
[null,1002924,null,"SEWERAGE Harness with 2 chest D Rings, one back D ring with webbing extension, comfort back pad and pocket for portable gas detector","EN361\nEN358",null,"1 unit","","EA","Price increase",307.4864,101470.512]
[null,null,null,"AGU 300 Harness with back and front fall arrest and one front D ring for guided type fall arrester use and comfort positioning belt (now supplied in green webbing with blue leg loops)","EN361\nEN358",null,""]
[null,1006977,null,"● Size S",null,null,"1 unit","","EA","Price increase",307.52999999999997,101484.9]
[null,1006949,null,"● Size M",null,null,"1 unit","","EA","Price increase",307.52999999999997,101484.9]
[null,1006975,null,"● Size L",null,null,"1 unit","","EA","Price increase",307.52999999999997,101484.9]
[null,1006255,null,"486/523 TOWER Harness with one back D ring, central front karabiner as anchorage point, one front suspension and access D ring, wide comfort belt and leg and shoulder pads","EN361\nEN358\nEN813",null,"1 unit","","EA","Price increase",253.292,83586.36]
[null,null,null,null,null,null,""]
[null,1007064,null,"MAGMA Fireman Harness; Specialist sit harness with tailored leg loops, stitched accessory loops, reflective high-vis strip, small pouch for equipment and front attachment loop for waist belt","EN813",null,"1 unit","","EA","Price increase",135.80549999999999,44815.814999999995]
[null,"ENERGY ABSORBING LANYARDS",null,null,null,null,""]
[null,null,null,"AMORSTOP Forked Lanyard; Webbing energy absorbing lanyard equipped with 2 GO60 lightweight hooks and 1 karabiner",null,null,""]
[null,1003232,null,"● Length 1m","EN355",null,"1 unit","","EA","Price increase",161.66799999999998,53350.439999999995]
[null,1003235,null,"● Length 2m","EN355",null,"1 unit","","EA","Price increase",172.15119999999999,56809.895999999993]
[null,"ENERGY ABSORBING LANYARDS WITH TIE-BACK LOOPS",null,null,null,null,""]
[null,"Upgraded lanyard design in polyester webbing",null,null,null,null,""]
[null,1007014,null,"Energy-absorbing webbing lanyard, length 1.2m, with 1 tie-back loop - no connectors","EN355",null,"1 unit","","EA","Price increase",74.869599999999991,24706.967999999997]
[null,1007011,null,"Energy-absorbing webbing lanyard, length 2m, with 2 tie-back loops and 2 x BA01 karabiners","EN355",null,"1 unit","","EA","Price increase",139.23519999999999,45947.615999999995]
[null,1007015,null,"Energy-absorbing twin webbing lanyard, length 1.5m, with 4 tie back loops - no connectors","EN355",null,"1 unit","","EA","Price increase",96.552199999999999,31862.225999999999]
[null,1007013,null,"Energy-absorbing twin webbing lanyard, length 1.5m, with 4 tie-back loops and 3 x BA01 karabiners","EN355",null,"1 unit","","EA","Price increase",202.84819999999999,66939.906000000003]
[null,1017847,null,"Energy-absorbing twin webbing lanyard, length 1.5m, with 4 tie-back loops, 2 scaffold hooks and no connector fitted to absorber end","EN355",null,"1 unit",null,"EA","Price increase",126.9944,41908.152000000002]
[null,1010206,null,"Energy-absorbing twin webbing lanyard, length 1.5m, with 4 tie-back loops, 1 x BA01 karabiner and 2 scaffold hooks","EN355",null,"1 unit","","EA","Price increase",100.6516,33215.027999999998]
[null,"ROPE ASCENDERS",null,null,null,null,""]
[null,1004254,null,"Cam-Clean ascender; Rope clamp for ascending fixed rope or as an anti-return system.","EN567",null,"1 unit","","EA","Price increase",49.0486,16186.038]
[null,1007041,null,"Alloy heavy duty handled rope ascender for ascending on 10mm to 13mm rope, right hand","EN567",null,"1 unit","","EA","Price increase",71.389300000000006,23558.469000000001]
[null,1007393,null,"Alloy heavy duty handled rope ascender for ascending on 10mm to 13mm rope, left hand","EN567",null,"1 unit","","EA","Price increase",71.389300000000006,23558.469000000001]
[null,null,null,null,null,null,""]
[null,"ROPE DESCENDERS",null,null,null,null,""]
[null,"ROPE GRABS",null,null,null,null,""]
[null,"ALTOCHUT AUTOMATIC LOCKING ROPE GRAB",null,null,null,null,""]
[null,1002933,null,"● for 10.5mm braided rope and 12mm twisted rope","EN353-2",null,"1 unit","","EA","Price increase",75.816000000000003,25019.280000000002]
[null,1003064,null,"● for 10.5mm braided rope and 12mm twisted rope, complete with 0.3m connection lanyard and screw gate karabiner","EN353-2",null,"1 unit","","EA","Price increase",104.72800000000001,34560.240000000005]
[null,1002937,null,"● for 14mm twisted rope","EN353-2",null,"1 unit","","EA","Price increase",76.897599999999997,25376.207999999999]
[null,1003071,null,"● for 14mm twisted rope, complete with 0.3m connection lanyard and screw gate karabiner","EN353-2",null,"1 unit","","EA","Price increase",105.5808,34841.663999999997]
[null,"ROCKER ROPE LOCK",null,null,null,null,""]
[null,1007031,null,"ROCKER rope grab (EN353-2)\nLength adjuster for positioning lanyard (EN358)\nTensioning device for horizontal lifeline (EN795)\nSuitable for 10mm / 12mm rope","EN353-2",null,"1 unit","","EA","Price increase",115.9059,38248.947]
[null,1010167,null,"ROCKER sling assembly","EN353-2",null,"1 unit","","EA","Price increase",30.796999999999997,10163.009999999998]
[null,"Fall Protection |  TECHNICAL ACCESS AND RESCUE",null,null,null,null,""]
[]
[null,"RESCUE KITS",null,null,null,null,""]
[null,1006026,null,"INDY rescue kit; ready to use self rescue kit including an Indy descender, 20 m rope, anchorage sling and storage bag, suitable to hold one person only",null,null,"1 unit","","EA","Price increase",251.59810000000002,83027.373000000007]
[null,1007042,null,"Casualty Pulley System; Light weight pulley system allowing clipping of the casualty to the rescuer's line",null,null,"1 unit","","EA","Price increase",268.41800000000001,88577.94]
[null,"PULLEYS AND ROLLERS",null,null,null,null,""]
[null,1007043,null,"Edge Roller; 50mm wide roller, each alloy roller rides on stainless steel shaft and brass bearings, can be used in pairs to position a self retracting lifeline over an edge",null,null,"1 unit","","EA","Price increase",137.2784,45301.872000000003]
[null,"LADDER SYSTEMS",null,null,null,null,""]
[null,1002997,null,"KITBLOC; Rope positioning system for ladder including two rope locking devices and 8m braided rope",null,null,"1 unit","","EA","Price increase",190.16890000000001,62755.737000000001]
[null,null,null,null,null,null,""]
[null,"JIRAF TELESCOPIC POLE",null,null,null,null,""]
[null,1006629,null,"JIRAF telescopic stick 5 elements fibre-glass telescopic stick with universal adapter, length 6.5m",null,null,"1 unit","","EA","Price increase",337.61269999999996,111412.19099999999]
[null,1002979,null,"JIRAF telescopic stick 5 elements fibre-glass telescopic stick with universal adapter, length 9.4m",null,null,"1 unit","","EA","Price increase",567.93169999999998,187417.46099999998]
[null,1003345,null,"JIRAF adapter; JIRAF direction adapter compatible with a universal adapter",null,null,"1 unit","","EA","Price increase",117.36200000000001,38729.460000000006]
[null,1002977,null,"JIRAF anchorage sling; Steel wire sling for JIRAF telescopic stick","EN795",null,"1 unit","","EA","Price increase",192.4555,63510.315000000002]
[null,1002981,null,"JIRAF GO100 hook; Light alloy connector (100mm) with self locking gate and rope latch for JIRAF telescopic stick compatible with universal adapter","EN795",null,"1 unit","","EA","Price increase",156.3177,51584.841]
[null,"BEAM GLIDE",null,null,null,null,""]
[null,1007066,null,"Beam Glide;  I Beam anchor device fully adjustable for beam widths up to 290mm","EN795",null,"1 unit","","EA","Price increase",337.55160000000001,111392.02800000001]
[null,"ROPES",null,null,null,null,""]
[null,null,null,"Low-stretch rope; 11mm rope with 16 cores for high strength: and a 32-braid sheath for smooth handling","EN1891",null,""]
[null,1010185,null,"● Length 50m ",null,null,"1 unit","","EA","Price increase",130.52000000000001,43071.600000000006]
[null,1010182,null,"● Length 200m",null,null,"1 unit","","EA","Price increase",521.47680000000003,172087.34400000001]
[null,1004512,null,"10.5mm braided polyamide static rope                                                             ● Length 200m","EN1891",null,"1 unit","","EA","Price increase",417.01920000000001,137616.33600000001]
[null,1010214,null,"Rope Protector; Black PVC reinforced nylon rope protector.",null,null,"1 unit","","EA","Price increase",13.482699999999999,4449.2910000000002]
[null,"CLIMBERS SEAT & CLIMBERS HELMETS",null,null,null,null,""]
[null,1007048,null,"Lightweight polypropylene climbing helmet, red, weight 410g, adjusts to fit 53cm - 61cm, supplied with an elastic attachment point for frontal lamp","EN397",null,"1 unit","","EA","Price increase",86.536800000000014,28557.144000000004]
[null,1030940,null,"Short-peak white HDPE safety helmet with 4-point nylon web suspension, forehead comfort band, 4 point chin strap anchorage, 3-level height adjustment and 30mm accessory slots fit accessories.including visors and earmuffs","EN397",null,"1 unit","","EA","Price increase",39.985900000000001,13195.347]
[null,"EQUIPMENT BAGS",null,null,null,null,""]
[null,1003041,null,"Leather tool bag, double pocket with hard pads to allow easy access.(27x25x16cm)",null,null,"1 unit","","EA","Price increase",101.1919,33393.327000000005]
[null,1010211,null,"Equipment bag with top lifting loop and shoulder carrying straps made from black PVC coated nylon, 30 litre",null,null,"1 unit","","EA","Price increase",57.3401,18922.233]
[]
[null,1002896,null,"MJ50 – Alloy connector (weight 1,274kg, opening 150mm)",null,null,"1 unit","1 unit",null,"Price increase",126.9166,41882.478000000003]
[null,1002927,null,"Tree Pruning standard harness - 2 point full body harness with positioning belt and seat strap, EN 358 & EN 361",null,null,"1 unit","1 unit",null,"Price increase",228.38819999999998,75368.106]
[null,1002928,null,"Evolution Belt - Belt with sternal anchorage D-rings for climbing line & side D-rings for positioning lanyard with rigid seat strap, EN 358",null,null,"1 unit","1 unit",null,"Price increase",261.10239999999999,86163.792000000001]
[null,1002965,null,"MOUSQUETON TRONCONNEUSE",null,null,"1 unit","1 unit",null,"Price increase",24.287399999999998,8014.8419999999996]
[null,1002986,null,"1 Spike Gaff (set of two)",null,null,"1 unit","1 unit",null,"Price increase",215.30169999999998,71049.560999999987]
[null,1003016,null,"Green Belt - Belt with sternal anchorage D-rings for climbing line & side D-rings for positioning lanyard-with rigid seat strap & removable shoulder straps, EN 358",null,null,"1 unit","1 unit",null,"Price increase",273.30899999999997,90191.969999999987]
[null,1003046,null,"Cambium saver-used with a climbing line-EN795 1.10m",null,null,"1 unit","1 unit",null,"Price increase",45.884300000000003,15141.819000000001]
[null,1003059,null,"Web fall arrester block AVIABLOC 1,5m with energy absorber equipped with 2 screw karabiners",null,null,"1 unit","1 unit",null,"Price increase",105.62649999999999,34856.744999999995]
[null,1003099,null,"REGLEX machoire 3m x 14mm rope with steel core with a RAPIDEX 2000 stainless steel jaw type length adjuster-EN358",null,null,"1 unit","1 unit",null,"Price increase",152.898,50456.34]
[null,1003100,null,"REGLEX machoire 4m x 14mm rope with steel core with a RAPIDEX 2000 stainless steel jaw type length adjuster-EN358",null,null,"1 unit","1 unit",null,"Price increase",158.71199999999999,52374.96]
[null,1003101,null,"REGLEX machoire 5m x 14mm rope with steel core with a RAPIDEX 2000 stainless steel jaw type length adjuster-EN358",null,null,"1 unit","1 unit",null,"Price increase",161.70060000000001,53361.198000000004]
[null,1003174,null,"support d'assurage ",null,null,"1 unit","1 unit",null,"Price increase",71.312799999999996,23533.223999999998]
[null,1003216,null,"Rope shock-absorbing lanyard complete AMORSTOP 1,5m with 2 screw karabiners",null,null,"1 unit","1 unit",null,"Price increase",58.562400000000004,19325.592000000001]
[null,1003220,null,"Rope shock-absorbing lanyard complete AMORSTOP 1,3m without connector",null,null,"1 unit","1 unit",null,"Price increase",47.039199999999994,15522.935999999998]
[null,1003233,null," Forked lanyard 1M + 2 Super Rapidex",null,null,"1 unit","1 unit",null,"Price increase",147.22239999999999,48583.392]
[null,1003260,null,"2 Spikes Gaff (set of two)",null,null,"1 pair","1 unit",null,"Price increase",221.31120000000001,73032.696000000011]
[null,1003278,null,"Complete box 20m",null,null,"1 unit","1 unit",null,"Price increase",800.50880000000006,264167.90400000004]
[null,1003279,null,"Complete box 30m",null,null,"1 unit","1 unit",null,"Price increase",833.65359999999998,275105.68799999997]
[null,1003314,null,"MOUSQUETON SPECIAL CEINTURE VERTE",null,null,"1 unit","1 unit",null,"Price increase",47.998000000000005,15839.340000000002]
[null,1003440,null,"TS HARNESS - Work and rescue full body harness with elasticated shoulder straps, front anchorage loops and back D ring and padded leg straps. Size M/L",null,null,"1 unit","1 unit",null,"Price increase",91.228799999999993,30105.503999999997]
[null,1004210,null,"ABS Lock - Rope automatic clam/descender to secure worker during climbing",null,null,"1 unit","1 unit",null,"Price increase",50.758400000000002,16750.272000000001]
[null,1004216,null,"Rope protector 0.70M (can be dismantled)",null,null,"1 unit","1 unit",null,"Price increase",13.7088,4523.9040000000005]
[null,1004245,null,"Harness Top 3",null,null,"1 unit","1 unit",null,"Price increase",65.718600000000009,21687.138000000003]
[null,1004348,null,"Ultra light helmet, white",null,null,"1 unit","1 unit",null,"Price increase",121.81610000000001,40199.313000000002]
[null,1004454,null,"SAC GRAND FORMAT",null,null,"1 unit","1 unit",null,"Price increase",63.0745,20814.584999999999]
[null,1004471,null,"Big Equipment case(Black)",null,null,"1 unit","1 unit",null,"Price increase",51.297899999999998,16928.307000000001]
[null,1004611,null,"CASQUE ECRIN NOUVELLE GENERATION ROUGE",null,null,"1 unit","1 unit",null,"Price increase",81.183799999999991,26790.653999999999]
[null,1006319,null,"520 - Support belt with 100mm wide backpad with quick adjustment buckle. Size M",null,null,"1 unit","1 unit",null,"Price increase",87.577200000000005,28900.476000000002]
[null,1006320,null,"520 - Support belt with 100mm wide backpad with quick adjustment buckle. Size L",null,null,"1 unit","1 unit",null,"Price increase",87.577200000000005,28900.476000000002]
[null,1006321,null,"522 - Support belt with 200mm wide comfort backpad with quick adjustment buckle. Size M",null,null,"1 unit","1 unit",null,"Price increase",92.238600000000005,30438.738000000001]
[null,1006322,null,"522 - Support belt with 200mm wide comfort backpad with quick adjustment buckle. Size L",null,null,"1 unit","1 unit",null,"Price increase",92.238600000000005,30438.738000000001]
[null,1007025,null,"RAM Sit haness - Sit harness, fitted with the ITC harness and combi sling (Size STD)",null,null,"1 unit","1 unit",null,"Price increase",109.56399999999999,36156.119999999995]
[null,1007040,null,"Twin alloy pulleys - Troll double swivel cheek pulley with oil-lite bearing and dual attachment",null,null,"1 unit","1 unit",null,"Price increase",79.67049999999999,26291.264999999996]
[null,1007056,null,"Industrial climbers seat - Working-at-height seat. Made from marine ply and covered with closed cell foam and abrasion resistant PVC coated nylon. Must only be used in conjunction with an appropriate safety harness.",null,null,"1 unit","1 unit",null,"Price increase",161.52459999999999,53303.117999999995]
[null,1007057,null,"Pro ALLP Tech - Screw and auto-lock, controlled-rate rope descender for use with kernmantel 10,5mm to 12,7mm rope purple",null,null,"1 unit","1 unit",null,"Price increase",254.90439999999998,84118.45199999999]
[null,1007058,null,"Cowstail slings 60cm with flat sling eyes at each end",null,null,"1 unit","1 unit",null,"Price increase",18.292800000000003,6036.6240000000007]
[null,1007059,null,"Cowstail slings 30cm with flat sling eyes at each end",null,null,"1 unit","1 unit",null,"Price increase",13.0604,4309.9319999999998]
[null,1007063,null,"Emergency rescue sling - Emergency rescue Sling",null,null,"1 unit","1 unit",null,"Price increase",238.08449999999999,78567.884999999995]
[null,1008362,null,"Anchorage Sling 20mm x 1m",null,null,"1 unit","1 unit",null,"Price increase",6.2919999999999998,2076.36]
[null,1009248,null,"KARABINER GIROUETTE OPENING 22MM",null,null,"1 unit","1 unit",null,"Price increase",32.864000000000004,10845.12]
[null,1009249,null,"Karabiner open.55mm Steel",null,null,"1 unit","1 unit",null,"Price increase",19.971700000000002,6590.661000000001]
[null,1009258,null,"Karabiner open.85mm Steel",null,null,"1 unit","1 unit",null,"Price increase",71.564400000000006,23616.252]
[null,1009454,null,"PULLEY FOR 8 TO 13 MM KERNMANTEL ROPE",null,null,"1 unit","1 unit",null,"Price increase",19.281599999999997,6362.927999999999]
[null,1009960,null,"CON/Fall Indic SWIVEL Zn STEEL SnHk 19mm",null,null,"1 unit","1 unit",null,"Price increase",44.393000000000001,14649.69]
[null,1010168,null,"Shorco sling and foot loop set",null,null,"1 unit","1 unit",null,"Price increase",25.059899999999999,8269.7669999999998]
[null,1010220,null,"Self rescue descender for braided rope from 9 to 12 mm - Light alloy body. ",null,null,"1 unit","1 unit",null,"Price increase",12.720499999999999,4197.7649999999994]
[null,1010221,null,"Troll ROCKER Rope lock black - Automatic rope lock",null,null,"1 unit","1 unit",null,"Price increase",117.0312,38620.296000000002]
[null,1010222,null,"Pro ALLP Tech - Screw and auto-lock, controlled-rate rope descender for use with kernmantel 10,5mm to 12,7mm rope black",null,null,"1 unit","1 unit",null,"Price increase",257.08799999999997,84839.039999999994]
[null,1010224,null,"Aluminium Single Swivel Cheek Pulley Ø12,7 mm ropes dual attachment",null,null,"1 unit","1 unit",null,"Price increase",72.120599999999996,23799.797999999999]
[null,1011701,null,"Butterfly II - Belt with front anchorage point & leg straps, side D-rings for positioning lanyard-EN 358 & EN 813 - Size S (36 to 40)",null,null,"1 unit","1 unit",null,"Price increase",249.50220000000002,82335.72600000001]
[null,1011702,null,"Butterfly II - Belt with front anchorage point & leg straps, side D-rings for positioning lanyard-EN 358 & EN 813 - Size M/L (42 to 46)",null,null,"1 unit","1 unit",null,"Price increase",249.50220000000002,82335.72600000001]
[null,1011705,null,"Front anchorage strap EN 358 length 25 cm",null,null,"1 unit","1 unit",null,"Price increase",12.362399999999999,4079.5919999999996]
[null,1011706,null,"Front anchorage strap EN 358 length 30 cm",null,null,"1 unit","1 unit",null,"Price increase",12.362399999999999,4079.5919999999996]
[null,1011707,null,"Front anchorage strap EN 813 length 30 cm",null,null,"1 unit","1 unit",null,"Price increase",15.667199999999999,5170.1759999999995]
[null,1011708,null,"Seat strap Butterfly 2 Small",null,null,"1 unit","1 unit",null,"Price increase",114.5154,37790.082000000002]
[null,1011709,null,"Seat strap Butterfly 2 Medium/Large",null,null,"1 unit","1 unit",null,"Price increase",114.5154,37790.082000000002]
[null,1011710,null,"Legs straps kit ",null,null,"1 unit","1 unit",null,"Price increase",83.32480000000001,27497.184000000005]
[null,1011711,null,"Butterfly 2 & Dragonfly Chainsaw karabiner ",null,null,"1 unit","1 unit",null,"Price increase",44.197299999999998,14585.109]
[null,1011725,null,"AMAZONE climbing line 2 stitched splices by meter",null,null,"1 meter","1 meter",null,"Price increase",5.7473999999999998,1896.6420000000001]
[null,1011950,null,"Falcon SRL Steel spring, steel thimble with SST swivel + snap hook at bottom (10m)",null,null,"1 unit","1 unit",null,"Price increase",323.62720000000002,106796.97600000001]
[null,1012230,null,"Aluminium ring for front anchorage strap",null,null,"1 unit","1 unit",null,"Price increase",8.484,2799.72]
[null,1012231,null,"Pair of lyre shackle for Butterfly 2",null,null,"1 pair","1 pair",null,"Price increase",9.2515999999999998,3053.0279999999998]
[null,1012232,null,"Front anchorage strap EN 358 length 35cm",null,null,"1 unit","1 unit",null,"Price increase",12.362399999999999,4079.5919999999996]
[null,1012247,null,"Belt-harness vest Elastokuik Comfort (1003023) high-visibility. Size S",null,null,"1 unit","1 unit",null,"Price increase",411.315,135733.95000000001]
[null,1012248,null,"Belt-harness vest Elastokuik Comfort (1003022) high-visibility. Size M/L",null,null,"1 unit","1 unit",null,"Price increase",411.315,135733.95000000001]
[null,1012433,null,"Falcon SRL Eco, Steel Spring, Galvanised steel cable, load indicator with swivel snap hook (6,2m)",null,null,"1 unit","1 unit",null,"Price increase",362.08640000000003,119488.512]
[null,1012434,null,"Falcon SRL Eco, Steel Spring, Galvanised steel cable, load indicator with swivel snap hook (10m)",null,null,"1 unit","1 unit",null,"Price increase",373.83839999999998,123366.67199999999]
[null,1012436,null,"Falcon SRL Eco, Steel Spring, Galvanised steel cable, load indicator with swivel snap hook (15m)",null,null,"1 unit","1 unit",null,"Price increase",422.99920000000003,139589.736]
[null,1012437,null,"Falcon SRL Eco, Steel Spring, Galvanised steel cable, load indicator with swivel snap hook (20m)",null,null,"1 unit","1 unit",null,"Price increase",436.71680000000003,144116.54400000002]
[null,1012940,null,"AMAZONE climbing line without splice by meter",null,null,"1 meter","1 meter",null,"Price increase",4.8513000000000002,1600.9290000000001]
[null,1013453,null,"Belt-harness vest Elastolight (1010142) high-visibility. Size M/L",null,null,"1 unit","1 unit",null,"Price increase",340.29239999999999,112296.492]
[null,1013456,null,"Belt-harness vest Elastokuik Export (1003027) high-visibility. Size S",null,null,"1 unit","1 unit",null,"Price increase",371.90219999999999,122727.726]
[null,1013457,null,"Belt-harness vest Elastokuik Export (1003027) high-visibility. Size M/L",null,null,"1 unit","1 unit",null,"Price increase",371.90219999999999,122727.726]
[null,1013582,null,"Falcon SRL Steel spring, steel thimble with SST swivel + snap hook at bottom (20m)",null,null,"1 unit","1 unit",null,"Price increase",460.99039999999997,152126.83199999999]
[null,1013620,null,"Cambium saver-used with a climbing line-EN795 1.30m",null,null,"1 unit","1 unit",null,"Price increase",49.388999999999996,16298.369999999999]
[null,1013621,null,"Cambium saver-used with a climbing line-EN795 0.90m",null,null,"1 unit","1 unit",null,"Price increase",44.500600000000006,14685.198000000002]
[null,1013641,null,"Butterfly II - Belt with front anchorage point & leg straps, side D-rings for positioning lanyard-EN 358 & EN 813 - Size XL (48 to 60) ",null,null,"1 unit","1 unit",null,"Price increase",226.3074,74681.441999999995]
[null,1013724,null,"Butterfly II - Harness with front anchorage point & leg straps, side D-rings for positioning lanyard-EN 358 & EN 813 - Size S (36 to 40)",null,null,"1 unit","1 unit",null,"Price increase",284.48820000000001,93881.106]
[null,1013725,null,"Butterfly II - Harness with front anchorage point & leg straps, side D-rings for positioning lanyard-EN 358 & EN 813 - Size M/L (42 to 46)",null,null,"1 unit","1 unit",null,"Price increase",284.48820000000001,93881.106]
[null,1013726,null,"Butterfly II - Harness with front anchorage point & leg straps, side D-rings for positioning lanyard-EN 358 & EN 813 - Size XL (48 to 60) ",null,null,"1 unit","1 unit",null,"Price increase",284.48820000000001,93881.106]
[null,1013727,null,"Dragonfly - Harness with front anchorage point & seat strap, side D-rings for positioning lanyard-EN 358 & EN 813 - Size S (36 to 40)",null,null,"1 unit","1 unit",null,"Price increase",319.54559999999998,105450.048]
[null,1013728,null,"Dragonfly - Harness with front anchorage point & seat strap, side D-rings for positioning lanyard-EN 358 & EN 813 - Size M/L (42 to 46)",null,null,"1 unit","1 unit",null,"Price increase",319.54559999999998,105450.048]
[null,1013729,null,"Dragonfly - Harness with front anchorage point & seat strap, side D-rings for positioning lanyard-EN 358 & EN 813 - Size X/L(48 to 60) ",null,null,"1 unit","1 unit",null,"Price increase",319.54559999999998,105450.048]
[null,1014020,null,"Furling bowl",null,null,"1 unit","1 unit",null,"Price increase",4.5651999999999999,1506.5160000000001]
[null,1014991,null,"SPIKES - Climbing gaff",null,null,"1 unit","1 unit",null,"Price increase",447.67239999999998,147731.89199999999]
[null,1014994,null,"Replacement spikes kit",null,null,"1 kit","1 unit",null,"Price increase",139.4709,46025.396999999997]
[null,1014996,null,"Protective sheaths",null,null,"1 kit","1 unit",null,"Price increase",15.614600000000001,5152.8180000000002]
[null,1014998,null,"Calf straps",null,null,"1 kit","1 unit",null,"Price increase",46.823599999999999,15451.788]
[null,1015000,null,"Ankle straps",null,null,"1 kit","1 unit",null,"Price increase",33.431000000000004,11032.230000000001]
[null,1015006,null,"Fastening kit",null,null,"1 kit","1 unit",null,"Price increase",3.5249000000000001,1163.2170000000001]
[null,1015008,null,"Protective padding kit",null,null,"1 kit","1 unit",null,"Price increase",132.00699999999998,43562.30999999999]
[null,1015192,null,"Green Belt XS",null,null,"1 unit","1 unit",null,"Price increase",268.37220000000002,88562.826000000001]
[null,1015615,null,"SNAP TOGETHER CLIP FOR MINIPHONE HOLDER",null,null,"1 unit","1 unit",null,"Price increase",4.4472000000000005,1467.5760000000002]
[null,1016490,null,"Chainsaw Lanyard",null,null,"1 unit","1 unit",null,"Price increase",17.826499999999999,5882.7449999999999]
[null,1016681,null,"Dragonfly - Belt with front anchorage point & seat strap, side D-rings for positioning lanyard-EN 358 & EN 813 - Size S (36 to 40)",null,null,"1 unit","1 unit",null,"Price increase",270.93240000000003,89407.69200000001]
[null,1016682,null,"Dragonfly - Belt with front anchorage point & seat strap, side D-rings for positioning lanyard-EN 358 & EN 813 - Size M/L (42 to 46)",null,null,"1 unit","1 unit",null,"Price increase",270.93240000000003,89407.69200000001]
[null,1016683,null,"Dragonfly - Belt with front anchorage point & seat strap, side D-rings for positioning lanyard-EN 358 & EN 813 - Size X/L(48 to 60) ",null,null,"1 unit","1 unit",null,"Price increase",270.93240000000003,89407.69200000001]
[null,1016792,null,"REVO BACK D.RING PROTECTION",null,null,"1 unit","1 unit",null,"Price increase",27.1524,8960.2919999999995]
[null,1016824,null,"ARBORIST BELT MORPHO EN358-813 T1",null,null,"1 unit","1 unit",null,"Price increase",301.43039999999996,99472.031999999992]
[null,1016825,null,"ARBORIST BELT MORPHO EN358-813 T2",null,null,"1 unit","1 unit",null,"Price increase",301.43039999999996,99472.031999999992]
[null,1016826,null,"ARBORIST BELT MORPHO EN358-813 T3",null,null,"1 unit","1 unit",null,"Price increase",301.43039999999996,99472.031999999992]
[null,1017022,null,"Tree Pruning Kit with Butterfly Belt S",null,null,"1 kit","1 unit",null,"Price increase",871.97759999999994,287752.60800000001]
[null,1017023,null,"Tree Pruning Kit with Butterfly Belt M/L",null,null,"1 kit","1 unit",null,"Price increase",871.97759999999994,287752.60800000001]
[null,1017592,null,"MORPHO 18 CM TRIANGULATION",null,null,"1 unit","1 unit",null,"Price increase",12.8826,4251.2579999999998]
[null,1017821,null,"CRAVATE JIRAF 1,80M",null,null,"1 unit","1 unit",null,"Price increase",200.73669999999998,66243.11099999999]
[null,1017822,null,"STEEL SLING 0,66m",null,null,"1 unit","1 unit",null,"Price increase",38.779499999999999,12797.234999999999]
[null,1017844,null,"PRUNING KIT TALUS",null,null,"1 kit","1 unit",null,"Price increase",1334.2160000000001,440291.28]
[null,1018973,null,"Snap Hook Steel open.18mm",null,null,"1 unit","1 unit",null,"Price increase",10.691400000000002,3528.1620000000007]
[null,1018976,null,"Karabiner open.110mm Alu",null,null,"1 unit","1 unit",null,"Price increase",82.338200000000001,27171.606]
[null,1029502,null,"TOTEM DURAHOIST POST MILLER",null,null,"1 unit","1 unit",null,"Price increase",1033.9861000000001,341215.413]
[null,1029503,null,"Plate to Screw Totem DuraHoist Miller",null,null,"1 unit","1 unit",null,"Price increase",504.1026,166353.85800000001]
[null,1029720,null,"BACK PACK FOR TOTEM DURAHOIST",null,null,"1 unit","1 unit",null,"Price increase",68.770899999999997,22694.397000000001]
[null,1013628,null,"Sangle d'ancrage réglable 1,5m",null,null,"1 unit","1 unit",null,"Price increase",37.668599999999998,12430.637999999999]
[null,1013629,null,"Sangle d'ancrage réglable 3m",null,null,"1 unit","1 unit",null,"Price increase",51.214199999999998,16900.685999999998]
[null,1012473,null,"Sangle d'ancrage réglable 6m",null,null,"1 unit","1 unit",null,"Price increase",62.281200000000005,20552.796000000002]
[null,1014830,null,"Sangle d'ancrage réglable 10m",null,null,"1 unit","1 unit",null,"Price increase",68.484699999999989,22599.950999999997]

{"sheet":"errors","index":10,"n_rows":1,"n_cols":2,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Number","Description"]